{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Customer Information","Chilled Water System Template","Hot Water System Template","Air Side System Template","Engineering Report","Report Look Up Tables","CTZ2","General Look Up Tables","_SSC"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":39,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Customer Information","index":0,"n_rows":36,"n_cols":11,"rows_kept":36,"cut":false,"hidden":false,"merged":[[28,7,28,8],[28,9,28,10],[1,1,3,3],[10,7,10,10],[16,7,25,10],[27,7,27,8],[27,9,27,10],[6,3,6,5],[7,3,7,5],[6,7,6,10],[7,7,7,10],[10,3,10,5],[11,3,11,5],[11,7,11,10],[12,7,12,10]]}
[]
[null,null,null,null,null,null,null,null,null,null,"HVAC Calculator Tool"]
[]
[null,null,null,null,null,null,null,null,null,null,"V.1.3"]
[]
[null,"Customer Information"]
[null,null,"Name",null,null,null,"Phone"]
[null,null,"Contact",null,null,null,"Email"]
[]
[null,"Building Information"]
[null,null,"Address",null,null,null,"Type","Convention Center"]
[null,null,"City",null,null,null,"SQFT"]
[null,null,"Zip",94127,"Zone",{"$f":"VLOOKUP(D13,tbl_ZIP_Code,2,0)","v":3},"Year Built"]
[]
[null,"Consumption"]
[null,null,"Peak kW","kWh","Therms","Electric Cost","Therm Cost"]
[null,"Jan",null,null,null,null,null,"Include Total Cost for customers that receive bundled service. If the customer is direct access and the commodity cost is available, it should be included. Otherwise the Total Cost can be omitted."]
[null,"Feb"]
[null,"Mar"]
[null,"Apr"]
[null,"May"]
[null,"Jun"]
[null,"Jul"]
[null,"Aug"]
[null,"Sep"]
[null,"Oct"]
[null,"Nov"]
[null,"Dec",null,null,null,null,null,"$/kWh",null,"$/Therm"]
[null,"Annual",{"$f":"MAX($C$17:$C$28)","v":0},{"$f":"SUM($D$17:$D$28)","v":0},{"$f":"SUM($E$17:$E$28)","v":0},{"$f":"MAX($F$17:$F$28)","v":0},{"$f":"SUM($G$17:$G$28)","v":0},{"$f":"$F$29/$D$29","v":{"$error":"#DIV/0!"}},null,{"$f":"$G$29/$E$29","v":{"$error":"#DIV/0!"}}]
[]
[null,"Current PG&E Incentive Rates ($/unit)"]
[null,null,"Basic Non Lighting",0.08,"/kWh",null,null,"Peak Demand",150,"/kW"]
[null,null,"Target Non Lighting",0.15,"/kWh",null,null,"Natural Gas",1,"/therm"]
[null,null,"To Code/ISP Electric",0.03,"/kWh",null,null,"To Code/ISP Natural Gas",0.4,"/therm"]
[]
[null,"Additional Information Section"]

{"sheet":"Chilled Water System Template","index":1,"n_rows":243,"n_cols":43,"rows_kept":243,"cut":false,"hidden":true,"merged":[[10,6,10,8],[11,7,11,9],[61,3,61,4],[61,8,61,9],[68,3,68,4],[68,8,68,9],[46,5,46,7],[64,5,64,7],[17,7,17,8],[17,3,17,4],[17,5,17,6],[20,2,20,3],[12,7,12,9],[13,7,13,9],[62,3,62,4],[62,8,62,9],[6,5,6,6],[7,5,7,6],[5,5,5,6],[135,5,135,11],[135,12,135,18],[16,7,16,8],[107,5,107,7],[108,5,108,7],[99,5,99,7],[78,8,78,9],[92,8,92,9],[9,5,9,6],[8,5,8,6],[96,8,96,9],[18,5,18,6],[19,5,19,6],[99,3,99,4],[99,8,99,9],[69,3,69,4],[96,5,96,7],[96,3,96,4],[69,5,69,7],[72,5,72,7],[71,5,71,7],[77,3,77,4],[77,5,77,7],[77,8,77,9],[69,8,69,9],[75,3,75,4],[75,8,75,9],[76,3,76,4],[76,5,76,7],[76,8,76,9],[16,3,16,4],[109,3,109,4],[109,5,109,7],[109,8,109,9],[105,3,105,4],[105,8,105,9],[101,5,101,7],[102,5,102,7],[105,5,105,7],[78,3,78,4],[78,5,78,7],[92,5,92,7],[94,5,94,7],[95,5,95,7],[92,3,92,4]]}
[null,"Chilled Water Side System Calculations"]
[null,"Chillers, Cooling Towers & Pumps Specifications",null,null,null,null,null,null,"Cost",null,"Enable",null,null,null,"Savings From Baseline",null,null,"Chiller, PCHWP, SCHWP kW","Chiller, PCHWP, SCHWP kWh","Cooling Tower Fan kW","Cooling Tower Fan  kWh","Condenser Pump kW","Condenser Pump kWh","Total kW","Total kWh","Cost","Incentives"]
[null,"Chiller Specifications",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chiller Replacement (or Load Change)",{"$f":"R27-R28","v":0},0,0,0,0,0,{"$f":"SUM(R3,T3,V3)","v":0},{"$f":"SUM(S3,U3,W3)","v":0},{"$f":"J2","v":0},0]
[null,null,null,"Baseline",null,null,null,null,"Proposed",null,null,null,null,null,null,null,"Chilled Water Plant Lockout Control",{"$f":"R28-R29","v":0},0,0,0,0,0,{"$f":"SUM(R4,T4,V4)","v":0},{"$f":"SUM(S4,U4,W4)","v":0},{"$f":"K45","v":0},0]
[null,null,"CH1","CH2","CH3",null,null,"CH1","CH2","CH3",null,null,null,null,null,null,"Chiller Staging Sequence Optimization",{"$f":"R29-R30","v":0},0,0,0,0,0,0,0,{"$f":"K49","v":0},0]
[null,null,"Main Chiller","Lag Chiller","Third Chiller","Equipment Name",null,"Main Chiller","Lag Chiller","Third Chiller",null,null,null,null,null,null,"Chilled Water Temperature Reset",{"$f":"R30-R31","v":0},0,0,0,0,0,0,0,{"$f":"K61","v":0},0]
[null,null,700,700,700,"Capacity (tons)",null,700,700,700,{"$f":"IF(OR(C7<>H7,D7<>I7,E7<>J7),\"*\",\"\")","v":""},null,null,null,null,null,"Condenser Water Temperature Reset",{"$f":"R31-R32","v":0},0,0,0,0,0,0,0,{"$f":"K68","v":0},0]
[null,null,0.55000000000000004,0.55000000000000004,0.55000000000000004,"kW/Ton (part load)",null,0.55000000000000004,0.55000000000000004,0.55000000000000004,{"$f":"IF(OR(C8<>H8,D8<>I8,E8<>J8),\"*\",\"\")","v":""},null,null,null,null,null,"Water Side Economizer Optimization",{"$f":"R32-R33","v":0},0,0,0,0,0,0,0,{"$f":"K75","v":0},0]
[null,null,44,44,44,"Design CHWT",null,44,44,44,{"$f":"IF(OR(C9<>H9,D9<>I9,E9<>J9),\"*\",\"\")","v":""},null,null,null,null,null,"Cooling Tower Staging Sequence Optimization",{"$f":"R33-R34","v":0},0,0,0,0,0,0,0,{"$f":"K81","v":0},0]
[null,null,85,85,85,"Design CWT",null,85,85,85,{"$f":"IF(OR(C10<>H10,D10<>I10,E10<>J10),\"*\",\"\")","v":""},null,null,null,null,null,"Secondary Chilled Water Pump VFD",{"$f":"R34-R35","v":0},0,0,0,0,0,{"$f":"SUM(R10,T10,V10)","v":0},0,{"$f":"K92","v":0},0]
[null,null,null,"Start Time","Stop Time",null,"New Chiller Type (if replaced)",null,null,null,null,null,null,null,null,null,"Chilled Water Differential Pressure Reset",{"$f":"R35-R36","v":0},0,0,0,0,0,0,0,{"$f":"K99","v":0},0]
[null,null,"Weekday",4,18,null,"CH1","Chiller Not Being Replaced",null,null,null,null,null,null,null,null,"Condenser Water Pump VFD",{"$f":"R36-R37","v":0},0,0,0,0,0,0,0,{"$f":"K105","v":0},0]
[null,null,"Saturday",4,18,null,"CH2","Chiller Not Being Replaced",null,null,null,null,null,null,null,null,"Total",{"$f":"SUM(R3:R12)","v":0},0,0,0,0,0,0,0,{"$f":"SUM(Z3:Z12)","v":0},{"$f":"SUM(AA3:AA12)","v":0}]
[null,null,"Sunday",4,18,null,"CH3","Chiller Not Being Replaced",null,null,null,null,null,null,"Savings From Title 24",null,null,"Chiller, PCHWP, SCHWP kW","Chiller, PCHWP, SCHWP kWh","Cooling Tower Fan kW","Cooling Tower Fan  kWh","Condenser Pump kW","Condenser Pump kWh","Total kW","Total kWh"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chiller Replacement (or Load Change)",0,0,0,0,0,0,{"$f":"SUM(R15,T15,V15)","v":0},{"$f":"SUM(S15,U15,W15)","v":0}]
[null,"Building Cooling Load Change",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water Plant Lockout Control",0,0,0,0,0,0,{"$f":"SUM(R16,T16,V16)","v":0},{"$f":"SUM(S16,U16,W16)","v":0}]
[null,null,null,"Baseline",null,null,null,"Proposed",null,null,null,null,null,null,null,null,"Chiller Staging Sequence Optimization",0,0,0,0,0,0,0,0]
[null,null,null,"Simple Data",null,"Data Type",null,"Simple Data",null,null,null,null,null,null,null,null,"Chilled Water Temperature Reset",0,0,0,0,0,0,0,0]
[null,null,null,200,1400,"Building Load Tons",null,200,1400,{"$f":"IF(OR(D19<>H19,E19<>I19),\"*\",\"\")","v":""},null,null,null,null,null,null,"Condenser Water Temperature Reset",0,0,0,0,0,0,0,0]
[null,null,null,55,90,{"$f":"\"@OAT\"","v":"@OAT"},null,55,90,{"$f":"IF(OR(D20<>H20,E20<>I20),\"*\",\"\")","v":""},null,null,null,null,null,null,"Water Side Economizer Optimization",0,0,0,0,0,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Cooling Tower Staging Sequence Optimization",0,0,0,0,0,0,0,0]
[null,"Primary Pumps",null,null,null,null,null,"Secondary Pumps",null,null,null,null,null,null,null,null,"Secondary Chilled Water Pump VFD",0,0,0,0,0,0,{"$f":"SUM(R22,T22,V22)","v":0},0]
[null,null,null,"PCHWP1","PCHWP2","PCHWP3",null,"SCHWP",null,null,null,null,null,null,null,null,"Chilled Water Differential Pressure Reset",0,0,0,0,0,0,0,0]
[null,null,"Flow (gpm)",1120,1120,1120,null,1120,"Flow (gpm)",null,null,null,null,null,null,null,"Condenser Water Pump VFD",0,0,0,0,0,0,0,0]
[null,null,"Head (ft)",20,20,20,null,40,"Motor (hp)",null,null,null,null,null,null,null,"Total",{"$f":"SUM(R15:R24)","v":0},0,0,0,0,0,0,0]
[null,null,"Motor Eff (%)",0.8,0.8,0.8,null,0.82,"Motor Efficiency (%)",null,null,null,null,null,"Consumption",null,null,"Chiller, PCHWP, SCHWP kW","Chiller, PCHWP, SCHWP kWh","Cooling Tower Fan kW","Cooling Tower Fan  kWh","Condenser Pump kW","Condenser Pump kWh","Total kW","Total kWh"]
[null,null,"Pump Eff (%)",0.8,0.8,0.8,null,0.8,"Pump Efficiency (%)",null,null,null,null,null,null,null,"Baseline",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,{"$f":"SUM(R27,T27,V27)","v":483.90026544095736},{"$f":"SUM(S27,U27,W27)","v":1272817.4803981604}]
[null,null,null,null,null,null,null,"Max","Min",null,null,null,null,null,null,null,"Chiller Replacement (or Load Change)",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,{"$f":"SUM(R28,T28,V28)","v":483.90026544095736},{"$f":"SUM(S28,U28,W28)","v":1272817.4803981604}]
[null,null,null,null,null,null,null,2,1,"Pump Qty Operating",null,null,null,null,null,null,"Chilled Water Plant Lockout Control",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,null,null,null,null,null,80,65,{"$f":"\"@OAT\"","v":"@OAT"},null,null,null,null,null,null,"Chiller Staging Sequence Optimization",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Chilled Water Temperature Reset",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,"Cooling Tower Specs",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Condenser Water Temperature Reset",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,null,"CT - 1","CT - 2","CT - 3",null,null,null,null,null,null,null,null,null,null,"Water Side Economizer Optimization",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,"Capacity (tons)",875,875,875,null,null,null,null,null,null,null,null,null,null,"Cooling Tower Staging Sequence Optimization",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,"Fan (hp)",30,30,30,null,null,null,null,null,null,null,null,null,null,"Secondary Chilled Water Pump VFD",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,"Motor Eff (%)",0.85,0.85,0.85,null,null,null,null,null,null,null,null,null,null,"Chilled Water Differential Pressure Reset",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,"Min Fan Speed",0.2,0.2,0.2,null,null,null,null,null,null,null,null,null,null,"Condenser Water Pump VFD",361.61967383668218,1016006.9435057872,75.738702121209215,86281.053826419855,46.541889483065951,170529.48306595359,483.90026544095736,1272817.4803981604]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Proposed",{"$f":"INDEX(tbl_Chiller_Calc_Engine736[Chiller kW],$C$126)","v":361.61967383668218},{"$f":"SUM(tbl_Chiller_Calc_Engine736[Chiller kWh])","v":1016006.9435057872},{"$f":"INDEX(tbl_Chiller_Calc_Engine736[CT Fan kW],$C$126)","v":75.738702121209215},{"$f":"SUM(tbl_Chiller_Calc_Engine736[CT Fan  kWh])","v":86281.053826419855},{"$f":"INDEX(tbl_Chiller_Calc_Engine736[CWP kW],$C$126)","v":46.541889483065951},{"$f":"SUM(tbl_Chiller_Calc_Engine736[CWP kWh])","v":170529.48306595359},{"$f":"SUM(R38,T38,V38)","v":483.90026544095736},{"$f":"SUM(S38,U38,W38)","v":1272817.4803981604}]
[null,"Condenser Pumps"]
[null,null,"Flow (gpm)",2100,null,"Max","Min"]
[null,null,"Head (ft)",40,null,2,1,"# Pumps operating"]
[null,null,"Motor Eff",0.85,null,85,60,{"$f":"\"@OAT\"","v":"@OAT"}]
[null,null,"Pump Eff",0.8]
[]
[null,"Chilled Water Plant Lockout Control",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,null,"Baseline",null,null,null,"Proposed"]
[null,null,null,null,50,"Cooling Lookout Temp",null,null,50,{"$f":"IF(OR(E47<>I47),\"*\",\"\")","v":""}]
[]
[null,"Chiller Staging Sequence Optimization",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Baseline",null,null,null,null,null,"Proposed"]
[null,null,"CH1","CH2","CH3","Capacity","Stage","Capacity","CH1","CH2","CH3"]
[null,null,{"$f":"C7","v":700},{"$f":"D7","v":700},{"$f":"E7","v":700},"Tons",null,"Tons",{"$f":"H7","v":700},{"$f":"I7","v":700},{"$f":"J7","v":700}]
[null,null,"On",null,null,{"$f":"SUMIF(C53:E53,\"On\",$C$52:$E$52)","v":700},1,{"$f":"SUMIF($I53:$K53,\"On\",$I$52:$K$52)","v":700},"On",null,null,{"$f":"IF(OR(C53<>I53,D53<>J53,E53<>K53),\"*\",\"\")","v":""}]
[null,null,null,null,"On",{"$f":"SUMIF(C54:E54,\"On\",$C$52:$E$52)","v":700},2,700,null,null,"On",{"$f":"IF(OR(C54<>I54,D54<>J54,E54<>K54),\"*\",\"\")","v":""}]
[null,null,"On",null,"On",1400,3,1400,"On",null,"On",""]
[null,null,"On","On","On",2100,4,2100,"On","On","On",""]
[null,null,null,null,null,0,5,0,null,null,null,""]
[null,null,null,null,null,0,6,0,null,null,null,""]
[null,null,null,null,null,0,7,0,null,null,null,""]
[]
[null,"Chilled Water Temperature Reset",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,null,"Simple Data",null,null,"Data Type",null,"Simple Data"]
[null,null,null,"Min OAT","Max OAT",null,null,null,"Min OAT","Max OAT"]
[null,null,null,45,45,"Chilled Water Temperature Reset",null,null,45,50,{"$f":"IF(OR(D65<>I65,E65<>J65),\"*\",\"\")","v":"*"}]
[null,null,null,55,85,null,"@ OAT",null,55,85,{"$f":"IF(OR(D66<>I66,E66<>J66),\"*\",\"\")","v":""}]
[]
[null,"Condenser Water Temperature Reset",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,null,"Min OAT","Max OAT",null,null,null,"Min OAT","Max OAT"]
[null,null,null,75,75,"Condenser Water Temp",null,null,75,75,{"$f":"IF(OR(D72<>I72,E72<>J72),\"*\",\"\")","v":""}]
[null,null,null,55,75,"@ OAT (wet bulb)",null,null,55,75,{"$f":"IF(OR(D73<>I73,E73<>J73),\"*\",\"\")","v":""}]
[]
[null,"Water Side Economizer Optimization",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,null,6,null,"CT Approach for WSE (°F)",null,null,6,null,{"$f":"IF(OR(D77<>I77,E77<>J77),\"*\",\"\")","v":""}]
[null,null,null,-1,null,"WSE Enable OAT Wet Bulb (°F)",null,null,-1,null,{"$f":"IF(OR(D78<>I78,E78<>J78),\"*\",\"\")","v":""}]
[null,null,null,2,null,"HX Approach (°F)",null,null,2,null,{"$f":"IF(OR(D79<>I79,E79<>J79),\"*\",\"\")","v":""}]
[]
[null,"Cooling Tower Staging Sequence Optimization",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Baseline Staging ",null,null,null,null,null,"Proposed Staging "]
[null,null,"CT1","CT2","CT3","Tons","Stage","Tons","CT1","CT2","CT3"]
[null,null,"On",null,null,{"$f":"SUMIF(C84:E84,\"On\",$D$34:$F$34)","v":875},1,{"$f":"SUMIF(I84:K84,\"On\",$D$34:$F$34)","v":875},"On",null,null,{"$f":"IF(OR(C84<>I84,D84<>J84,E84<>K84),\"*\",\"\")","v":""}]
[null,null,null,"On",null,875,2,875,null,"On",null,{"$f":"IF(OR(C85<>I85,D85<>J85,E85<>K85),\"*\",\"\")","v":""}]
[null,null,"On","On","On",2625,3,2625,"On","On","On",""]
[null,null,null,null,null,0,4,0,null,null,null,""]
[null,null,null,null,null,0,5,0,null,null,null,""]
[null,null,null,null,null,0,6,0,null,null,null,""]
[null,null,null,null,null,0,7,0,null,null,null,""]
[]
[null,"Secondary Chilled Water Pump VFD And Speed Control",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,null,"Min OAT","Max OAT",null,null,null,"Min OAT","Max OAT"]
[null,null,null,0.2,1,"Pump Speed (%)",null,null,0.2,1,{"$f":"IF(OR(D95<>I95,E95<>J95),\"*\",\"\")","v":""}]
[null,null,null,60,80,"@ OAT",null,null,60,80,{"$f":"IF(OR(D96<>I96,E96<>J96),\"*\",\"\")","v":""}]
[null,null,null,"VFD",null,"Pump Control",null,null,"VFD",null,{"$f":"IF(OR(D97<>I97,E97<>J97),\"*\",\"\")","v":""}]
[]
[null,"Chilled Water Differential Pressure Reset",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,null,45,45,"Chilled Water Differential PSI",null,null,45,45,{"$f":"IF(OR(D102<>I102,E102<>J102),\"*\",\"\")","v":""}]
[null,null,null,65,80,"@ OAT",null,null,65,80,{"$f":"IF(OR(D103<>I103,E103<>J103),\"*\",\"\")","v":""}]
[]
[null,"Condenser Water Pump VFD And Speed Control",null,null,null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,null,1,1,"Pump Speed (%)",null,null,0.8,0.8,{"$f":"IF(OR(D108<>I108,E108<>J108),\"*\",\"\")","v":"*"}]
[null,null,null,60,80,"@ OAT",null,null,60,80,{"$f":"IF(OR(D109<>I109,E109<>J109),\"*\",\"\")","v":""}]
[null,null,null,"Constant",null,"Pump Control",null,null,"VFD",null,{"$f":"IF(OR(D110<>I110,E110<>J110),\"*\",\"\")","v":"*"}]
[]
[null,"Processing"]
[null,null,false,"Title 24"]
[null,null,"Proposed","Cooling Load/Chiller Change",null,null,null,null,"Condenser Water Temperature Reset",null,null,null,null,"Chilled Water Temperature Reset",null,null,"Cooling Tower Staging Sequence Optimization",null,null,null,null,null,"Chiller Staging Sequence Optimization"]
[null,null,"Proposed","Chilled Water Plant Lockout Control",null,null,null,null,{"$f":"IF(OR($L$68=\"Disable\",I70=\"\",$C$118=\"Baseline\"),D70,I70)","v":"Simple Data"},"Data Type",null,null,null,{"$f":"IF(OR($L$61=\"Disable\",I63=\"\",$C$117=\"Baseline\"),D63,I63)","v":"Simple Data"},"Data Type",null,"Baseline","Proposed",null,null,null,null,"Baseline","Proposed","T24",{"$f":"IF($H$12<>\"Chiller Not Being Replaced\",Find_Title24_Eff($H$12,Z117,$AE$118:$AE$129,$AF$118:$AF$129,$AG$118:$AG$129,$AH$118:$AH$129),$C$8)","v":0.55000000000000004},{"$f":"IF($H$13<>\"Chiller Not Being Replaced\",Find_Title24_Eff($H$13,AA117,$AE$118:$AE$129,$AF$118:$AF$129,$AG$118:$AG$129,$AH$118:$AH$129),$D$8)","v":0.55000000000000004},{"$f":"IF($H$14<>\"Chiller Not Being Replaced\",Find_Title24_Eff($H$14,AB117,$AE$118:$AE$129,$AF$118:$AF$129,$AG$118:$AG$129,$AH$118:$AH$129),$E$8)","v":0.55000000000000004},null,null,"TABLE 110.2-D WATER CHILLING PACKAGES – MINIMUM EFFICIENCY REQUIREMENTS"]
[null,null,"Proposed","Chiller Staging Sequence Optimization",null,null,null,null,"Min OAT","Max OAT","",null,null,"Min OAT","Max OAT","",{"$f":"TRIM(CONCATENATE(IF($C84=\"On\",$C$83&\" \",\"\")&IF($D84=\"On\",$D$83&\" \",\"\")&IF($E84=\"On\",$E$83&\" \",\"\")))","v":"CT1"},{"$f":"TRIM(CONCATENATE(IF($I84=\"On\",$I$83&\" \",\"\")&IF($J84=\"On\",$J$83&\" \",\"\")&IF($K84=\"On\",$K$83&\" \",\"\")))","v":"CT1"},null,"CT1","CT2","CT3",{"$f":"TRIM(CONCATENATE(IF($C53=\"On\",$C$51&\" \",\"\")&IF($D53=\"On\",$D$51&\" \",\"\")&IF($E53=\"On\",$E$51&\" \",\"\")))","v":"CH1"},{"$f":"TRIM(IF($I53=\"On\",$I$51&\" \",\"\")&IF($J53=\"On\",$J$51&\" \",\"\")&IF($K53=\"On\",$K$51&\"  \",\"\"))","v":"CH1"},null,"CH1","CH2","CH3",null,null,"Equipment Type","Size (Tons)",null,"Path A Efficiency"]
[null,null,"Proposed","Chilled Water Temperature Reset",null,null,null,null,{"$f":"IF(OR($L$68=\"Disable\",I72=\"\",$C$118=\"Baseline\"),D72,I72)","v":75},{"$f":"IF(OR($L$68=\"Disable\",J72=\"\",$C$118=\"Baseline\"),E72,J72)","v":75},"CWT",null,null,{"$f":"IF(OR($L$61=\"Disable\",I65=\"\",$C$117=\"Baseline\"),D65,I65)","v":45},{"$f":"IF(OR($L$61=\"Disable\",J65=\"\",$C$117=\"Baseline\"),E65,J65)","v":45},"CHWT","CT2","CT2","Capacity",{"$f":"D34","v":875},875,875,"CH3","CH3","Capacity",{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),C7,H7)","v":700},{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),D7,I7)","v":700},{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),E7,J7)","v":700},null,null,null,">=","<","IPLV kW/ton"]
[null,null,"Proposed","Condenser Water Temperature Reset",null,null,null,null,{"$f":"IF(OR($L$68=\"Disable\",I73=\"\",$C$118=\"Baseline\"),D73,I73)","v":55},{"$f":"IF(OR($L$68=\"Disable\",J73=\"\",$C$118=\"Baseline\"),E73,J73)","v":75},"@ OAT",null,null,{"$f":"IF(OR($L$61=\"Disable\",I66=\"\",$C$117=\"Baseline\"),D66,I66)","v":55},{"$f":"IF(OR($L$61=\"Disable\",J66=\"\",$C$117=\"Baseline\"),E66,J66)","v":85},"@ OAT","CT1 CT2 CT3","CT1 CT2 CT3","HP",30,30,30,"CH1 CH3","CH1 CH3","kW/Ton",{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),IF($C$113,Z$115,C$8),H$8)","v":0.55000000000000004},{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),IF($C$113,AA$115,D$8),I$8)","v":0.55000000000000004},{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),IF($C$113,AB$115,E$8),J$8)","v":0.55000000000000004},null,null,"Air Cooled",0,150,0.876]
[null,null,"Proposed","Water Side Economizer Optimization",null,null,null,null,"Chilled Water Differential Pressure Reset",null,null,null,null,"Building Cooling Load Change",null,null,"","","Motor Efficiency (%)",0.85,0.85,0.85,"CH1 CH2 CH3","CH1 CH2 CH3","Design CHWT",{"$f":"IF(OR($K$2=\"Disable\",$C$114=\"Baseline\"),C9,H9)","v":44},44,44,null,null,"Air Cooled",150,0,0.85699999999999998]
[null,null,"Proposed","Cooling Tower Staging Sequence Optimization",null,null,null,null,{"$f":"IF(OR($L$99=\"Disable\",I100=\"\",$C$122=\"Baseline\"),D100,I100)","v":"Simple Data"},"Data Type",null,null,null,"Min OA Temp","Max OA Temp",null,"","","Minimum Fan Speed",0.2,0.2,0.2,"","","Design CWT",85,85,85,null,null,"Water Cooled (Non-Centrifugal)",0,75,0.6]
[null,null,"Proposed","Secondary Chilled Water Pump VFD",null,null,null,null,"Min","Max","",null,null,{"$f":"IF(OR($C$114=\"Baseline\",H18=\"\",$K$2=\"Disable\"),D18,H18)","v":"Simple Data"},null,null,"","",null,null,null,null,"","",null,null,null,null,null,null,"Water Cooled (Non-Centrifugal)",75,150,0.56000000000000005]
[null,null,"Proposed","Chilled Water Differential Pressure Reset",null,null,null,null,{"$f":"IF(OR($L$99=\"Disable\",I102=\"\",$C$123=\"Baseline\"),D102,I102)","v":45},{"$f":"IF(OR($L$99=\"Disable\",J102=\"\",$C$123=\"Baseline\"),E102,J102)","v":45},"Psi",null,null,{"$f":"IF(OR($C$114=\"Baseline\",$K$2=\"Disable\"),D19,H19)","v":200},{"$f":"IF(OR($C$114=\"Baseline\",$K$2=\"Disable\"),E19,I19)","v":1400},"Tons","","",null,null,null,null,"","",null,null,null,null,null,null,"Water Cooled (Non-Centrifugal)",150,300,0.54]
[null,null,"Proposed","Condenser Water Pump VFD",null,null,null,null,{"$f":"IF(OR($L$99=\"Disable\",I103=\"\",$C$123=\"Baseline\"),D103,I103)","v":65},{"$f":"IF(OR($L$99=\"Disable\",J103=\"\",$C$123=\"Baseline\"),E103,J103)","v":80},"@ OAT",null,null,{"$f":"IF(OR($C$114=\"Baseline\",$K$2=\"Disable\"),D20,H20)","v":55},{"$f":"IF(OR($C$114=\"Baseline\",$K$2=\"Disable\"),E20,I20)","v":90},{"$f":"\"@OAT\"","v":"@OAT"},"Stage","Capacity","Cooling Tower","CT1 % Load","CT2 % Load","CHT3 % Load","Stage","Capacity","Chiller","CH1 % Load","CH2 % Load","CH3 % Load",null,null,"Water Cooled (Non-Centrifugal)",300,600,0.52]
[null,null,null,null,null,null,null,null,"Condenser Water Pump VFD",null,null,null,null,"Secondary Chilled Water Pump VFD",null,null,{"$f":"IF(S124=\"\",\"\",$G84)","v":1},{"$f":"IF(S124=\"\",\"\",SUMPRODUCT(--(ISNUMBER(FIND($T$116:$V$116,S124))),$T$117:$V$117))","v":875},{"$f":"IF(OR($L$81=\"Disable\",$C$120=\"Baseline\"),$Q116,$R116)","v":"CT1"},{"$f":"IF(ISNUMBER(SEARCH(T$116,$S124)),T$117/$R124,0)","v":1},0,0,{"$f":"IF(Y124=\"\",\"\",$G53)","v":1},{"$f":"IF(Y124=\"\",\"\",SUMPRODUCT(--(ISNUMBER(FIND($Z$116:$AB$116,Y124))),$Z$117:$AB$117))","v":700},{"$f":"IF(OR($L$49=\"Disable\",$C$116=\"Baseline\"),$W116,$X116)","v":"CH1"},{"$f":"IF(ISNUMBER(SEARCH(Z$116,$Y124)),Z$117/$X124,0)","v":1},0,0,null,null,"Water Cooled (Non-Centrifugal)",600,0,0.5]
[null,null,{"$f":"'CTZ2'!$U$3","v":69},"Peak Demand Temp",null,null,null,null,{"$f":"IF(OR($L$105=\"Disable\",I106=\"\",$C$123=\"Baseline\"),D106,I106)","v":"Simple Data"},"Data Type",null,null,null,{"$f":"IF(OR($L$92=\"Disable\",I93=\"\",$C$121=\"Baseline\"),D93,I93)","v":"Simple Data"},"Data Type",null,2,875,"CT2",0,1,0,2,700,"CH3",0,0,1,null,null,"Water Cooled (Centrifugal)",0,150,0.55000000000000004]
[null,null,{"$f":"MATCH(C125,tbl_Chiller_Calc_Engine736[OAT],0)","v":47},"Peak Line",null,null,null,null,"Min","Max","",null,null,"Min OAT","Max OAT",null,3,2625,"CT1 CT2 CT3",0.33333333333333331,0.33333333333333331,0.33333333333333331,3,1400,"CH1 CH3",0.5,0,0.5,null,null,"Water Cooled (Centrifugal)",150,300,0.55000000000000004]
[null,null,1.4E-2,"Eff Gain (assumption)",null,null,null,null,{"$f":"IF(OR($L$105=\"Disable\",I108=\"\",$C$123=\"Baseline\"),D108,I108)","v":1},{"$f":"IF(OR($L$105=\"Disable\",J108=\"\",$C$123=\"Baseline\"),E108,J108)","v":1},"Pump Speed (%)",null,null,{"$f":"IF(OR($L$92=\"Disable\",I95=\"\",$C$121=\"Baseline\"),D95,I95)","v":0.2},{"$f":"IF(OR($L$92=\"Disable\",J95=\"\",$C$121=\"Baseline\"),E95,J95)","v":1},"Pump Speed (%)","","","",0,0,0,4,2100,"CH1 CH2 CH3",0.33333333333333331,0.33333333333333331,0.33333333333333331,null,null,"Water Cooled (Centrifugal)",300,400,0.52]
[null,null,0.97,"VFD Eff",null,"Pump Control Type",null,null,{"$f":"IF(OR($L$105=\"Disable\",I109=\"\",$C$123=\"Baseline\"),D109,I109)","v":60},{"$f":"IF(OR($L$105=\"Disable\",J109=\"\",$C$123=\"Baseline\"),E109,J109)","v":80},"@ OAT",null,null,{"$f":"IF(OR($L$92=\"Disable\",I96=\"\",$C$121=\"Baseline\"),D96,I96)","v":60},{"$f":"IF(OR($L$92=\"Disable\",J96=\"\",$C$121=\"Baseline\"),E96,J96)","v":80},"@ OAT","","","",0,0,0,"","","",0,0,0,null,null,"Water Cooled (Centrifugal)",400,600,0.5]
[null,null,0.746,"Hp to kW",null,"Constant",null,null,{"$f":"IF(OR($L$105=\"Disable\",I110=\"\",$C$123=\"Baseline\"),D110,I110)","v":"Constant"},"Pump Control",null,null,null,{"$f":"IF(OR($L$92=\"Disable\",I97=\"\",$C$121=\"Baseline\"),D97,I97)","v":"VFD"},"Pump Control",null,"","","",0,0,0,"","","",0,0,0,null,null,"Water Cooled (Centrifugal)",600,0,0.5]
[null,null,2.5,"Affinity Factor",null,"VFD",null,null,"Water Side Economizer Optimization",null,null,null,null,"Chilled Water Plant Lockout Control",null,null,"","","",0,0,0,"","","",0,0,0]
[null,null,1.25,"Cooling Load Tons Factor",null,null,null,null,{"$f":"IF(OR($L$75=\"Disable\",I77=\"\",$C$119=\"Baseline\"),D77,I77)","v":6},"CT Approach for WSE (°F)",null,null,null,{"$f":"IF(OR($L$45=\"Disable\",I47=\"\",$C$115=\"Baseline\"),E47,I47)","v":50},"Cooling Lookout @ OAT"]
[null,null,null,"PCHWP1","PCHWP2","PCHWP3",null,null,{"$f":"IF(OR($L$75=\"Disable\",I78=\"\",$C$119=\"Baseline\"),D78,I78)","v":-1},"WSE Enable OAT Wet Bulb (°F)"]
[null,null,"kW",{"$f":"(D24*D25*$C$129)/(3960*D26*D27)","v":6.5934343434343434},{"$f":"(E24*E25*$C$129)/(3960*E26*E27)","v":6.5934343434343434},{"$f":"(F24*F25*$C$129)/(3960*F26*F27)","v":6.5934343434343434},null,null,{"$f":"IF(OR($L$75=\"Disable\",I79=\"\",$C$119=\"Baseline\"),D79,I79)","v":2},"HX Approach (°F)"]
[]
[null,"Calculation Engine"]
[null,null,null,null,null,"Baseline Trended Data",null,null,null,null,null,null,"Proposed Tended Data"]
[null,null,"OAT","Average WBT","Hours"," CHWST (°F)","CWST (°F)","Cooling Load (tons)","SCHWP Speed","# CWP","CWP Speed","Head in ft"," CHWST (°F)2","CWST (°F)3","Cooling Load (tons)3","SCHWP Speed3","# CWP2","CWP Speed2","Head in ft2","CHWST (°F)","CWST (°F)2","Cooling Load (tons)2","CT Load (Tons)","SCHWP Speed2","CWP Qty","CWP Speed3","SCHWP Qty","SCHWP Head","Econ Engaged","CH Stage","CT Stage","Chiller Load kW","Chiller Load kWh","PCHWP kW","PCHWP kWh","SCHWP kW","SCHWP kWh","Chiller kW","Chiller kWh","CT Fan kW","CT Fan  kWh","CWP kW","CWP kWh"]
[null,null,115,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H138),FORECAST(C138,$H$138:$H$243,$C$138:$C$243),H138),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O138),FORECAST(C138,$O$138:$O$243,$C$138:$C$243),O138),\nIF(C138>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C138),0),0))))","v":0},{"$f":"IF(E138>0,V138*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"ROUNDUP(IF(C138<$N$131,0,IF(C138>=$H$30,$H$29,IF(C138<$I$30,$I$29,TREND($H$29:$I$29,$H$30:$I$30,C138,TRUE)))),0)","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},{"$f":"AND(SUM(D138,$I$131,$I$133)<=T138,D138<=$I$132)","v":false},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},{"$f":"AF138*E138","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,114,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H139),FORECAST(C139,$H$138:$H$243,$C$138:$C$243),H139),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O139),FORECAST(C139,$O$138:$O$243,$C$138:$C$243),O139),\nIF(C139>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C139),0),0))))","v":0},{"$f":"IF(E139>0,V139*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},{"$f":"AND(SUM(D139,$I$131,$I$133)<=T139,D139<=$I$132)","v":false},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,113,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H140),FORECAST(C140,$H$138:$H$243,$C$138:$C$243),H140),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O140),FORECAST(C140,$O$138:$O$243,$C$138:$C$243),O140),\nIF(C140>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C140),0),0))))","v":0},{"$f":"IF(E140>0,V140*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,112,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H141),FORECAST(C141,$H$138:$H$243,$C$138:$C$243),H141),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O141),FORECAST(C141,$O$138:$O$243,$C$138:$C$243),O141),\nIF(C141>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C141),0),0))))","v":0},{"$f":"IF(E141>0,V141*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,111,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H142),FORECAST(C142,$H$138:$H$243,$C$138:$C$243),H142),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O142),FORECAST(C142,$O$138:$O$243,$C$138:$C$243),O142),\nIF(C142>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C142),0),0))))","v":0},{"$f":"IF(E142>0,V142*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,110,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H143),FORECAST(C143,$H$138:$H$243,$C$138:$C$243),H143),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O143),FORECAST(C143,$O$138:$O$243,$C$138:$C$243),O143),\nIF(C143>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C143),0),0))))","v":0},{"$f":"IF(E143>0,V143*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,109,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H144),FORECAST(C144,$H$138:$H$243,$C$138:$C$243),H144),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O144),FORECAST(C144,$O$138:$O$243,$C$138:$C$243),O144),\nIF(C144>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C144),0),0))))","v":0},{"$f":"IF(E144>0,V144*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,108,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H145),FORECAST(C145,$H$138:$H$243,$C$138:$C$243),H145),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O145),FORECAST(C145,$O$138:$O$243,$C$138:$C$243),O145),\nIF(C145>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C145),0),0))))","v":0},{"$f":"IF(E145>0,V145*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,107,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H146),FORECAST(C146,$H$138:$H$243,$C$138:$C$243),H146),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O146),FORECAST(C146,$O$138:$O$243,$C$138:$C$243),O146),\nIF(C146>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C146),0),0))))","v":0},{"$f":"IF(E146>0,V146*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,106,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H147),FORECAST(C147,$H$138:$H$243,$C$138:$C$243),H147),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O147),FORECAST(C147,$O$138:$O$243,$C$138:$C$243),O147),\nIF(C147>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C147),0),0))))","v":0},{"$f":"IF(E147>0,V147*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,105,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H148),FORECAST(C148,$H$138:$H$243,$C$138:$C$243),H148),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O148),FORECAST(C148,$O$138:$O$243,$C$138:$C$243),O148),\nIF(C148>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C148),0),0))))","v":0},{"$f":"IF(E148>0,V148*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,104,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H149),FORECAST(C149,$H$138:$H$243,$C$138:$C$243),H149),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O149),FORECAST(C149,$O$138:$O$243,$C$138:$C$243),O149),\nIF(C149>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C149),0),0))))","v":0},{"$f":"IF(E149>0,V149*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,103,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H150),FORECAST(C150,$H$138:$H$243,$C$138:$C$243),H150),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O150),FORECAST(C150,$O$138:$O$243,$C$138:$C$243),O150),\nIF(C150>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C150),0),0))))","v":0},{"$f":"IF(E150>0,V150*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,102,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H151),FORECAST(C151,$H$138:$H$243,$C$138:$C$243),H151),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O151),FORECAST(C151,$O$138:$O$243,$C$138:$C$243),O151),\nIF(C151>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C151),0),0))))","v":0},{"$f":"IF(E151>0,V151*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,101,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H152),FORECAST(C152,$H$138:$H$243,$C$138:$C$243),H152),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O152),FORECAST(C152,$O$138:$O$243,$C$138:$C$243),O152),\nIF(C152>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C152),0),0))))","v":0},{"$f":"IF(E152>0,V152*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,100,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H153),FORECAST(C153,$H$138:$H$243,$C$138:$C$243),H153),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O153),FORECAST(C153,$O$138:$O$243,$C$138:$C$243),O153),\nIF(C153>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C153),0),0))))","v":0},{"$f":"IF(E153>0,V153*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,99,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H154),FORECAST(C154,$H$138:$H$243,$C$138:$C$243),H154),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O154),FORECAST(C154,$O$138:$O$243,$C$138:$C$243),O154),\nIF(C154>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C154),0),0))))","v":0},{"$f":"IF(E154>0,V154*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,98,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H155),FORECAST(C155,$H$138:$H$243,$C$138:$C$243),H155),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O155),FORECAST(C155,$O$138:$O$243,$C$138:$C$243),O155),\nIF(C155>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C155),0),0))))","v":0},{"$f":"IF(E155>0,V155*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,97,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H156),FORECAST(C156,$H$138:$H$243,$C$138:$C$243),H156),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O156),FORECAST(C156,$O$138:$O$243,$C$138:$C$243),O156),\nIF(C156>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C156),0),0))))","v":0},{"$f":"IF(E156>0,V156*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,96,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H157),FORECAST(C157,$H$138:$H$243,$C$138:$C$243),H157),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O157),FORECAST(C157,$O$138:$O$243,$C$138:$C$243),O157),\nIF(C157>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C157),0),0))))","v":0},{"$f":"IF(E157>0,V157*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,95,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H158),FORECAST(C158,$H$138:$H$243,$C$138:$C$243),H158),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O158),FORECAST(C158,$O$138:$O$243,$C$138:$C$243),O158),\nIF(C158>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C158),0),0))))","v":0},{"$f":"IF(E158>0,V158*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,94,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H159),FORECAST(C159,$H$138:$H$243,$C$138:$C$243),H159),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O159),FORECAST(C159,$O$138:$O$243,$C$138:$C$243),O159),\nIF(C159>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C159),0),0))))","v":0},{"$f":"IF(E159>0,V159*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,93,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H160),FORECAST(C160,$H$138:$H$243,$C$138:$C$243),H160),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O160),FORECAST(C160,$O$138:$O$243,$C$138:$C$243),O160),\nIF(C160>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C160),0),0))))","v":0},{"$f":"IF(E160>0,V160*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,92,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H161),FORECAST(C161,$H$138:$H$243,$C$138:$C$243),H161),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O161),FORECAST(C161,$O$138:$O$243,$C$138:$C$243),O161),\nIF(C161>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C161),0),0))))","v":0},{"$f":"IF(E161>0,V161*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,91,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":64},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H162),FORECAST(C162,$H$138:$H$243,$C$138:$C$243),H162),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O162),FORECAST(C162,$O$138:$O$243,$C$138:$C$243),O162),\nIF(C162>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C162),0),0))))","v":1434.2857142857142},{"$f":"IF(E162>0,V162*'Chilled Water System Template'!$C$131,0)","v":1792.8571428571427},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":4},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":667.37314285714285},667.37314285714285,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6.5934343434343425},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":68.968284809371056},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":742.93486200994823},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":742.93486200994823},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":31.392913405865169},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":31.392913405865169},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":46.541889483065951}]
[null,null,90,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H163),FORECAST(C163,$H$138:$H$243,$C$138:$C$243),H163),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O163),FORECAST(C163,$O$138:$O$243,$C$138:$C$243),O163),\nIF(C163>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C163),0),0))))","v":0},{"$f":"IF(E163>0,V163*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,89,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":64},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H164),FORECAST(C164,$H$138:$H$243,$C$138:$C$243),H164),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O164),FORECAST(C164,$O$138:$O$243,$C$138:$C$243),O164),\nIF(C164>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C164),0),0))))","v":1365.7142857142858},{"$f":"IF(E164>0,V164*'Chilled Water System Template'!$C$131,0)","v":1707.1428571428573},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":635.46685714285718},3177.3342857142861,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":32.967171717171709},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":344.84142404685531},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":711.02857629566256},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":3555.142881478313},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":27.774232759697277},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":138.87116379848638},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":232.70944741532975}]
[null,null,88,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":66.333333333333329},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H165),FORECAST(C165,$H$138:$H$243,$C$138:$C$243),H165),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O165),FORECAST(C165,$O$138:$O$243,$C$138:$C$243),O165),\nIF(C165>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C165),0),0))))","v":1331.4285714285711},{"$f":"IF(E165>0,V165*'Chilled Water System Template'!$C$131,0)","v":1664.2857142857138},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":619.51371428571417},1858.5411428571424,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":19.780303030303028},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":206.90485442811317},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":695.07543343851955},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":2085.2263003155585},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":26.063763182443431},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":78.191289547330285},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":139.62566844919786}]
[null,null,87,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":67.8},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H166),FORECAST(C166,$H$138:$H$243,$C$138:$C$243),H166),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O166),FORECAST(C166,$O$138:$O$243,$C$138:$C$243),O166),\nIF(C166>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C166),0),0))))","v":1297.1428571428569},{"$f":"IF(E166>0,V166*'Chilled Water System Template'!$C$131,0)","v":1621.4285714285711},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":603.56057142857128},3017.8028571428563,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":32.967171717171709},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":344.84142404685531},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":679.12229058137666},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":3395.6114529068836},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":24.418105250572566},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":122.09052625286283},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":232.70944741532975}]
[null,null,86,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":66.7},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":10},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H167),FORECAST(C167,$H$138:$H$243,$C$138:$C$243),H167),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O167),FORECAST(C167,$O$138:$O$243,$C$138:$C$243),O167),\nIF(C167>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C167),0),0))))","v":1262.8571428571427},{"$f":"IF(E167>0,V167*'Chilled Water System Template'!$C$131,0)","v":1578.5714285714284},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":587.6074285714285},5876.074285714285,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":65.934343434343418},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":689.68284809371062},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":663.16914772423388},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":6631.6914772423388},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":22.836418989512012},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":228.36418989512012},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":465.4188948306595}]
[null,null,85,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":66.166666666666671},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H168),FORECAST(C168,$H$138:$H$243,$C$138:$C$243),H168),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O168),FORECAST(C168,$O$138:$O$243,$C$138:$C$243),O168),\nIF(C168>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C168),0),0))))","v":1228.5714285714284},{"$f":"IF(E168>0,V168*'Chilled Water System Template'!$C$131,0)","v":1535.7142857142856},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":571.65428571428561},3429.9257142857136,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":39.560606060606055},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":413.80970885622634},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":647.21600486709099},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":3883.2960292025459},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":21.317853246420082},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":127.90711947852049},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":279.25133689839572}]
[null,null,84,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":63.125},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H169),FORECAST(C169,$H$138:$H$243,$C$138:$C$243),H169),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O169),FORECAST(C169,$O$138:$O$243,$C$138:$C$243),O169),\nIF(C169>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C169),0),0))))","v":1194.2857142857142},{"$f":"IF(E169>0,V169*'Chilled Water System Template'!$C$131,0)","v":1492.8571428571427},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":555.70114285714283},4445.6091428571426,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":52.74747474747474},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":551.74627847496845},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":631.26286200994821},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":5050.1028960795857},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":19.861545231606485},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":158.89236185285188},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":372.33511586452761}]
[null,null,83,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":65.8},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":15},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H170),FORECAST(C170,$H$138:$H$243,$C$138:$C$243),H170),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O170),FORECAST(C170,$O$138:$O$243,$C$138:$C$243),O170),\nIF(C170>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C170),0),0))))","v":1160},{"$f":"IF(E170>0,V170*'Chilled Water System Template'!$C$131,0)","v":1450},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},{"$f":"AND(SUM(D170,$I$131,$I$133)<=T170,D170<=$I$132)","v":false},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":539.74799999999993},{"$f":"AF170*E170","v":8096.2199999999993},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":98.901515151515142},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1034.5242721405659},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":615.30971915280531},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":9229.6457872920819},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":18.466620027708963},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":276.99930041563442},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":698.1283422459893}]
[null,null,82,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":66.333333333333329},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":15},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H171),FORECAST(C171,$H$138:$H$243,$C$138:$C$243),H171),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O171),FORECAST(C171,$O$138:$O$243,$C$138:$C$243),O171),\nIF(C171>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C171),0),0))))","v":1125.7142857142858},{"$f":"IF(E171>0,V171*'Chilled Water System Template'!$C$131,0)","v":1407.1428571428573},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":523.79485714285715},7856.9228571428575,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":98.901515151515142},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1034.5242721405659},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":599.35657629566253},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":8990.3486444349383},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":17.132190063359332},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":256.98285095039},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":698.1283422459893}]
[null,null,81,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":66.900000000000006},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":10},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H172),FORECAST(C172,$H$138:$H$243,$C$138:$C$243),H172),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O172),FORECAST(C172,$O$138:$O$243,$C$138:$C$243),O172),\nIF(C172>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C172),0),0))))","v":1091.4285714285711},{"$f":"IF(E172>0,V172*'Chilled Water System Template'!$C$131,0)","v":1364.2857142857138},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":507.84171428571415},5078.4171428571417,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":65.934343434343418},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":689.68284809371062},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":583.40343343851953},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":5834.0343343851964},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":15.857354547634191},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":158.57354547634191},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":465.4188948306595}]
[null,null,80,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":65.178571428571431},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":28},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H173),FORECAST(C173,$H$138:$H$243,$C$138:$C$243),H173),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O173),FORECAST(C173,$O$138:$O$243,$C$138:$C$243),O173),\nIF(C173>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C173),0),0))))","v":1057.1428571428569},{"$f":"IF(E173>0,V173*'Chilled Water System Template'!$C$131,0)","v":1321.4285714285711},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":491.88857142857131},13772.879999999997,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":184.61616161616161},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":68.968284809371056},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1931.1119746623895},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":567.45029058137675},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":15888.608136278548},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":14.641198861072866},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":409.95356811004024},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1303.1729055258465}]
[null,null,79,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":65.407407407407405},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":27},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H174),FORECAST(C174,$H$138:$H$243,$C$138:$C$243),H174),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O174),FORECAST(C174,$O$138:$O$243,$C$138:$C$243),O174),\nIF(C174>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C174),0),0))))","v":1022.8571428571427},{"$f":"IF(E174>0,V174*'Chilled Water System Template'!$C$131,0)","v":1278.5714285714284},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.96},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":475.93542857142853},12850.25657142857,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":178.02272727272725},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":66.209553416996215},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1787.6579422588977},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":548.73841633185907},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":14815.937240960197},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":13.482793898443035},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":364.03543525796192},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1256.6310160427806}]
[null,null,78,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":65.393939393939391},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":33},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H175),FORECAST(C175,$H$138:$H$243,$C$138:$C$243),H175),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O175),FORECAST(C175,$O$138:$O$243,$C$138:$C$243),O175),\nIF(C175>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C175),0),0))))","v":988.57142857142844},{"$f":"IF(E175>0,V175*'Chilled Water System Template'!$C$131,0)","v":1235.7142857142856},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.91999999999999993},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":459.98228571428564},15179.415428571427,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":217.58333333333331},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":63.450822024621353},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2093.8771268125047},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":530.02654208234139},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":17490.875888717266},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":12.381195357725442},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":408.57944680493961},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1535.8823529411764}]
[null,null,77,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":65.45},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":20},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H176),FORECAST(C176,$H$138:$H$243,$C$138:$C$243),H176),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O176),FORECAST(C176,$O$138:$O$243,$C$138:$C$243),O176),\nIF(C176>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C176),0),0))))","v":954.28571428571422},{"$f":"IF(E176>0,V176*'Chilled Water System Template'!$C$131,0)","v":1192.8571428571427},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.87999999999999989},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":444.02914285714286},8880.5828571428574,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":131.86868686868684},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":60.692090632246526},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1213.8418126449305},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":511.31466783282372},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":10226.293356656475},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":11.335442968945078},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":226.70885937890154},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":930.83778966131899}]
[null,null,76,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":64.819999999999993},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":50},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H177),FORECAST(C177,$H$138:$H$243,$C$138:$C$243),H177),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O177),FORECAST(C177,$O$138:$O$243,$C$138:$C$243),O177),\nIF(C177>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C177),0),0))))","v":920},{"$f":"IF(E177>0,V177*'Chilled Water System Template'!$C$131,0)","v":1150},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.83999999999999986},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":428.07600000000002},21403.800000000003,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":329.67171717171715},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":57.93335923987167},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2896.6679619935835},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":492.60279358330604},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":24630.139679165302},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":10.344559655472255},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":517.22798277361278},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2327.0944741532976}]
[null,null,75,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":64.319148936170208},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":46},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H178),FORECAST(C178,$H$138:$H$243,$C$138:$C$243),H178),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O178),FORECAST(C178,$O$138:$O$243,$C$138:$C$243),O178),\nIF(C178>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C178),0),0))))","v":885.71428571428578},{"$f":"IF(E178>0,V178*'Chilled Water System Template'!$C$131,0)","v":1107.1428571428573},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.80000000000000027},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":412.12285714285719},18957.651428571429,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":303.29797979797974},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":55.174627847496858},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2538.0328809848556},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":473.89091933378842},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":21798.982289354262},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":9.4075506192107188},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":432.74732848369308},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2140.9269162210339}]
[null,null,74,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":64.73770491803279},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":60},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H179),FORECAST(C179,$H$138:$H$243,$C$138:$C$243),H179),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O179),FORECAST(C179,$O$138:$O$243,$C$138:$C$243),O179),\nIF(C179>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C179),0),0))))","v":851.4285714285711},{"$f":"IF(E179>0,V179*'Chilled Water System Template'!$C$131,0)","v":1064.2857142857138},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.76000000000000023},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":396.16971428571418},23770.182857142852,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":395.60606060606057},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":52.415896455122017},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3144.9537873073209},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":455.17904508427057},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":27310.742705056233},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":8.523402339634238},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":511.40414037805431},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2792.5133689839572}]
[null,null,73,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":63.191176470588232},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":65},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H180),FORECAST(C180,$H$138:$H$243,$C$138:$C$243),H180),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O180),FORECAST(C180,$O$138:$O$243,$C$138:$C$243),O180),\nIF(C180>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C180),0),0))))","v":817.14285714285688},{"$f":"IF(E180>0,V180*'Chilled Water System Template'!$C$131,0)","v":1021.4285714285711},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.7200000000000002},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":380.21657142857134},24714.077142857139,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":428.57323232323228},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":49.657165062747175},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3227.7157290785663},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":436.46717083475289},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":28370.366104258937},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":7.6910814748631138},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":499.92029586610238},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3025.2228163992868}]
[null,null,72,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":62.5625},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":77},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H181),FORECAST(C181,$H$138:$H$243,$C$138:$C$243),H181),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O181),FORECAST(C181,$O$138:$O$243,$C$138:$C$243),O181),\nIF(C181>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C181),0),0))))","v":782.85714285714266},{"$f":"IF(E181>0,V181*'Chilled Water System Template'!$C$131,0)","v":978.57142857142833},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.68000000000000016},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":364.26342857142851},28048.283999999996,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":507.6944444444444},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":46.89843367037232},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3611.1793926186688},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":417.75529658523516},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":32167.15783706311},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":6.9095336508052148},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":532.03409111200153},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3583.7254901960782}]
[null,null,71,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":62.306569343065696},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":133},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H182),FORECAST(C182,$H$138:$H$243,$C$138:$C$243),H182),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O182),FORECAST(C182,$O$138:$O$243,$C$138:$C$243),O182),\nIF(C182>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C182),0),0))))","v":748.57142857142844},{"$f":"IF(E182>0,V182*'Chilled Water System Template'!$C$131,0)","v":935.71428571428555},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.64000000000000012},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":348.31028571428567},46325.267999999996,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":876.92676767676755},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":44.139702277997479},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":5870.5804029736646},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":399.04342233571748},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":53072.775170650435},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":6.1776821217127509},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":821.63172218779584},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6190.0713012477718}]
[null,null,70,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":61.387387387387385},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":103},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H183),FORECAST(C183,$H$138:$H$243,$C$138:$C$243),H183),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O183),FORECAST(C183,$O$138:$O$243,$C$138:$C$243),O183),\nIF(C183>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C183),0),0))))","v":714.28571428571422},{"$f":"IF(E183>0,V183*'Chilled Water System Template'!$C$131,0)","v":892.85714285714278},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.60000000000000009},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":3},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":3},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":332.35714285714283},34232.78571428571,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343425},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":679.1237373737373},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":41.380970885622631},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4262.240001219131},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":380.3315480861998},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":39174.149452878577},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":5.4944262821784369},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":565.92590706437898},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4793.8146167557934}]
[null,null,69,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":60.68888888888889},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":124},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H184),FORECAST(C184,$H$138:$H$243,$C$138:$C$243),H184),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O184),FORECAST(C184,$O$138:$O$243,$C$138:$C$243),O184),\nIF(C184>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C184),0),0))))","v":680},{"$f":"IF(E184>0,V184*'Chilled Water System Template'!$C$131,0)","v":850},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.56000000000000005},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":316.40400000000005},39234.096000000005,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":817.58585858585855},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":38.62223949324779},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4789.1576971627255},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":361.61967383668218},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":44840.839555748593},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":75.738702121209215},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":9391.599063029942},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":5771.1942959001781}]
[null,null,68,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":60.456521739130437},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":131},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H185),FORECAST(C185,$H$138:$H$243,$C$138:$C$243),H185),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O185),FORECAST(C185,$O$138:$O$243,$C$138:$C$243),O185),\nIF(C185>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C185),0),0))))","v":645.71428571428578},{"$f":"IF(E185>0,V185*'Chilled Water System Template'!$C$131,0)","v":807.14285714285722},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.52000000000000046},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":300.45085714285722},39359.062285714295,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":863.73989898989896},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":35.863508100872977},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4698.1195612143601},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":342.90779958716456},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":44920.92174591856},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":66.549770769728312},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":8718.019970834408},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6096.9875222816399}]
[null,null,67,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":59.6},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":157},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H186),FORECAST(C186,$H$138:$H$243,$C$138:$C$243),H186),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O186),FORECAST(C186,$O$138:$O$243,$C$138:$C$243),O186),\nIF(C186>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C186),0),0))))","v":611.4285714285711},{"$f":"IF(E186>0,V186*'Chilled Water System Template'!$C$131,0)","v":764.28571428571388},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.48000000000000043},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":284.49771428571415},44666.141142857123,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1035.1691919191919},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":33.104776708498136},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":5197.4499432342072},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":324.19592533764666},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":50898.760278010523},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":58.064394212725738},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":9116.1098913979404},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":7307.0766488413547}]
[null,null,66,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":59.109090909090909},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":149},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H187),FORECAST(C187,$H$138:$H$243,$C$138:$C$243),H187),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O187),FORECAST(C187,$O$138:$O$243,$C$138:$C$243),O187),\nIF(C187>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C187),0),0))))","v":577.14285714285688},{"$f":"IF(E187>0,V187*'Chilled Water System Template'!$C$131,0)","v":721.4285714285711},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.44000000000000039},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},2,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":268.54457142857132},40013.141142857123,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":982.42171717171721},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":30.346045316123284},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4521.5607521023694},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":305.48405108812898},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":45517.12361213121},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":50.263634610945857},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":7489.2815570309331},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6934.7415329768264}]
[null,null,65,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":58.456621004566209},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":177},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H188),FORECAST(C188,$H$138:$H$243,$C$138:$C$243),H188),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O188),FORECAST(C188,$O$138:$O$243,$C$138:$C$243),O188),\nIF(C188>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C188),0),0))))","v":542.85714285714266},{"$f":"IF(E188>0,V188*'Chilled Water System Template'!$C$131,0)","v":678.57142857142833},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.40000000000000036},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":252.59142857142851},44708.682857142849,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1167.0378787878788},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":13.793656961874223},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2441.4772822517375},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":272.97851987673704},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":48317.198018182469},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":43.128014854338154},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":7633.6586292178536},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":8237.9144385026739}]
[null,null,64,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":57.853061224489792},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":187},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H189),FORECAST(C189,$H$138:$H$243,$C$138:$C$243),H189),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O189),FORECAST(C189,$O$138:$O$243,$C$138:$C$243),O189),\nIF(C189>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C189),0),0))))","v":508.57142857142844},{"$f":"IF(E189>0,V189*'Chilled Water System Template'!$C$131,0)","v":635.71428571428555},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.36000000000000032},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":236.63828571428567},44251.359428571421,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1232.9722222222222},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":12.414291265686801},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2321.4724666834318},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":255.64601132340684},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":47805.80411747707},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":36.637469659244204},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6851.2068262786661},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":8703.3333333333321}]
[null,null,63,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":57.094999999999999},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":153},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H190),FORECAST(C190,$H$138:$H$243,$C$138:$C$243),H190),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O190),FORECAST(C190,$O$138:$O$243,$C$138:$C$243),O190),\nIF(C190>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C190),0),0))))","v":474.28571428571422},{"$f":"IF(E190>0,V190*'Chilled Water System Template'!$C$131,0)","v":592.85714285714278},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.32000000000000028},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":220.68514285714284},33764.826857142856,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1008.7954545454545},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":11.034925569499379},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1688.343612133405},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":238.31350277007658},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":36461.965923821714},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":30.771288789360405},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4708.007184772142},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":7120.9090909090901}]
[null,null,62,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":56.990384615384613},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":202},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H191),FORECAST(C191,$H$138:$H$243,$C$138:$C$243),H191),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O191),FORECAST(C191,$O$138:$O$243,$C$138:$C$243),O191),\nIF(C191>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C191),0),0))))","v":440},{"$f":"IF(E191>0,V191*'Chilled Water System Template'!$C$131,0)","v":550},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.28000000000000025},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":204.73200000000003},41355.864000000009,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1331.8737373737374},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":9.6555598733119563},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1950.4230944090152},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":220.98099421674632},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":44638.160831782763},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":25.508050499604881},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":5152.6262009201855},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":9401.4616755793213}]
[null,null,61,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":55.976676384839649},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":218},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H192),FORECAST(C192,$H$138:$H$243,$C$138:$C$243),H192),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O192),FORECAST(C192,$O$138:$O$243,$C$138:$C$243),O192),\nIF(C192>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C192),0),0))))","v":405.71428571428578},{"$f":"IF(E192>0,V192*'Chilled Water System Template'!$C$131,0)","v":507.14285714285722},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.24000000000000021},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":188.77885714285719},41153.790857142871,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1437.3686868686868},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":8.276194177124534},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1804.2103306131485},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":203.64848566341607},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":44395.369874624703},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":20.825542667477741},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4539.9683015101473},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":46.541889483065951},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":10146.131907308378}]
[null,null,60,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":55.359743040685224},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":268},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H193),FORECAST(C193,$H$138:$H$243,$C$138:$C$243),H193),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O193),FORECAST(C193,$O$138:$O$243,$C$138:$C$243),O193),\nIF(C193>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C193),0),0))))","v":371.4285714285711},{"$f":"IF(E193>0,V193*'Chilled Water System Template'!$C$131,0)","v":464.28571428571388},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.20000000000000018},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":172.82571428571416},46317.291428571392,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1767.0404040404039},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371116},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1848.3500328911459},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":186.31597711008561},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":49932.681865502942},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":16.70066816180907},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4475.7790673648306},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6236.6131907308372}]
[null,null,59,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":54.808791208791206},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C194,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C194,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C194,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":243},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H194),FORECAST(C194,$H$138:$H$243,$C$138:$C$243),H194),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O194),FORECAST(C194,$O$138:$O$243,$C$138:$C$243),O194),\nIF(C194>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C194),0),0))))","v":337.14285714285711},{"$f":"IF(E194>0,V194*'Chilled Water System Template'!$C$131,0)","v":421.42857142857139},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":156.8725714285714},38120.034857142855,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1602.2045454545455},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1675.9293208677168},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":170.36283425294286},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":41398.168723465118},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":13.109329644645396},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3185.5671036488311},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":5654.8395721925126}]
[null,null,58,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":54.029357798165137},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C195,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C195,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C195,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":297},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H195),FORECAST(C195,$H$138:$H$243,$C$138:$C$243),H195),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O195),FORECAST(C195,$O$138:$O$243,$C$138:$C$243),O195),\nIF(C195>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C195),0),0))))","v":302.85714285714266},{"$f":"IF(E195>0,V195*'Chilled Water System Template'!$C$131,0)","v":378.57142857142833},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":140.91942857142848},41853.070285714261,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1958.25},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2048.3580588383206},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":154.40969139579994},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":45859.67834455258},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":10.026286934303805},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2977.8072194882302},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6911.4705882352937}]
[null,null,57,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":53.540948275862071},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C196,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C196,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C196,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":234},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H196),FORECAST(C196,$H$138:$H$243,$C$138:$C$243),H196),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O196),FORECAST(C196,$O$138:$O$243,$C$138:$C$243),O196),\nIF(C196>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C196),0),0))))","v":268.57142857142844},{"$f":"IF(E196>0,V196*'Chilled Water System Template'!$C$131,0)","v":335.71428571428555},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":124.96628571428568},29242.110857142849,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1542.8636363636363},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1613.8578645392829},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":138.45654853865713},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":32398.832358045769},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":7.4249767832403881},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1737.4445672782508},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":5445.4010695187162}]
[null,null,56,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":52.444015444015442},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C197,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C197,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C197,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":264},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H197),FORECAST(C197,$H$138:$H$243,$C$138:$C$243),H197),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O197),FORECAST(C197,$O$138:$O$243,$C$138:$C$243),O197),\nIF(C197>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C197),0),0))))","v":234.28571428571422},{"$f":"IF(E197>0,V197*'Chilled Water System Template'!$C$131,0)","v":292.85714285714278},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":109.01314285714284},28779.469714285711,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1740.6666666666667},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1820.762718967396},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":122.50340568151428},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":32340.899099919774},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":5.2772795085074033},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1393.2017902459545},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":6143.5294117647054}]
[null,null,55,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":51.470715835141},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C198,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C198,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C198,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":214},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H198),FORECAST(C198,$H$138:$H$243,$C$138:$C$243),H198),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O198),FORECAST(C198,$O$138:$O$243,$C$138:$C$243),O198),\nIF(C198>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C198),0),0))))","v":199.99999999999977},{"$f":"IF(E198>0,V198*'Chilled Water System Template'!$C$131,0)","v":249.99999999999972},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":93.059999999999903},19914.839999999978,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1410.9949494949494},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1475.9212949205407},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":106.55026282437134},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":22801.756244415468},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":3.5532074666402886},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":760.38639786102181},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4979.9821746880571}]
[null,null,54,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":50.649532710280376},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C199,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C199,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C199,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":187},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H199),FORECAST(C199,$H$138:$H$243,$C$138:$C$243),H199),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O199),FORECAST(C199,$O$138:$O$243,$C$138:$C$243),O199),\nIF(C199>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C199),0),0))))","v":165.71428571428555},{"$f":"IF(E199>0,V199*'Chilled Water System Template'!$C$131,0)","v":207.14285714285694},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":77.106857142857081},14418.982285714274,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1232.9722222222222},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1289.7069259352388},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":90.597119967228522},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":16941.661433871734},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":2.2204727608241184},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":415.22840627411011},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4351.6666666666661}]
[null,null,53,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":49.739856801909305},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C200,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C200,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C200,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":185},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H200),FORECAST(C200,$H$138:$H$243,$C$138:$C$243),H200),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O200),FORECAST(C200,$O$138:$O$243,$C$138:$C$243),O200),\nIF(C200>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C200),0),0))))","v":131.42857142857133},{"$f":"IF(E200>0,V200*'Chilled Water System Template'!$C$131,0)","v":164.28571428571416},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":61.153714285714244},11313.437142857136,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1219.7853535353536},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1275.9132689733647},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":74.643977110085686},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":13809.135765365854},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":1.4566850601269703},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":269.48673612348949},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":4305.1247771836006}]
[null,null,52,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":48.656424581005588},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C201,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C201,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C201,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":152},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H201),FORECAST(C201,$H$138:$H$243,$C$138:$C$243),H201),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O201),FORECAST(C201,$O$138:$O$243,$C$138:$C$243),O201),\nIF(C201>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C201),0),0))))","v":97.14285714285711},{"$f":"IF(E201>0,V201*'Chilled Water System Template'!$C$131,0)","v":121.42857142857139},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":45.200571428571415},6870.4868571428551,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1002.2020202020202},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1048.3179291024401},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":58.690834252942864},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":8921.0068064473162},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":1.4566850601269703},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":221.41612913929947},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3537.1836007130123}]
[null,null,51,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":47.901685393258425},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C202,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C202,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C202,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":160},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H202),FORECAST(C202,$H$138:$H$243,$C$138:$C$243),H202),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O202),FORECAST(C202,$O$138:$O$243,$C$138:$C$243),O202),\nIF(C202>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C202),0),0))))","v":62.857142857142662},{"$f":"IF(E202>0,V202*'Chilled Water System Template'!$C$131,0)","v":78.571428571428328},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},{"$f":"ROUNDUP(IF(C202<$N$131,0,IF(C202>=$H$30,$H$29,IF(C202<$I$30,$I$29,TREND($H$29:$I$29,$H$30:$I$30,C202,TRUE)))),0)","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},{"$f":"AND(SUM(D202,$I$131,$I$133)<=T202,D202<=$I$132)","v":false},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":29.247428571428486},{"$f":"AF202*E202","v":4679.5885714285578},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1054.9494949494949},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1103.4925569499369},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":42.737691395799942},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":6838.0306233279898},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":1.4566850601269703},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":233.06960962031525},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":3723.351158645276}]
[null,null,50,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":46.942857142857143},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C203,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C203,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C203,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":98},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H203),FORECAST(C203,$H$138:$H$243,$C$138:$C$243),H203),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O203),FORECAST(C203,$O$138:$O$243,$C$138:$C$243),O203),\nIF(C203>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C203),0),0))))","v":28.571428571428442},{"$f":"IF(E203>0,V203*'Chilled Water System Template'!$C$131,0)","v":35.714285714285552},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},1,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":1},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":13.294285714285655},1302.8399999999942,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":6.5934343434343434},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":646.1565656565657},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":6.8968284809371063},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":675.88919113183647},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":26.784548538657106},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":2624.8857567883965},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":1.4566850601269703},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":142.75513589244309},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2280.5525846702317}]
[null,null,49,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":45.992481203007522},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C204,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C204,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C204,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":106},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H204),FORECAST(C204,$H$138:$H$243,$C$138:$C$243),H204),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O204),FORECAST(C204,$O$138:$O$243,$C$138:$C$243),O204),\nIF(C204>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C204),0),0))))","v":0},{"$f":"IF(E204>0,V204*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2466.7201426024953}]
[null,null,48,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":45.185929648241206},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C205,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C205,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C205,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":86},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H205),FORECAST(C205,$H$138:$H$243,$C$138:$C$243),H205),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O205),FORECAST(C205,$O$138:$O$243,$C$138:$C$243),O205),\nIF(C205>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C205),0),0))))","v":0},{"$f":"IF(E205>0,V205*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":2001.301247771836}]
[null,null,47,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":44.24},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C206,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C206,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C206,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":80},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H206),FORECAST(C206,$H$138:$H$243,$C$138:$C$243),H206),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O206),FORECAST(C206,$O$138:$O$243,$C$138:$C$243),O206),\nIF(C206>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C206),0),0))))","v":0},{"$f":"IF(E206>0,V206*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1861.675579322638}]
[null,null,46,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":42.944055944055947},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C207,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C207,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C207,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":64},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H207),FORECAST(C207,$H$138:$H$243,$C$138:$C$243),H207),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O207),FORECAST(C207,$O$138:$O$243,$C$138:$C$243),O207),\nIF(C207>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C207),0),0))))","v":0},{"$f":"IF(E207>0,V207*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1489.3404634581104}]
[null,null,45,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":42.29059829059829},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C208,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C208,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C208,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":54},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H208),FORECAST(C208,$H$138:$H$243,$C$138:$C$243),H208),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O208),FORECAST(C208,$O$138:$O$243,$C$138:$C$243),O208),\nIF(C208>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C208),0),0))))","v":0},{"$f":"IF(E208>0,V208*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1256.6310160427806}]
[null,null,44,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":40.954128440366972},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C209,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C209,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C209,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":46},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H209),FORECAST(C209,$H$138:$H$243,$C$138:$C$243),H209),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O209),FORECAST(C209,$O$138:$O$243,$C$138:$C$243),O209),\nIF(C209>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C209),0),0))))","v":0},{"$f":"IF(E209>0,V209*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":1070.463458110517}]
[null,null,43,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":40.481481481481481},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C210,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C210,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C210,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":28},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H210),FORECAST(C210,$H$138:$H$243,$C$138:$C$243),H210),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O210),FORECAST(C210,$O$138:$O$243,$C$138:$C$243),O210),\nIF(C210>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C210),0),0))))","v":0},{"$f":"IF(E210>0,V210*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":651.58645276292327}]
[null,null,42,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":39.394366197183096},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C211,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C211,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C211,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":40},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H211),FORECAST(C211,$H$138:$H$243,$C$138:$C$243),H211),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O211),FORECAST(C211,$O$138:$O$243,$C$138:$C$243),O211),\nIF(C211>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C211),0),0))))","v":0},{"$f":"IF(E211>0,V211*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":930.83778966131899}]
[null,null,41,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":38.641025641025642},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C212,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C212,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C212,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":17},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H212),FORECAST(C212,$H$138:$H$243,$C$138:$C$243),H212),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O212),FORECAST(C212,$O$138:$O$243,$C$138:$C$243),O212),\nIF(C212>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C212),0),0))))","v":0},{"$f":"IF(E212>0,V212*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":395.60606060606057}]
[null,null,40,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":37.415094339622641},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C213,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C213,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C213,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":28},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H213),FORECAST(C213,$H$138:$H$243,$C$138:$C$243),H213),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O213),FORECAST(C213,$O$138:$O$243,$C$138:$C$243),O213),\nIF(C213>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C213),0),0))))","v":0},{"$f":"IF(E213>0,V213*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":651.58645276292327}]
[null,null,39,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":36.200000000000003},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C214,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C214,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C214,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":16},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H214),FORECAST(C214,$H$138:$H$243,$C$138:$C$243),H214),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O214),FORECAST(C214,$O$138:$O$243,$C$138:$C$243),O214),\nIF(C214>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C214),0),0))))","v":0},{"$f":"IF(E214>0,V214*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":372.33511586452761}]
[null,null,38,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":35},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C215,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C215,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C215,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H215),FORECAST(C215,$H$138:$H$243,$C$138:$C$243),H215),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O215),FORECAST(C215,$O$138:$O$243,$C$138:$C$243),O215),\nIF(C215>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C215),0),0))))","v":0},{"$f":"IF(E215>0,V215*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":139.62566844919786}]
[null,null,37,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":34.384615384615387},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C216,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C216,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C216,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":7},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H216),FORECAST(C216,$H$138:$H$243,$C$138:$C$243),H216),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O216),FORECAST(C216,$O$138:$O$243,$C$138:$C$243),O216),\nIF(C216>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C216),0),0))))","v":0},{"$f":"IF(E216>0,V216*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":162.89661319073082}]
[null,null,36,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":33},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C217,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C217,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C217,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H217),FORECAST(C217,$H$138:$H$243,$C$138:$C$243),H217),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O217),FORECAST(C217,$O$138:$O$243,$C$138:$C$243),O217),\nIF(C217>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C217),0),0))))","v":0},{"$f":"IF(E217>0,V217*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":186.1675579322638}]
[null,null,35,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":32.5},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C218,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C218,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C218,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":45},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":75},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H218),FORECAST(C218,$H$138:$H$243,$C$138:$C$243),H218),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O218),FORECAST(C218,$O$138:$O$243,$C$138:$C$243),O218),\nIF(C218>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C218),0),0))))","v":0},{"$f":"IF(E218>0,V218*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0.2},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":1},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":1},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":104},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":23.270944741532976},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":93.083778966131902}]
[null,null,34,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":31.666666666666668},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C219,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C219,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C219,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H219),FORECAST(C219,$H$138:$H$243,$C$138:$C$243),H219),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O219),FORECAST(C219,$O$138:$O$243,$C$138:$C$243),O219),\nIF(C219>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C219),0),0))))","v":0},{"$f":"IF(E219>0,V219*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,33,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C220,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C220,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C220,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H220),FORECAST(C220,$H$138:$H$243,$C$138:$C$243),H220),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O220),FORECAST(C220,$O$138:$O$243,$C$138:$C$243),O220),\nIF(C220>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C220),0),0))))","v":0},{"$f":"IF(E220>0,V220*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,32,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C221,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C221,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C221,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H221),FORECAST(C221,$H$138:$H$243,$C$138:$C$243),H221),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O221),FORECAST(C221,$O$138:$O$243,$C$138:$C$243),O221),\nIF(C221>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C221),0),0))))","v":0},{"$f":"IF(E221>0,V221*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,31,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C222,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C222,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C222,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H222),FORECAST(C222,$H$138:$H$243,$C$138:$C$243),H222),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O222),FORECAST(C222,$O$138:$O$243,$C$138:$C$243),O222),\nIF(C222>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C222),0),0))))","v":0},{"$f":"IF(E222>0,V222*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,30,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C223,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C223,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C223,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H223),FORECAST(C223,$H$138:$H$243,$C$138:$C$243),H223),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O223),FORECAST(C223,$O$138:$O$243,$C$138:$C$243),O223),\nIF(C223>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C223),0),0))))","v":0},{"$f":"IF(E223>0,V223*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,29,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C224,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C224,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C224,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H224),FORECAST(C224,$H$138:$H$243,$C$138:$C$243),H224),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O224),FORECAST(C224,$O$138:$O$243,$C$138:$C$243),O224),\nIF(C224>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C224),0),0))))","v":0},{"$f":"IF(E224>0,V224*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,28,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C225,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C225,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C225,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H225),FORECAST(C225,$H$138:$H$243,$C$138:$C$243),H225),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O225),FORECAST(C225,$O$138:$O$243,$C$138:$C$243),O225),\nIF(C225>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C225),0),0))))","v":0},{"$f":"IF(E225>0,V225*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,27,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C226,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C226,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C226,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H226),FORECAST(C226,$H$138:$H$243,$C$138:$C$243),H226),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O226),FORECAST(C226,$O$138:$O$243,$C$138:$C$243),O226),\nIF(C226>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C226),0),0))))","v":0},{"$f":"IF(E226>0,V226*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,26,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C227,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C227,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C227,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H227),FORECAST(C227,$H$138:$H$243,$C$138:$C$243),H227),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O227),FORECAST(C227,$O$138:$O$243,$C$138:$C$243),O227),\nIF(C227>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C227),0),0))))","v":0},{"$f":"IF(E227>0,V227*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,25,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C228,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C228,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C228,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H228),FORECAST(C228,$H$138:$H$243,$C$138:$C$243),H228),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O228),FORECAST(C228,$O$138:$O$243,$C$138:$C$243),O228),\nIF(C228>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C228),0),0))))","v":0},{"$f":"IF(E228>0,V228*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,24,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C229,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C229,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C229,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H229),FORECAST(C229,$H$138:$H$243,$C$138:$C$243),H229),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O229),FORECAST(C229,$O$138:$O$243,$C$138:$C$243),O229),\nIF(C229>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C229),0),0))))","v":0},{"$f":"IF(E229>0,V229*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,23,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C230,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C230,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C230,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H230),FORECAST(C230,$H$138:$H$243,$C$138:$C$243),H230),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O230),FORECAST(C230,$O$138:$O$243,$C$138:$C$243),O230),\nIF(C230>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C230),0),0))))","v":0},{"$f":"IF(E230>0,V230*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,22,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C231,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C231,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C231,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H231),FORECAST(C231,$H$138:$H$243,$C$138:$C$243),H231),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O231),FORECAST(C231,$O$138:$O$243,$C$138:$C$243),O231),\nIF(C231>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C231),0),0))))","v":0},{"$f":"IF(E231>0,V231*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,21,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C232,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C232,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C232,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H232),FORECAST(C232,$H$138:$H$243,$C$138:$C$243),H232),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O232),FORECAST(C232,$O$138:$O$243,$C$138:$C$243),O232),\nIF(C232>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C232),0),0))))","v":0},{"$f":"IF(E232>0,V232*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,20,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C233,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C233,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C233,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H233),FORECAST(C233,$H$138:$H$243,$C$138:$C$243),H233),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O233),FORECAST(C233,$O$138:$O$243,$C$138:$C$243),O233),\nIF(C233>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C233),0),0))))","v":0},{"$f":"IF(E233>0,V233*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,19,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C234,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C234,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C234,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H234),FORECAST(C234,$H$138:$H$243,$C$138:$C$243),H234),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O234),FORECAST(C234,$O$138:$O$243,$C$138:$C$243),O234),\nIF(C234>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C234),0),0))))","v":0},{"$f":"IF(E234>0,V234*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},{"$f":"AND(SUM(D234,$I$131,$I$133)<=T234,D234<=$I$132)","v":false},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},{"$f":"AF234*E234","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,18,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C235,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C235,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C235,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H235),FORECAST(C235,$H$138:$H$243,$C$138:$C$243),H235),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O235),FORECAST(C235,$O$138:$O$243,$C$138:$C$243),O235),\nIF(C235>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C235),0),0))))","v":0},{"$f":"IF(E235>0,V235*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,17,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C236,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C236,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C236,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H236),FORECAST(C236,$H$138:$H$243,$C$138:$C$243),H236),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O236),FORECAST(C236,$O$138:$O$243,$C$138:$C$243),O236),\nIF(C236>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C236),0),0))))","v":0},{"$f":"IF(E236>0,V236*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,16,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C237,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C237,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C237,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H237),FORECAST(C237,$H$138:$H$243,$C$138:$C$243),H237),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O237),FORECAST(C237,$O$138:$O$243,$C$138:$C$243),O237),\nIF(C237>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C237),0),0))))","v":0},{"$f":"IF(E237>0,V237*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,15,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C238,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C238,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C238,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H238),FORECAST(C238,$H$138:$H$243,$C$138:$C$243),H238),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O238),FORECAST(C238,$O$138:$O$243,$C$138:$C$243),O238),\nIF(C238>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C238),0),0))))","v":0},{"$f":"IF(E238>0,V238*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,14,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C239,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C239,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C239,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H239),FORECAST(C239,$H$138:$H$243,$C$138:$C$243),H239),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O239),FORECAST(C239,$O$138:$O$243,$C$138:$C$243),O239),\nIF(C239>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C239),0),0))))","v":0},{"$f":"IF(E239>0,V239*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,13,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C240,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C240,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C240,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H240),FORECAST(C240,$H$138:$H$243,$C$138:$C$243),H240),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O240),FORECAST(C240,$O$138:$O$243,$C$138:$C$243),O240),\nIF(C240>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C240),0),0))))","v":0},{"$f":"IF(E240>0,V240*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,12,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C241,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C241,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C241,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H241),FORECAST(C241,$H$138:$H$243,$C$138:$C$243),H241),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O241),FORECAST(C241,$O$138:$O$243,$C$138:$C$243),O241),\nIF(C241>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C241),0),0))))","v":0},{"$f":"IF(E241>0,V241*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,11,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C242,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C242,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C242,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H242),FORECAST(C242,$H$138:$H$243,$C$138:$C$243),H242),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O242),FORECAST(C242,$O$138:$O$243,$C$138:$C$243),O242),\nIF(C242>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C242),0),0))))","v":0},{"$f":"IF(E242>0,V242*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]
[null,null,10,{"$f":"IFERROR(AVERAGEIF(tbl_Climate_Zone[Dry_Bulb],tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Climate_Zone[Wet_Bulb]),0)","v":0},{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C243,tbl_Climate_Zone[Weekday],$C$12,tbl_Climate_Zone[Hour],\">\"&$D$12,tbl_Climate_Zone[Hour],\"<=\"&$E$12),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C243,tbl_Climate_Zone[Weekday],$C$13,tbl_Climate_Zone[Hour],\">\"&$D$13,tbl_Climate_Zone[Hour],\"<=\"&$E$13),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C243,tbl_Climate_Zone[Weekday],$C$14,tbl_Climate_Zone[Hour],\">\"&$D$14,tbl_Climate_Zone[Hour],\"<=\"&$E$14))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),IF($N$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)]]),MEDIAN($N$117,$O$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[ CHWST (°F)2],tbl_Chiller_Calc_Engine736[OAT])),tbl_Chiller_Calc_Engine736[[#This Row],[ CHWST (°F)2]]),\nMEDIAN($N$117,$O$117,TREND($N$117:$O$117,$N$118:$O$118,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$115=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),IF($I$115=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)]]),MEDIAN($I$117,$J$117,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]],tbl_Chiller_Calc_Engine736[CWST (°F)3],tbl_Chiller_Calc_Engine736[Average WBT])),tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)3]]),\nMEDIAN($I$117,$J$117,TREND($I$117:$J$117,$I$118:$J$118,tbl_Chiller_Calc_Engine736[[#This Row],[Average WBT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$121=\"Baseline Trend Data\",IF(ISBLANK(H243),FORECAST(C243,$H$138:$H$243,$C$138:$C$243),H243),\nIF($N$121 = \"Proposed Trend Data\",IF(ISBLANK(O243),FORECAST(C243,$O$138:$O$243,$C$138:$C$243),O243),\nIF(C243>=$N$131,MAX(TREND($N$122:$O$122,$N$123:$O$123,C243),0),0))))","v":0},{"$f":"IF(E243>0,V243*'Chilled Water System Template'!$C$131,0)","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($N$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($N$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed3]]),MEDIAN($N$127,$O$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[SCHWP Speed3],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($N$127,$O$127,TREND($N$127:$O$127,$N$128:$O$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],['# CWP2]]),MEDIAN($F$41,$G$41,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736['# CWP2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($F$41,$G$41,TREND($F$41:$G$41,$F$42:$G$42,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])),0))))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$125=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$125=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed2]]),MEDIAN($I$127,$J$127,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[CWP Speed2],tbl_Chiller_Calc_Engine736[OAT]))),\nMEDIAN($I$127,$J$127,TREND($I$127:$J$127,$I$128:$J$128,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]])))))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0,0,IF($I$120=\"Baseline Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft],tbl_Chiller_Calc_Engine736[OAT]))),\nIF($I$120=\"Proposed Trend Data\",IF(ISBLANK(tbl_Chiller_Calc_Engine736[[#This Row],[Head in ft2]]),MEDIAN($I$122,$J$122,FORECAST(tbl_Chiller_Calc_Engine736[[#This Row],[OAT]],tbl_Chiller_Calc_Engine736[Head in ft2],tbl_Chiller_Calc_Engine736[OAT]))),\nROUNDUP(MEDIAN($I$122,$J$122,TREND($I$122:$J$122,$I$123:$J$123,tbl_Chiller_Calc_Engine736[[#This Row],[OAT]]))*2.31,0))))","v":0},false,{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]=0,tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]]),0,MEDIAN(0,MAX($W$124:$W$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]],$X$124:$X$130,1),0)+1))","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]=0,0,IFERROR(MEDIAN(0,MAX($Q$124:$Q$130),IFERROR(MATCH(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]],$R$124:$R$130,1),0)+1),0))","v":0},{"$f":"IF(OR(tbl_Chiller_Calc_Engine736[[#This Row],[Econ Engaged]],tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]=0),0,SUMPRODUCT(tbl_Chiller_Calc_Engine736[[#This Row],[Cooling Load (tons)2]]*INDEX($Z$124:$AB$130,tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]],0)*$Z$118:$AB$118*(1-((tbl_Chiller_Calc_Engine736[[#This Row],[CHWST (°F)]]-$Z$119:$AB$119)+($Z$120:$AB$120-tbl_Chiller_Calc_Engine736[[#This Row],[CWST (°F)2]]))*$C$127)))","v":0},0,{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CH Stage]]=0,0,SUMPRODUCT(INDEX($T$124:$V$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$D$133:$F$133))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Qty]]*$C$129*$H$24*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Speed2]]*tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP Head]])/\n(3960*$H$26*$H$27*IF($N$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kW]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kW]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kW]])","v":0},{"$f":"SUM(tbl_Chiller_Calc_Engine736[[#This Row],[Chiller Load kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[PCHWP kWh]],tbl_Chiller_Calc_Engine736[[#This Row],[SCHWP kWh]])","v":0},{"$f":"IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]]=0,0,SUMPRODUCT((IF(tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0)>=$T$120:$V$120,tbl_Chiller_Calc_Engine736[[#This Row],[CT Load (Tons)]]/INDEX($R$124:$R$130,tbl_Chiller_Calc_Engine736[[#This Row],[CT Stage]],0),$T$120:$V$120)^$C$130*$T$118:$V$118*$C$129)/($C$128*$T$119:$V$119)))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CT Fan kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0},{"$f":"(tbl_Chiller_Calc_Engine736[[#This Row],[CWP Qty]]*$C$129*$D$40*tbl_Chiller_Calc_Engine736[[#This Row],[CWP Speed3]]*$D$41)/\n(3960*$D$42*$D$43*IF($I$129=$F$129,1,$C$128))","v":0},{"$f":"tbl_Chiller_Calc_Engine736[[#This Row],[CWP kW]]*tbl_Chiller_Calc_Engine736[[#This Row],[Hours]]","v":0}]

{"sheet":"Hot Water System Template","index":2,"n_rows":193,"n_cols":23,"rows_kept":193,"cut":false,"hidden":true,"merged":[[85,7,85,9],[3,8,3,9],[5,8,5,9],[48,7,48,8],[52,4,52,6],[38,7,38,8],[44,7,44,8],[23,7,23,8],[24,7,24,8],[53,4,53,6],[46,4,46,6],[47,4,47,6],[48,4,48,6],[40,4,40,6],[41,4,41,6],[44,4,44,6],[8,2,8,3],[9,2,9,3],[7,2,7,3],[23,2,23,3],[85,4,85,6],[38,4,38,6],[48,2,48,3],[44,2,44,3],[21,4,21,5],[24,2,24,3],[24,4,24,6],[38,2,38,3]]}
[null,"Hot Water Side System Calculations"]
[null,"Boilers & Pumps Specifications",null,null,null,null,null,null,null,null,null,"Savings",null,null,"PHWP kW","PHWP kWh","SHWP kW","SHWP kWh","Therms","Total kW","Total kWh","Cost","Incentives"]
[null,null,"Boilers",null,"B1","B2","B3",null,null,"Main Location Of Boilers",null,null,null,"HW Lockout Control",{"$f":"IF(ISBLANK(O12),0,O11-O12)","v":0},0,0,0,0,0,0,{"$f":"I23","v":0},0]
[null,null,null,"Equipment Vintage",2009,2009,2009,null,"Indoor",null,null,null,null,"Boiler Staging Sequence",0,0,0,0,0,0,0,{"$f":"I27","v":0},0]
[null,null,null,"Capacity (kBtu/h)",6400,6400,6400,null,null,"Air Temperature If Indoor",null,null,null,"HW Temp Reset",0,0,0,0,0,0,0,{"$f":"I38","v":0},0]
[null,null,null,"Efficiency (%)",0.8,0.85,0.95,null,60,null,null,null,null,"SHWP VFD And Speed Control",0,0,0,0,0,0,0,{"$f":"I44","v":0},0]
[null,null,null,null,null,null,null,null,"Start Time","Stop Time",null,null,null,"HW Differential Pressure Reset",0,0,0,0,0,0,0,{"$f":"I51","v":0},0]
[null,null,"Building Heating Load ",null,"Min Temp","Max Temp",null,"Weekday",0,24,null,null,null,"Total",{"$f":"SUM(O3:O7)","v":0},{"$f":"SUM(P3:P7)","v":0},0,0,0,0,0,{"$f":"SUM(V3:V7)","v":0},{"$f":"SUM(W3:W7)","v":0}]
[null,null,"Simple Data",null,12000,200,"kBtu/h","Saturday",0,24]
[null,null,null,null,30,65,{"$f":"\"@OAT\"","v":"@OAT"},"Sunday",0,24,null,"Consumption",null,null,"PHWP kW","PHWP kWh","SHWP kW","SHWP kWh","Therms","Total kW","Total kWh"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Baseline",2.4529145622895623,13503.294665404042,11.192544724075194,65956.69046360167,176220.14968253969,{"$f":"SUM(O11,Q11)","v":13.645459286364757},{"$f":"SUM(P11,R11)","v":79459.985129005712}]
[null,null,"Primary Pumps",null,"PHWP1","PHWP2","PHWP3",null,null,null,null,null,null,"HW Lockout Control",2.4529145622895623,13503.294665404042,11.192544724075194,65956.69046360167,176220.14968253969,{"$f":"SUM(O12,Q12)","v":13.645459286364757},{"$f":"SUM(P12,R12)","v":79459.985129005712}]
[null,null,null,"Flow (gpm)",325,325,325,null,null,null,null,null,null,"Boiler Staging Sequence",2.4529145622895623,13503.294665404042,11.192544724075194,65956.69046360167,176220.14968253969,13.645459286364757,79459.985129005712]
[null,null,null,"Head (ft)",25,25,25,null,null,null,null,null,null,"HW Temp Reset",2.4529145622895623,13503.294665404042,11.192544724075194,65956.69046360167,176220.14968253969,13.645459286364757,79459.985129005712]
[null,null,null,"Motor Efficiency (%)",0.78,0.78,0.78,null,null,null,null,null,null,"SHWP VFD And Speed Control",2.4529145622895623,13503.294665404042,11.192544724075194,65956.69046360167,176220.14968253969,13.645459286364757,79459.985129005712]
[null,null,null,"Pump Efficiency (%)",0.8,0.8,0.8,null,null,null,null,null,null,"HW Differential Pressure Reset",2.4529145622895623,13503.294665404042,11.192544724075194,65956.69046360167,176220.14968253969,13.645459286364757,79459.985129005712]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Proposed",{"$f":"INDEX(tbl_HW_Calc_Engine[[PWHP kW ]],MATCH($L$69,tbl_HW_Calc_Engine[OAT],0))","v":2.4529145622895623},{"$f":"SUM(tbl_HW_Calc_Engine[PHWP kWh])","v":23209.477588383841},{"$f":"INDEX(tbl_HW_Calc_Engine[[SHWP kW ]],MATCH($L$69,tbl_HW_Calc_Engine[OAT],0))","v":11.192544724075194},{"$f":"SUM(tbl_HW_Calc_Engine[SHWP kWh])","v":117558.89943526378},{"$f":"SUM(tbl_HW_Calc_Engine[Total Therms])","v":341631.11550700269},13.645459286364757,140768.37702364763]
[null,null,"Secondary Pumps",null,"SHWP",null,"Secondary Pump staging"]
[null,null,null,"Flow (gpm)",325,null,"Max","Min"]
[null,null,null,"Motor Efficiency (%)",0.85,null,2,1,"# Pumps operating"]
[null,null,null,"Pump Efficiency (%)",0.8,null,45,75,{"$f":"\"@OAT\"","v":"@OAT"}]
[]
[null,"Hot Water Plant Lockout Control",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,75,null,"Heating Lookout",null,null,70,null,{"$f":"IF(OR(C25<>H25,D25<>I25),\"*\",\"\")","v":"*"}]
[]
[null,"Boiler Staging Sequence",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,null,"Baseline Staging ",null,null,null,"Proposed Staging "]
[null,null,"B1","B2",null,"Stage","B1","B2","B3"]
[null,null,"On",null,null,1,null,null,"On",{"$f":"IF(OR(B30<>G30,C30<>H30,D30<>I30),\"*\",\"\")","v":"*"}]
[null,null,"On","On",null,2,null,"On","On",""]
[null,null,null,null,null,3,null,null,null,""]
[null,null,null,null,null,4,null,null,null,""]
[null,null,null,null,null,5,null,null,null,""]
[null,null,null,null,null,6,null,null,null,""]
[null,null,null,null,null,7,null,null,null,""]
[]
[null,"Hot Water Temperature Reset",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,180,180,"HW Temp",null,null,140,180,{"$f":"IF(OR(C41<>H41,D41<>I41),\"*\",\"\")","v":"*"}]
[null,null,45,65,"@ OAT",null,null,45,65,{"$f":"IF(OR(C42<>H42,D42<>I42),\"*\",\"\")","v":""}]
[]
[null,"Secondary Hot Water Pump VFD And Speed Control",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,1,0.9,"Pump Speed (%)",null,null,1,0.4,{"$f":"IF(OR(C47<>H47,D47<>I47),\"*\",\"\")","v":"*"}]
[null,null,45,65,"@ OAT",null,null,45,65,{"$f":"IF(OR(C48<>H48,D48<>I48),\"*\",\"\")","v":""}]
[null,null,"VFD",null,"Pump Control",null,null,"VFD",null,{"$f":"IF(OR(C49<>H49,D49<>I49),\"*\",\"\")","v":""}]
[]
[null,"Hot Water Differential Pressure Reset (Secondary)",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,35,20,"Psi",null,null,35,15,{"$f":"IF(OR(C53<>H53,D53<>I53),\"*\",\"\")","v":"*"}]
[null,null,65,75,"@ OAT",null,null,65,75,{"$f":"IF(OR(C54<>H54,D54<>I54),\"*\",\"\")","v":""}]
[]
[null,"Processing"]
[null,null,"Switch"]
[null,1,"Proposed","HW Lockout Control",null,null,null,null,"Assumption"]
[null,2,"Proposed","Boiler Staging Sequence",null,null,null,null,0.01,"Jacket Losses",null,"Boiler Location Types",null,"Pump Control Type"]
[null,3,"Proposed","Hot Water Temperature Reset",null,null,null,null,0.01,"kBtu to therms",null,"Indoor",null,"Constant"]
[null,4,"Proposed","Secondary Hot Water Pump VFD And Speed Control",null,null,null,null,90,"Standard Boiler Room Temperature",null,"Outdoor",null,"VFD"]
[null,5,"Proposed","Hot Water Differential Pressure Reset (Secondary)",null,null,null,null,0.97,"VFD Efficiency"]
[null,null,null,null,null,null,null,null,0.746,"HP to kW"]
[null,null,"Calculation",null,null,null,null,null,180,"Design HWST"]
[null,null,null,"PHWP1","PHWP2","PHWP3"]
[null,null,"kW",{"$f":"($I$63*E$13*E$14/(3960*E$16*E$15))","v":2.4529145622895623},{"$f":"($I$63*F$13*F$14/(3960*F$16*F$15))","v":2.4529145622895623},{"$f":"($I$63*G$13*G$14/(3960*G$16*G$15))","v":2.4529145622895623}]
[]
[null,null,{"$f":"$D$59","v":"Boiler Staging Sequence"},null,null,null,null,null,null,{"$f":"$D$58","v":"HW Lockout Control"},null,"Peak Demand Temp"]
[null,null,"Baseline","Proposed",null,null,null,null,null,{"$f":"IF(OR($C$58=\"Baseline\",$J$23=\"Disable\",ISBLANK(H25)),$C$25,$H$25)","v":75},null,{"$f":"'CTZ2'!$U$3","v":69}]
[null,null,{"$f":"TRIM(CONCATENATE(IF($C30=\"On\",$C$29&\" \",\"\")&IF($D30=\"On\",$D$29&\" \",\"\")&IF($E30=\"On\",$E$29&\" \",\"\")))","v":"B1"},{"$f":"TRIM(IF($G30=\"On\",$G$29&\" \",\"\")&IF($H30=\"On\",$H$29&\" \",\"\")&IF($I30=\"On\",$I$29&\"  \",\"\"))","v":"B3"},null,"B1","B2","B3"]
[null,null,{"$f":"TRIM(CONCATENATE(IF($C31=\"On\",$C$29&\" \",\"\")&IF($D31=\"On\",$D$29&\" \",\"\")&IF($E31=\"On\",$E$29&\" \",\"\")))","v":"B1 B2"},"B2 B3","Capacity",{"$f":"E5","v":6400},6400,6400,null,{"$f":"$D$60","v":"Hot Water Temperature Reset"}]
[null,null,"","","Efficiency",0.8,0.85,0.95,null,{"$f":"IF(OR($C$60=\"Baseline\",$J$38=\"Disable\",ISBLANK($H$39)),$C$39,$H$39)","v":"Simple Data"}]
[null,null,"","","Location",{"$f":"I$4","v":"Indoor"},"Temp",{"$f":"$I$6","v":60},null,{"$f":"IF(OR($C$60=\"Baseline\",$J$38=\"Disable\",ISBLANK(H41)),C41,H41)","v":180},{"$f":"IF(OR($C$60=\"Baseline\",$J$38=\"Disable\",ISBLANK(I41)),D41,I41)","v":180},"HW Temp"]
[null,null,"","",null,null,null,null,null,{"$f":"IF(OR($C$60=\"Baseline\",$J$38=\"Disable\",ISBLANK(H42)),C42,H42)","v":45},{"$f":"IF(OR($C$60=\"Baseline\",$J$38=\"Disable\",ISBLANK(I42)),D42,I42)","v":65},"@ OAT"]
[null,null,"",""]
[null,null,"","",null,null,null,null,null,{"$f":"$D$61","v":"Secondary Hot Water Pump VFD And Speed Control"}]
[null,null,"Stage","Capacity","Boilers","B1 % Load","B2 % Load","B3 % Load",null,{"$f":"IF(OR($C$61=\"Baseline\",$J$44=\"Disable\",ISBLANK($H$45)),$C$45,$H$45)","v":"Simple Data"}]
[null,null,{"$f":"IF(E78=\"\",\"\",$F30)","v":1},{"$f":"IF(E78=\"\",\"\",SUMPRODUCT(--(ISNUMBER(FIND($F$70:$H$70,E78))),$F$71:$H$71))","v":6400},{"$f":"IF(OR($C$59=\"Baseline\",$J$27=\"Disable\"),$C70,$D70)","v":"B1"},{"$f":"IF(ISNUMBER(SEARCH(LEFT(F$70,2),$E78)),F$71/$D78,0)","v":1},{"$f":"IF(ISNUMBER(SEARCH(LEFT(G$70,2),$E78)),G$71/$D78,0)","v":0},0,null,{"$f":"IF(OR($C$61=\"Baseline\",$J$44=\"Disable\",ISBLANK(H47)),C47,H47)","v":1},{"$f":"IF(OR($C$61=\"Baseline\",$J$44=\"Disable\",ISBLANK(I47)),D47,I47)","v":0.9},"Pump Speed (%)"]
[null,null,2,{"$f":"IF(E79=\"\",\"\",SUMPRODUCT(--(ISNUMBER(FIND($F$70:$H$70,E79))),$F$71:$H$71))","v":12800},"B1 B2",{"$f":"IF(ISNUMBER(SEARCH(LEFT(F$70,2),$E79)),F$71/$D79,0)","v":0.5},0.5,0,null,{"$f":"IF(OR($C$61=\"Baseline\",$J$44=\"Disable\",ISBLANK(H48)),C48,H48)","v":45},{"$f":"IF(OR($C$61=\"Baseline\",$J$44=\"Disable\",ISBLANK(I48)),D48,I48)","v":65},"@ OAT"]
[null,null,"","","",{"$f":"IF(ISNUMBER(SEARCH(LEFT(F$70,2),$E80)),F$71/$D80,0)","v":0},0,0,null,{"$f":"IF(OR($C$61=\"Baseline\",$J$44=\"Disable\",ISBLANK(H49)),C49,H49)","v":"VFD"},"Pump Control"]
[null,null,"","","",0,0,0]
[null,null,"","","",0,0,0,null,{"$f":"$D$62","v":"Hot Water Differential Pressure Reset (Secondary)"}]
[null,null,"","","",0,0,0,null,{"$f":"IF(OR($C$62=\"Baseline\",$J$51=\"Disable\",ISBLANK(H53)),C53,H53)","v":35},{"$f":"IF(OR($C$62=\"Baseline\",$J$51=\"Disable\",ISBLANK(I53)),D53,I53)","v":20},"Psi"]
[null,null,"","","",0,0,0,null,{"$f":"IF(OR($C$62=\"Baseline\",$J$51=\"Disable\",ISBLANK(H54)),C54,H54)","v":65},{"$f":"IF(OR($C$62=\"Baseline\",$J$51=\"Disable\",ISBLANK(I54)),D54,I54)","v":75},"@ OAT"]
[]
[null,"Calculation Engine",null,null,"Optional",null,null,"Optional"]
[null,null,"OAT","Hours","Baseline Trend Heating Load (kBtu/h)","Baseline Trend HWST (F)","Baseline Trend SHWP Speed (%)","Proposed Trend Heating Load (kBtu/h)","Proposed Trend HWST (F)","Proposed Trend SHWP Speed (%)","Heating Load (kBtu/h)","HWST (F)","Stage","Therms","Therms Lost","SHWP Qty","Head (ft H2O)","SHWP Speed %","PWHP kW ","PHWP kWh","SHWP kW ","SHWP kWh","Total Therms"]
[null,null,115,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C88,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C88,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C88,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C88,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S88*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},{"$f":"U88*D88","v":0},{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,114,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C89,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C89,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C89,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C89,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S89*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,113,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C90,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C90,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C90,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C90,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S90*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,112,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C91,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C91,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C91,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C91,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S91*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,111,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C92,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C92,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C92,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C92,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S92*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,110,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C93,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C93,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C93,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C93,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S93*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,109,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C94,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C94,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C94,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C94,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S94*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,108,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C95,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C95,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C95,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C95,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S95*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,107,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C96,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C96,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C96,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C96,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S96*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,106,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C97,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C97,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C97,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C97,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S97*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,105,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C98,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C98,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C98,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C98,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S98*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,104,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C99,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C99,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C99,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C99,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S99*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,103,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C100,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C100,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C100,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C100,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S100*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,102,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C101,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C101,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C101,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C101,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S101*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,101,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C102,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C102,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C102,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C102,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S102*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,100,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C103,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C103,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C103,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C103,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S103*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,99,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C104,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C104,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C104,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C104,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S104*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,98,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C105,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C105,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C105,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C105,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S105*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,97,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C106,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C106,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C106,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C106,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S106*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,96,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C107,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C107,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C107,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C107,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S107*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,95,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C108,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C108,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C108,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C108,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S108*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,94,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C109,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C109,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C109,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C109,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S109*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,93,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C110,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C110,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C110,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C110,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S110*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,92,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C111,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C111,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C111,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C111,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S111*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,91,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C112,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C112,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C112,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":1},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C112,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0.91022222222222227},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S112*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":2.4529145622895623},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0.91022222222222227}]
[null,null,90,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C113,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C113,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C113,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C113,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S113*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,89,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C114,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C114,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C114,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":5},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C114,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":4.5511111111111111},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S114*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":12.264572811447811},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":4.5511111111111111}]
[null,null,88,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C115,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C115,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C115,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":3},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C115,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":2.730666666666667},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S115*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":7.3587436868686869},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":2.730666666666667}]
[null,null,87,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C116,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C116,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C116,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":5},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C116,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":4.5511111111111111},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S116*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":12.264572811447811},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":4.5511111111111111}]
[null,null,86,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C117,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C117,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C117,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":10},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C117,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":9.1022222222222222},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S117*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":24.529145622895623},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":9.1022222222222222}]
[null,null,85,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C118,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C118,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C118,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":6},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C118,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":5.461333333333334},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S118*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":14.717487373737374},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":5.461333333333334}]
[null,null,84,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C119,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C119,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C119,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":8},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C119,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":7.2817777777777781},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S119*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":19.623316498316498},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":7.2817777777777781}]
[null,null,83,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C120,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C120,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C120,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":15},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C120,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":13.653333333333334},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S120*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":36.793718434343432},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},{"$f":"U120*D120","v":0},{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":13.653333333333334}]
[null,null,82,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C121,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C121,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C121,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":15},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C121,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":13.653333333333334},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S121*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":36.793718434343432},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":13.653333333333334}]
[null,null,81,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C122,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C122,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C122,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":10},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C122,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":9.1022222222222222},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S122*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":24.529145622895623},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":9.1022222222222222}]
[null,null,80,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C123,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C123,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C123,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":28},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C123,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":25.486222222222224},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S123*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":68.681607744107737},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":25.486222222222224}]
[null,null,79,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C124,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C124,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C124,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":27},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C124,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":24.576000000000001},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S124*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":66.228693181818187},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":24.576000000000001}]
[null,null,78,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C125,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C125,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C125,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":33},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C125,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":30.037333333333336},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S125*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":80.946180555555557},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":30.037333333333336}]
[null,null,77,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C126,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C126,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C126,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":20},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C126,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":18.204444444444444},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S126*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":49.058291245791246},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":18.204444444444444}]
[null,null,76,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C127,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C127,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C127,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":50},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C127,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":0},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":45.511111111111113},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":0},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S127*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":122.64572811447812},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":0},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":45.511111111111113}]
[null,null,75,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C128,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C128,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C128,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":47},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C128,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":117.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":42.780444444444448},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":1},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":46.2},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S128*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":115.28698442760943},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":3.8594981807155841},181.39641449363245,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":160.28044444444444}]
[null,null,74,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C129,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C129,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C129,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":61},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C129,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":152.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":55.523555555555561},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":49.664999999999999},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S129*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":149.62778829966331},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":8.2979210885385051},506.17318640084881,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":208.02355555555556}]
[null,null,73,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C130,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C130,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C130,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":68},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C130,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":170},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":61.895111111111113},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":53.13},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S130*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":166.79819023569024},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":8.8768458156458436},603.6255154639174,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":231.89511111111111}]
[null,null,72,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C131,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C131,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C131,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":80},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C131,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":200},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":72.817777777777778},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":56.594999999999999},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S131*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":196.23316498316498},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":9.4557705427531804},756.4616434202544,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":272.81777777777779}]
[null,null,71,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C132,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C132,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C132,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":137},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C132,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":342.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":124.70044444444446},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":60.06},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S132*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":336.04929503367003},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":10.034695269860519},1374.7532519708911,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":467.20044444444443}]
[null,null,70,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C133,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C133,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C133,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":111},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C133,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":277.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":101.03466666666667},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":63.524999999999999},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S133*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":272.2735164141414},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":10.613619996967856},1178.111819663432,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":378.53466666666668}]
[null,null,69,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C134,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C134,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C134,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":135},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C134,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":337.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":122.88000000000001},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":66.989999999999995},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S134*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":331.14346590909093},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":11.192544724075194},1510.9935377501513,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":460.38}]
[null,null,68,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C135,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C135,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C135,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":138},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C135,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":345},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":125.61066666666667},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":70.454999999999998},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S135*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":338.50220959595958},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":11.771469451182531},1624.4627842631892,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":470.6106666666667}]
[null,null,67,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C136,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C136,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C136,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":180},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C136,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":450},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":163.84},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":73.92},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S136*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":441.52462121212119},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":12.35039417828987},2223.0709520921764,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":613.84}]
[null,null,66,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C137,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C137,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C137,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":165},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C137,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":412.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":150.18666666666667},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":77.385000000000005},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S137*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":404.73090277777777},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":12.929318905397208},2133.3376193905392,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":562.68666666666672}]
[null,null,65,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":219},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C138,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":200},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":547.5},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":199.33866666666668},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.89999999999999991},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S138*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":537.18828914141409},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.508243632504545},2958.3053555184952,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":746.83866666666665}]
[null,null,64,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":245},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C139,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":537.14285714285506},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":1644.9999999999936},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":223.00444444444446},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.90500000000000003},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S139*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":600.96406776094273},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.583289430462907},3327.9059104634121,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":1868.0044444444381}]
[null,null,63,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":200},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C140,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":874.28571428571377},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":2185.7142857142844},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":182.04444444444445},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.90999999999999992},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S140*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":490.58291245791247},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.658335228421265},2731.667045684253,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":2367.7587301587287}]
[null,null,62,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":312},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C141,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":1211.4285714285688},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":4724.5714285714184},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":283.98933333333332},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.91500000000000004},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S141*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":765.30934343434342},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.733381026379623},4284.8148802304422,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":5008.5607619047514}]
[null,null,61,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":343},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C142,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":1548.5714285714275},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":6639.4999999999955},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":312.20622222222221},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.91999999999999993},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S142*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":841.34969486531986},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.808426824337982},4736.2904007479274,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":6951.7062222222175}]
[null,null,60,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":467},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C143,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":1885.7142857142826},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":11007.857142857125},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":425.07377777777782},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.92500000000000004},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S143*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1145.5111005892256},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.883472622296344},6483.5817146123927,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":11432.930920634903}]
[null,null,59,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":455},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C144,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":2222.8571428571413},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":12642.499999999991},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":414.15111111111111},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.92999999999999994},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S144*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1116.0761258417508},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":13.958518420254698},6351.1258812158876,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":13056.651111111101}]
[null,null,58,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":545},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C145,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":2560},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":17440},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":496.07111111111112},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.93499999999999994},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S145*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1336.8384364478115},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.033564218213057},7648.2924989261155,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":17936.071111111112}]
[null,null,57,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":464},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C146,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":2897.1428571428551},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":16803.428571428558},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":422.34311111111111},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.94},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S146*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1138.1523569023568},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.108610016171417},6546.3950475035372,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":17225.771682539667}]
[null,null,56,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":518},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C147,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":3234.2857142857138},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":20941.999999999996},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":471.49511111111116},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.94499999999999995},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S147*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1270.6097432659933},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.183655814129775},7347.1337117192234,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":21413.495111111108}]
[null,null,55,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":461},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C148,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":3571.4285714285688},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":20580.357142857127},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":419.61244444444446},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.95},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S148*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1130.7936132154882},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.258701612088135},6573.2614431726306,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":20999.96958730157}]
[null,null,54,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":428},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C149,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":3908.5714285714275},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":20910.857142857138},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":389.57511111111114},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.95499999999999996},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S149*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1049.8474326599326},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.333747410046492},6134.8438914998987,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":21300.432253968247}]
[null,null,53,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":419},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C150,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":4245.7142857142862},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":22236.928571428572},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":381.38311111111113},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.96},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S150*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":1027.7712015993266},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.408793208004852},6037.2843541540333,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":22618.311682539683}]
[null,null,52,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":358},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C151,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":4582.8571428571413},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":20508.285714285706},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":325.85955555555557},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.96499999999999997},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S151*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":878.14341329966328},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.483839005963212},5185.2143641348302,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":20834.145269841261}]
[null,null,51,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":356},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C152,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":4920},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":21894},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":324.03911111111114},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.97},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S152*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":873.23758417508418},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.55888480392157},{"$f":"U152*D152","v":5182.9629901960789},{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":22218.039111111109}]
[null,null,50,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":245},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C153,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":5257.1428571428551},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":16099.999999999993},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":223.00444444444446},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.97499999999999998},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S153*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":600.96406776094273},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.633930601879928},3585.3129974605827,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":16323.004444444437}]
[null,null,49,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":266},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C154,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":5594.2857142857138},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":18600.999999999996},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":242.11911111111112},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.98},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S154*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":652.47527356902356},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.708976399838287},3912.5877223569842,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":18843.119111111107}]
[null,null,48,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":199},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C155,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":5931.4285714285706},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":14754.428571428571},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":181.13422222222223},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.98499999999999988},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S155*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":488.12999789562292},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.784022197796642},2942.0204173615316,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":14935.562793650794}]
[null,null,47,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":200},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C156,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":6268.5714285714275},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":1},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":15671.428571428569},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":182.04444444444445},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.99},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":2.4529145622895623},{"$f":"S156*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":490.58291245791247},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.859067995755003},2971.8135991510007,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":15853.473015873013}]
[null,null,46,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":143},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C157,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":6605.7142857142844},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":11460.428571428569},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":134.22933333333336},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":0.99499999999999988},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S157*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":701.53356481481478},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":14.934113793713358},2135.5782725010104,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":11594.657904761902}]
[null,null,45,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":117},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C158,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":6942.8571428571431},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":9855.2836134453792},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":109.82400000000001},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S158*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":573.98200757575762},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},1756.0716722255913,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":9965.1076134453797}]
[null,null,44,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":109},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C159,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":7280},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":9627.264705882355},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":102.31466666666668},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S159*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":534.7353745791246},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},1635.9983954922175,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":9729.5793725490221}]
[null,null,43,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":81},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C160,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":7617.1428571428569},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":7485.5231092436961},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":76.032000000000011},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S160*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":397.37215909090907},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},1215.7419269254094,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":7561.5551092436963}]
[null,null,42,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":71},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C161,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":7954.2857142857138},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":6851.7983193277314},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":66.64533333333334},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S161*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":348.31386784511784},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},1065.6503310086921,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":6918.4436526610643}]
[null,null,41,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":39},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C162,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":8291.4285714285706},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":3923.1869747899159},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":36.608000000000004},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S162*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":191.32733585858585},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},585.35722407519711,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":3959.7949747899161}]
[null,null,40,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":53},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C163,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":8628.5714285714275},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":5548.2983193277305},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":49.74933333333334},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S163*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":260.00894360269359},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},795.48545835860114,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":5598.0476526610637}]
[null,null,39,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":30},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C164,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":8965.7142857142862},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":3263.2563025210088},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":28.160000000000004},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S164*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":147.17487373737373},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},450.27478775015157,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":3291.4163025210087}]
[null,null,38,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":21},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C165,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":9302.8571428571431},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":2370.1764705882351},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":19.712000000000003},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S165*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":103.02241161616162},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},315.1923514251061,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":2389.8884705882351}]
[null,null,37,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":13},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C166,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":9640},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":1520.4264705882356},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":12.202666666666667},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S166*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":63.775778619528623},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},195.11907469173235,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":1532.6291372549022}]
[null,null,36,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":12},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C167,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":9977.1428571428569},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":1452.5546218487393},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":11.264000000000001},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S167*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":58.869949494949495},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},180.10991510006065,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":1463.8186218487392}]
[null,null,35,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":10},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C168,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":10314.285714285714},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":1251.3655462184875},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":9.3866666666666667},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S168*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":49.058291245791246},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},150.09159591671721,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":1260.7522128851542}]
[null,null,34,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":3},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C169,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":10651.428571428572},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":387.68067226890759},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":2.8160000000000003},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S169*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":14.717487373737374},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},45.027478775015162,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":390.49667226890756}]
[null,null,33,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C170,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":10988.571428571429},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S170*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,32,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C171,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":11325.714285714286},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S171*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,31,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C172,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":11662.857142857143},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S172*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,30,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C173,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S173*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,29,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C174,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S174*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,28,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C175,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S175*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,27,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C176,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S176*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,26,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C177,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S177*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,25,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C178,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S178*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,24,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C179,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S179*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,23,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C180,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S180*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,22,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C181,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S181*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,21,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C182,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S182*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,20,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C183,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S183*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,19,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C184,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S184*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},{"$f":"U184*D184","v":0},{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,18,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C185,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S185*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,17,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C186,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S186*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,16,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C187,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S187*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,15,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C188,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S188*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,14,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C189,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S189*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,13,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C190,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S190*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,12,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C191,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S191*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,11,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C192,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S192*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]
[null,null,10,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$H$8,tbl_Climate_Zone[Hour],\">\"&$I$8,tbl_Climate_Zone[Hour],\"<=\"&$J$8),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$H$9,tbl_Climate_Zone[Hour],\">\"&$I$9,tbl_Climate_Zone[Hour],\"<=\"&$J$9),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$H$10,tbl_Climate_Zone[Hour],\">\"&$I$10,tbl_Climate_Zone[Hour],\"<=\"&$J$10))","v":0},null,null,null,null,null,null,{"$f":"MAX(0,IF($C$9=\"Simple Data\",IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]<=$J$69,MIN(MAX(TREND($E$9:$F$9,$E$10:$F$10,C193,TRUE),$F$9),$E$9),0),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Baseline Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend Heating Load (kBtu/h)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[Proposed Trend Heating Load (kBtu/h)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend Heating Load (kBtu/h)]]))))","v":12000},{"$f":"IF($J$72=\"Simple Data\",TREND($J$73:$K$73,$J$74:$K$74,MEDIAN($J$74,$K$74,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($C$9=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Baseline Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend HWST (F)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[[#Data],[#Totals],[Proposed Trend HWST (F)]],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend HWST (F)]])))","v":180},{"$f":"MIN(MAX($C$78:$C$84),IFERROR(MATCH(tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]],$D$78:$D$84,1)+1,1))","v":2},{"$f":"IFERROR(SUMPRODUCT(MIN(SUM($F$71:$H$71),tbl_HW_Calc_Engine[[#This Row],[Heating Load (kBtu/h)]])*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),1/INDEX($F$72:$H$72,1,0))*tbl_HW_Calc_Engine[[#This Row],[Hours]]*$I$60,0)","v":0},{"$f":"IFERROR(SUMPRODUCT($F$71:$H$71*INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0),INDEX($F$72:$H$72,1,0))*$I$60*((tbl_HW_Calc_Engine[[#This Row],[HWST (F)]]-IF($F$73=\"Indoor\",$H$73,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2/($I$64-IF($F$73=\"Indoor\",$I$61,tbl_HW_Calc_Engine[[#This Row],[OAT]]))^2)*$I$59*tbl_HW_Calc_Engine[[#This Row],[Hours]],0)","v":0},{"$f":"ROUNDUP(IF(tbl_HW_Calc_Engine[[#This Row],[OAT]]>$J$69,0,MIN(TREND($G$20:$H$20,$G$21:$H$21,tbl_HW_Calc_Engine[[#This Row],[OAT]]),$G$20)),0)","v":2},{"$f":"TREND($J$83:$K$83,$J$84:$K$84,MEDIAN($J$84,$K$84,tbl_HW_Calc_Engine[[#This Row],[OAT]]))*2.31","v":80.850000000000009},{"$f":"IF($J$77=\"Simple Data\",TREND($J$78:$K$78,$J$79:$K$79,MEDIAN($J$79,$K$79,tbl_HW_Calc_Engine[[#This Row],[OAT]])),IF($J$77=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Baseline Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Baseline Trend SHWP Speed (%)]]),\nIF(ISBLANK(tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]]),FORECAST(tbl_HW_Calc_Engine[[#This Row],[OAT]],tbl_HW_Calc_Engine[Proposed Trend SHWP Speed (%)],tbl_HW_Calc_Engine[OAT]),tbl_HW_Calc_Engine[[#This Row],[Proposed Trend SHWP Speed (%)]])))","v":1},{"$f":"IFERROR(SUMPRODUCT(--(INDEX($F$78:$H$84,tbl_HW_Calc_Engine[[#This Row],[Stage]],0)>0),$D$66:$F$66),0)","v":4.9058291245791246},{"$f":"S193*tbl_HW_Calc_Engine[[#This Row],[Hours]]","v":0},{"$f":"'Hot Water System Template'!$I$63 *'Hot Water System Template'!$E$19*tbl_HW_Calc_Engine[[#This Row],[SHWP Speed %]]*tbl_HW_Calc_Engine[[#This Row],[Head (ft H2O)]]*tbl_HW_Calc_Engine[[#This Row],[SHWP Qty]]/(3960* 'Hot Water System Template'!$E$20*'Hot Water System Template'!$E$21* IF($J$80=\"Constant\",1,'Hot Water System Template'!$I$62))","v":15.00915959167172},0,{"$f":"tbl_HW_Calc_Engine[[#This Row],[Therms]]+tbl_HW_Calc_Engine[[#This Row],[Therms Lost]]","v":0}]

{"sheet":"Air Side System Template","index":3,"n_rows":209,"n_cols":52,"rows_kept":209,"cut":false,"hidden":true,"merged":[[2,2,2,3],[2,7,2,8],[3,2,3,3],[3,7,3,8],[8,2,8,3],[8,7,8,8],[13,7,13,8],[14,2,14,3],[14,7,14,8],[13,2,13,3],[12,4,12,6],[13,4,13,6],[14,4,14,6],[15,7,15,8],[16,2,16,3],[16,7,16,8],[36,4,36,5],[36,19,36,20],[30,4,30,5],[24,4,24,6],[25,4,25,6],[31,4,31,6],[32,4,32,6],[29,2,29,3],[29,4,29,6],[29,7,29,8],[18,4,18,6],[18,2,18,3],[18,7,18,8],[17,2,17,3],[17,7,17,8],[21,2,21,3],[21,7,21,8],[15,2,15,3],[21,4,21,6],[22,4,22,6],[23,4,23,6],[3,29,3,30],[4,2,4,3],[4,7,4,8],[4,29,4,30],[5,2,5,3],[5,7,5,8],[5,29,5,30],[12,2,12,3],[12,7,12,8],[10,4,10,6],[11,4,11,6],[9,2,9,3],[9,7,9,8],[8,4,8,6],[9,4,9,6],[6,2,6,3],[6,7,6,8],[7,2,7,3],[7,7,7,8],[6,4,6,6],[7,4,7,6],[3,4,3,6],[4,4,4,6],[5,4,5,6],[73,21,73,24],[47,2,47,3],[47,7,47,8],[47,19,47,20],[46,2,46,3],[37,19,37,20],[41,2,41,3],[41,7,41,8],[41,19,41,20],[40,7,40,8],[40,4,40,6],[41,4,41,6],[42,4,42,6],[43,4,43,6],[46,7,46,8],[47,4,47,6],[52,19,52,20],[53,19,53,20],[54,19,54,20],[52,4,52,6],[53,4,53,6],[54,4,54,6],[49,19,49,20],[50,19,50,20],[65,19,65,20],[56,19,56,20],[57,19,57,20],[61,2,61,3],[61,7,61,8],[61,19,61,20],[60,2,60,3],[48,4,48,6],[37,4,37,6],[60,7,60,8],[61,4,61,6],[62,4,62,6],[63,4,63,6],[64,4,64,6],[65,4,65,6],[55,4,55,6],[56,4,56,6],[57,4,57,6],[63,19,63,20],[101,13,101,20],[101,5,101,12],[15,4,15,6],[16,4,16,6],[17,4,17,6],[75,17,75,18],[93,3,93,4],[35,2,35,3],[35,7,35,8],[40,2,40,3],[28,2,28,3],[28,7,28,8],[32,2,32,3],[32,7,32,8],[75,19,75,20],[76,17,76,18],[76,19,76,20],[42,19,42,20],[43,19,43,20],[51,19,51,20],[49,4,49,6],[50,4,50,6],[51,4,51,6],[62,19,62,20]]}
[null,"Air Side System Calculations"]
[null,"Equipment Specifications & Replacements",null,null,null,null,null,"Cost",null,"Disable",null,"Savings",null,null,"Fan kW","Fan kWh","Load kW","Load kWh","Therms","Total kW","Total kWh","Cost","Incentives"]
[null,null,"Baseline",null,null,null,null,"Proposed",null,null,null,null,null,"Equipment Replacements & Lockout",{"$f":"IF(ISBLANK(O14),0,O13-O14)","v":0},0,0,0,0,0,0,{"$f":"I2","v":0},0]
[null,null,"AHU-1",null,"Equipment Name",null,null,"AHU-1",null,{"$f":"IF(OR(C4<>H4,D4<>I4),\"*\",\"\")","v":""},null,null,null,"Scheduling Optimization",0,0,0,0,0,0,0,{"$f":"I21","v":0},0]
[null,null,2009,null,"Equipment Vintage",null,null,2009,null,{"$f":"IF(OR(C5<>H5,D5<>I5),\"*\",\"\")","v":""},null,null,null,"Economizer Optimization",0,0,0,0,0,0,0,{"$f":"I28","v":0},0]
[null,null," Efficiency",null,null,null,null," Efficiency",null,"",null,null,null,"Static Pressure Reset",0,0,0,0,0,0,0,{"$f":"I35","v":0},0]
[null,null,1.5,null,"Seasonal average kW/Ton",null,null,1.5,null,"",null,null,null,"Supply Air Temperature Reset",0,0,0,0,0,0,0,{"$f":"I40","v":0},0]
[null,null,"Gas",null,"Source of Heating",null,null,"Gas",null,"",null,null,null,"Temperature And Fan Setback",0,0,0,0,0,0,0,{"$f":"I46","v":0},0]
[null,null,0.8,null,"Gas Efficiency",null,null,0.8,null,"",null,null,null,"VAV Flow and Reheat Flow Adjustment",0,0,0,0,0,0,0,{"$f":"I60","v":0},0]
[null,null,7,null,"Heat Pump (HSPF)",null,null,7,null,"",null,null,null,"Total",{"$f":"SUM(O3:O9)","v":0},{"$f":"SUM(P3:P9)","v":0},0,0,0,0,0,{"$f":"SUM(V3:V9)","v":0},{"$f":"SUM(W3:W9)","v":0}]
[null,null,"Heating","Cooling",null,null,null,"Heating","Cooling"]
[null,null,75,55,"Lockout Temp",null,null,75,55,{"$f":"IF(OR(C12<>H12,D12<>I12),\"*\",\"\")","v":""},null,"Consumption",null,null,"Fan kW","Fan kWh","Load kW","Load kWh","Therms","Total kW","Total kWh"]
[null,null,40,null,"Supply Fan (HP)",null,null,40,null,"",null,null,null,"Baseline",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,{"$f":"SUM(O13,Q13)","v":138.74008723839705},{"$f":"SUM(P13,R13)","v":305904.74208039721}]
[null,null,60000,null,"Supply Fan (CFM)",null,null,60000,null,"",null,null,null,"Equipment Specifications & Replacements",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,{"$f":"SUM(O14,Q14)","v":138.74008723839705},305904.74208039721]
[null,null,"VFD",null,"Supply Fan Control",null,null,"VFD",null,"",null,null,null,"Scheduling Optimization",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,138.74008723839705,305904.74208039721]
[null,null,10,null,"Return Fan (HP)",null,null,10,null,"",null,null,null,"Economizer Optimization",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,138.74008723839705,305904.74208039721]
[null,null,60000,null,"Return Fan (CFM)",null,null,60000,null,"",null,null,null,"Static Pressure Reset",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,138.74008723839705,305904.74208039721]
[null,null,"VFD",null,"Return Fan Control",null,null,"VFD",null,"",null,null,null,"Supply Air Temperature Reset",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,138.74008723839705,305904.74208039721]
[null,null,0.9,null,"Return Fan % of Supply",null,null,0.9,null,null,null,null,null,"Temperature And Fan Setback",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,{"$f":"SUM(O19,Q19)","v":138.74008723839705},305904.74208039721]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"VAV Flow Adjustment",19.670087238397027,113396.16498039718,119.07000000000002,192508.57709999999,11480.225580000002,138.74008723839705,305904.74208039721]
[null,"Scheduling Optimization",null,null,null,null,null,"Cost",null,"Disable",null,null,null,"Proposed",{"$f":"INDEX(tbl_HVAC_Airside_Calc_Engine[Fan kW],MATCH($P$82,tbl_HVAC_Airside_Calc_Engine[OAT °F],0))","v":14.673885079844185},{"$f":"SUM(tbl_HVAC_Airside_Calc_Engine[Fan kWh])","v":84593.539075376306},{"$f":"INDEX(tbl_HVAC_Airside_Calc_Engine[Load kW],MATCH($P$82,tbl_HVAC_Airside_Calc_Engine[OAT °F],0))","v":119.07000000000002},{"$f":"SUM(tbl_HVAC_Airside_Calc_Engine[Load kWh])","v":192508.57709999999},{"$f":"SUM(tbl_HVAC_Airside_Calc_Engine[Heating Therms])","v":11480.225580000002},133.7438850798442,277102.11617537629]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,"Occupied (Start)","Unoccupied (Stop)",null,null,null,"Occupied (Start)","Unoccupied (Stop)"]
[null,null,4,18,"Weekday",null,null,4,18,{"$f":"IF(OR(C24<>H24,D24<>I24),\"*\",\"\")","v":""}]
[null,null,4,18,"Saturday",null,null,4,18,{"$f":"IF(OR(C25<>H25,D25<>I25),\"*\",\"\")","v":""}]
[null,null,4,18,"Sunday",null,null,4,18,{"$f":"IF(OR(C26<>H26,D26<>I26),\"*\",\"\")","v":""}]
[]
[null,"Economizer Optimization",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,null,null,"Data Type"]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,0.3,0.8,"Out Door Air %",null,null,0.3,1,{"$f":"IF(OR(C32<>H32,D32<>I32),\"*\",\"\")","v":"*"}]
[null,null,70,null,"Enable OAT",null,null,70,null,{"$f":"IF(OR(C33<>H33,D33<>I33),\"*\",\"\")","v":""}]
[]
[null,"Static Pressure Reset",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,1.8,1.8,"in. Water",null,null,1.8,1.8,{"$f":"IF(OR(C38<>H38,D38<>I38),\"*\",\"\")","v":""}]
[]
[null,"Supply Air Temperature Reset",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,55,55,"Supply Air Temp",null,null,58,55,{"$f":"IF(OR(C43<>H43,D43<>I43),\"*\",\"\")","v":"*"}]
[null,null,50,75,"@ OAT",null,null,50,75,{"$f":"IF(OR(C44<>H44,D44<>I44),\"*\",\"\")","v":""}]
[]
[null,"Fan and Space Temperature Setbacks",null,null,null,null,null,"Cost",null,"Disable"]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,0.4,1,"Occ Fan Speed % - Cool",null,null,0.4,1,{"$f":"IF(OR(C50<>H50,D50<>I50),\"*\",\"\")","v":""}]
[null,null,0.3,0.7,"Unocc Fan Speed % - Cool",null,null,0.3,0.7,""]
[null,null,55,95,"OA Cooling Temp Range",null,null,55,95,""]
[null,null,0.3,0.5,"Occ Fan Speed % - Heat",null,null,0.3,0.5,""]
[null,null,0.2,0.4,"Unocc Fan Speed % - Heat",null,null,0.2,0.4,""]
[null,null,50,30,"OA Heating Temp Range",null,null,50,30,""]
[null,null,"Heating","Cooling",null,null,null,"Heating","Cooling"]
[null,null,68,72,"Occ Space Temp",null,null,68,72,""]
[null,null,68,72,"Unocc Space Temp",null,null,68,72,""]
[]
[null,"VAV Flow Adjustment and Reheat Flow Adjustment",null,null,null,null,null,"Cost",null,"Enable"]
[null,null,"Baseline",null,null,null,null,"Proposed"]
[null,null,"Simple Data",null,"Data Type",null,null,"Simple Data"]
[null,null,70,70,"Discharge Air Temp",null,null,70,70,{"$f":"IF(OR(C63<>H63,D63<>I63),\"*\",\"\")","v":""}]
[null,null,85,40,"@ OAT",null,null,85,40,{"$f":"IF(OR(C64<>H64,D64<>I64),\"*\",\"\")","v":""}]
[null,null,"Min","Max",null,null,null,"Min","Max"]
[null,null,0.1,0.4,"Reheat Flow (% of fan flow)",null,null,0.1,0.4,{"$f":"IF(OR(C66<>H66,D66<>I66),\"*\",\"\")","v":""}]
[]
[null,"Processing"]
[null,null,"Switches"]
[null,null,"Proposed","Equipment Specifications & Replacements"]
[null,null,"Proposed","Scheduling Optimization"]
[null,null,"Proposed","Economizer Optimization"]
[null,null,"Proposed","Static Pressure Reset",null,null,null,null,null,null,null,null,null,null,null,null,null,"Fan Curves"]
[null,null,"Proposed","Supply Air Temperature Reset",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fan Curve"]
[null,null,"Proposed","Temperature And Fan Setback",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fan Penalty Per Delta SAT",0.01,null,"SF",null,"RF"]
[null,null,"Proposed","VAV Flow Adjustment",null,null,null,null,null,null,null,null,null,null,null,null,null,"Plenum (in)",null,{"$f":"1.5-($M$83-$L$83)","v":1.5},null,2,{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V76,1),VLOOKUP($C$90,$U$94:$Z$99,$V76,0)),0)","v":7.0428852E-2},"a",{"$f":"IFERROR(IF($C$93=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V76,1),VLOOKUP($C$93,$U$94:$Z$99,$V76,0)),0)","v":7.0428852E-2}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Return duct pressure loss",null,0.5,null,3,{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V77,1),VLOOKUP($C$90,$U$94:$Z$99,$V77,0)),0)","v":0.38533020099999998},"b",{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V77,1),VLOOKUP($C$90,$U$94:$Z$99,$V77,0)),0)","v":0.38533020099999998}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Est Supply Fan Eff",{"$f":"VLOOKUP($C$88,$R$82:$S$100,2,TRUE)","v":0.93},"VFD Eff",4,{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V78,1),VLOOKUP($C$90,$U$94:$Z$99,$V78,0)),0)","v":-0.46086411799999999},"c",{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V78,1),VLOOKUP($C$90,$U$94:$Z$99,$V78,0)),0)","v":-0.46086411799999999}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Est Return Fan Eff",{"$f":"VLOOKUP($C$91,$R$82:$S$100,2,TRUE)","v":0.89500000000000002},0.97,5,{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V79,1),VLOOKUP($C$90,$U$94:$Z$99,$V79,0)),0)","v":1.0092034400000001},"d",{"$f":"IFERROR(IF($C$90=\"VFD\",VLOOKUP($T$76,$U$82:$Y$90,$V79,1),VLOOKUP($C$90,$U$94:$Z$99,$V79,0)),0)","v":1.0092034400000001}]
[null,null,"Inputs"]
[null,null,"Equipment Specifications & Replacements",null,null,null,null,"Scheduling Optimization",null,null,null,"Static Pressure Reset",null,null,null,"Peak Demand Temp",null,"Motor HP","Efficiency",null,"Plenum in.","a","b","c","d"]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",H7=\"\",$C$70=\"Baseline\"),C7,H7)","v":1.5},"Seasonal average kW/Ton",null,null,null,"Occupied","Unoccupied",null,null,"Min","Max",null,null,{"$f":"'CTZ2'!$U$3","v":69},null,0,0.82499999999999996,null,0,2.7827882000000002E-2,2.6583195E-2,-8.7068699999999999E-2,1.03091975,"Perfect Reset"]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",H8=\"\",$C$70=\"Baseline\"),C8,H8)","v":"Gas"},"Source of Heating",null,null,null,{"$f":"IF(OR('Air Side System Template'!$J$21 = \"Disable\",'Air Side System Template'!H24=\"\",'Air Side System Template'!$C$71=\"Baseline\"),'Air Side System Template'!C24,'Air Side System Template'!H24)","v":4},{"$f":"IF(OR('Air Side System Template'!$J$21 = \"Disable\",'Air Side System Template'!I24=\"\",'Air Side System Template'!$C$71=\"Baseline\"),'Air Side System Template'!D24,'Air Side System Template'!I24)","v":18},{"$f":"'Air Side System Template'!E24","v":"Weekday"},null,{"$f":"IF(OR($J$35 = \"Disable\",H38=\"\",$C$73=\"Baseline\"),C38,H38)","v":1.8},{"$f":"IF(OR($J$35 = \"Disable\",I38=\"\",$C$73=\"Baseline\"),D38,I38)","v":1.8},"In H2O",null,null,null,1.5,0.84,null,0.3,3.4171263E-2,5.9448041E-2,-6.1049511000000001E-2,0.96614078199999998]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",H9=\"\",$C$70=\"Baseline\"),C9,H9)","v":0.8},"Gas Efficiency",null,null,null,{"$f":"IF(OR('Air Side System Template'!$J$21 = \"Disable\",'Air Side System Template'!H25=\"\",'Air Side System Template'!$C$71=\"Baseline\"),'Air Side System Template'!C25,'Air Side System Template'!H25)","v":4},{"$f":"IF(OR('Air Side System Template'!$J$21 = \"Disable\",'Air Side System Template'!I25=\"\",'Air Side System Template'!$C$71=\"Baseline\"),'Air Side System Template'!D25,'Air Side System Template'!I25)","v":18},{"$f":"'Air Side System Template'!E25","v":"Saturday"},null,null,null,null,null,null,null,2,0.84,null,0.4,3.7442571000000001E-2,7.2000619000000002E-2,-6.2564426000000006E-2,0.952238103]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",H10=\"\",$C$70=\"Baseline\"),C10,H10)","v":7},"Heat Pump (HSPF)",null,null,null,{"$f":"IF(OR('Air Side System Template'!$J$21 = \"Disable\",'Air Side System Template'!H26=\"\",'Air Side System Template'!$C$71=\"Baseline\"),'Air Side System Template'!C26,'Air Side System Template'!H26)","v":4},{"$f":"IF(OR('Air Side System Template'!$J$21 = \"Disable\",'Air Side System Template'!I26=\"\",'Air Side System Template'!$C$71=\"Baseline\"),'Air Side System Template'!D26,'Air Side System Template'!I26)","v":18},{"$f":"'Air Side System Template'!E26","v":"Sunday"},null,null,null,null,null,null,null,3,0.875,null,0.5,4.0759893999999998E-2,8.804497E-2,-7.2926119999999997E-2,0.94373982300000003]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",H12=\"\",$C$70=\"Baseline\"),C12,H12)","v":75},"Heating Lockout Temp",null,null,null,null,null,null,null,"Temperature And Fan Setback",null,null,null,null,null,5,0.875,null,0.6,4.4034586000000001E-2,0.107518462,-9.1288825000000004E-2,0.93991050399999998]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",I12=\"\",$C$70=\"Baseline\"),D12,I12)","v":55},"Cooling Lockout Temp",null,null,null,"Economizer Optimization",null,null,null,{"$f":"IF(OR($J$46 = \"Disable\",H48=\"\",$C$75=\"Baseline\"),C48,H48)","v":"Simple Data"},"Data type",null,null,null,null,7.5,0.89500000000000002,null,0.7,4.7182815000000003E-2,0.13054174199999999,-0.11728694200000001,0.94031374700000003]
[null,null,{"$f":"IF(OR($J$2 = \"Disable\",H13=\"\",$C$70=\"Baseline\"),C13,H13)","v":40},"Supply Fan (HP)",null,null,null,{"$f":"IF(OR($J$28 = \"Disable\",H30=\"\",$C$72=\"Baseline\"),H30,C30)","v":0},"Data Type",null,null,"Min","Max",null,null,null,null,10,0.89500000000000002,null,0.8,5.0254135999999998E-2,0.156227953,-0.14885733700000001,0.94369711899999997]
[null,null,60000,"Supply Fan (CFM)",null,null,null,"Min","Max",null,null,{"$f":"IF(OR($J$46 = \"Disable\",H50=\"\",$C$75=\"Baseline\"),C50,H50)","v":0.4},1,"Occ Fan Speed % - Cool",null,null,null,15,0.91,null,1,5.6118533999999998E-2,0.214726686,-0.22609305199999999,0.95764628799999996]
[null,null,"VFD","Supply Fan Control",null,null,null,{"$f":"IF(OR($J$28 = \"Disable\",H32=\"\",$C$72=\"Baseline\"),C32,H32)","v":0.3},{"$f":"IF(OR($J$28 = \"Disable\",I32=\"\",$C$72=\"Baseline\"),D32,I32)","v":0.8},"Out Door Air %",null,0.3,0.7,"Unocc Fan Speed % - Cool",null,null,null,20,0.91,null,1.5,7.0428852E-2,0.38533020099999998,-0.46086411799999999,1.0092034400000001,"No Reset"]
[null,null,10,"Return Fan (HP)",null,null,null,{"$f":"IF(OR($J$28 = \"Disable\",H33=\"\",$C$72=\"Baseline\"),C33,H33)","v":70},"Enable OAT",null,null,55,95,"OA Cooling Temp Range",null,null,null,25,0.92400000000000004,null,"https://energydesignresources.com/media/2651/EDR_DesignGuidelines_VAV.pdf?tracked=true"]
[null,null,60000,"Return Fan (CFM)",null,null,null,null,null,null,null,0.3,0.5,"Occ Fan Speed % - Heat",null,null,null,30,0.92400000000000004]
[null,null,"VFD","Return Fan Control",null,null,null,"VAV Flow Adjustment",null,null,null,0.2,0.4,"Unocc Fan Speed % - Heat",null,null,null,40,0.93,null,"FanType","a","b","c","d","Min Power"]
[null,null,0.9,"Return Fan % of Supply",null,null,null,{"$f":"IF(OR($J$60 = \"Disable\",H62=\"\",$C$75=\"Baseline\"),H62,C62)","v":"Simple Data"},"Data Type",null,null,50,30,"OA Heating Temp Range",null,null,null,50,0.93,null,"Damper",0.24891704000000001,1.1113770000000001,-0.36029412999999999,0.1,0.22]
[null,null,"Supply Air Temperature Reset",null,null,null,null,{"$f":"IF(OR($J$60 = \"Disable\",H63=\"\",$C$76=\"Baseline\"),C63,H63)","v":70},{"$f":"IF(OR($J$60 = \"Disable\",I63=\"\",$C$76=\"Baseline\"),D63,I63)","v":70},"Discharge Air Temp",null,"Heating","Cooling",null,null,null,null,60,0.93599999999999994,null,"IGV",0.62339776999999996,-0.73826223999999996,1.1148641100000001,0.25,0.22]
[null,null,{"$f":"IF(OR($J$40 = \"Disable\",H42=\"\",$C$74=\"Baseline\"),C42,H42)","v":"Simple Data"},"Data Type",null,null,null,{"$f":"IF(OR($J$60 = \"Disable\",H64=\"\",$C$76=\"Baseline\"),C64,H64)","v":85},{"$f":"IF(OR($J$60 = \"Disable\",I64=\"\",$C$76=\"Baseline\"),D64,I64)","v":40},"@ OAT",null,{"$f":"IF(OR($J$46 = \"Disable\",H57=\"\",$C$75=\"Baseline\"),C57,H57)","v":68},{"$f":"IF(OR($J$46 = \"Disable\",I57=\"\",$C$75=\"Baseline\"),D57,I57)","v":72},"Occ Space Temp",null,null,null,75,0.94099999999999995,null,"VFD",0.27196372000000002,-0.88568115000000003,1.66371739,0.2,0.1]
[null,null,null,null,null,null,null,"Min","Max",null,null,{"$f":"IF(OR($J$46 = \"Disable\",H58=\"\",$C$75=\"Baseline\"),C58,H58)","v":68},{"$f":"IF(OR($J$46 = \"Disable\",I58=\"\",$C$75=\"Baseline\"),D58,I58)","v":72},"Unocc Space Temp",null,null,null,100,0.94499999999999995,null,"Air-Foil or Backward-Inclined - Dampers Control Flow",0.22714300000000001,1.1789289999999999,-0.41071400000000002,0.45,0.68]
[null,null,null,null,null,null,null,{"$f":"IF(OR($J$60 = \"Disable\",H66=\"\",$C$76=\"Baseline\"),C66,H66)","v":0.1},{"$f":"IF(OR($J$60 = \"Disable\",I66=\"\",$C$76=\"Baseline\"),D66,I66)","v":0.4},"Reheat Flow (% of total)",null,null,null,null,null,null,null,125,0.94499999999999995,null,"Air-Foil or Backward-Inclined - Inlet Vanes",0.584345,-0.57916699999999999,0.97023800000000004,0.3,0.48]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,0.95,null,"Vane-Axial - Variable Pitch Blades",0.21204799999999999,-0.56928599999999996,1.3452379999999999,0.2,0.15]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,0.95,null,"*ASHRAE 90.1 Fan Curves"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,2,3,4,5,6,7,8,9,10,1,2,3,4,5,6,7,8,9,10]
[null,"Calculation Engine",null,null,null,"Baseline Trend Data",null,null,null,null,null,null,null,"Proposed Trend Data"]
[null,null,"OAT °F","Occ Hr","UnOcc Hr","SAT °F 1","DAT °F 1","RH Flow % 1","Occ SF Speed % 1"," Occ RAT °F 1","Unocc SF Speed % 1","UnOcc RAT °F 1","OA Flow % 1","SAT °F 2","DAT °F 2","RH Flow % 2","Occ SF Speed % 2","Occ RAT °F 2","Unocc SF Speed % 2","UnOcc RAT °F 2","OA Flow % 2","Base SAT","Proposed SAT","Delta SAT","SAT","DAT","RH Flow","Occ RAT °F","Occ OA Flow","Occ MAT °F","Occ Cooling Load","Occ Heating Load","Occ SF Speed %","Occ RF Speed %","Occ SF kW","Occ RF kW","Occ Load kW","UnOcc RAT °F","Unocc OA Flow %","UnOcc MAT °F","Unocc Cooling Load","Unocc Heating Load","Unocc SF Speed %","Unocc RF Speed %","Unocc SF kW","Unocc RF kW","Unocc Load kW","Fan kW","Fan kWh","Load kW","Load kWh","Heating Therms"]
[null,null,115,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C104,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C104,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C104,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q2-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C104>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},{"$f":"AB104*(1-AC104)+C104*AC104","v":84.9},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG104*(AD104-Y104)/12000),0),0)","v":161.46},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG104*AA104*(Z104-MIN(Y104,AD104))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},{"$f":"AG104*$C$94","v":0.8999999999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG104+$W$78*AG104^2+$W$79*AG104^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH104+$Y$78*AH104^2+$Y$79*AH104^3),0),0),0)","v":0},{"$f":"IF(D104>0,$C$82*AE104,0)+IFERROR(IF($C$83=\"Electric\",IF(D104>0,(AF104)/$C$85,0),0),0)","v":0},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C104>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},{"$f":"AL104*(1-AM104)+C104*AM104","v":84.9},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ104*(AN104-Y104)/12000),0),0)","v":113.02200000000001},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ104*AA104*(Z104-MIN(Y104,AN104))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},{"$f":"AQ104*$C$94","v":0.62999999999999989},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ104+$W$78*AQ104^2+$W$79*AQ104^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR104+$Y$78*AR104^2+$Y$79*AR104^3),0),0),0)","v":0},{"$f":"IF(E104>0,$C$82*AO104,0)+IFERROR(IF($C$83=\"Electric\",IF(E104>0,(AF104)/$C$85,0),0),0)","v":0},{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},{"$f":"IF($C$83=\"Gas\",(AF104/100/$C$84*D104)+(AP104/100/$C$84*E104),0)","v":0}]
[null,null,114,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C105,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C105,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C105,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q3-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C105>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},84.6,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG105*(AD105-Y105)/12000),0),0)","v":159.83999999999995},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG105*AA105*(Z105-MIN(Y105,AD105))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG105+$W$78*AG105^2+$W$79*AG105^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH105+$Y$78*AH105^2+$Y$79*AH105^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C105>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},84.6,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ105*(AN105-Y105)/12000),0),0)","v":111.88799999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ105*AA105*(Z105-MIN(Y105,AN105))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ105+$W$78*AQ105^2+$W$79*AQ105^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR105+$Y$78*AR105^2+$Y$79*AR105^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,113,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C106,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C106,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C106,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q4-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C106>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},84.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG106*(AD106-Y106)/12000),0),0)","v":158.21999999999997},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG106*AA106*(Z106-MIN(Y106,AD106))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG106+$W$78*AG106^2+$W$79*AG106^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH106+$Y$78*AH106^2+$Y$79*AH106^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C106>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},84.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ106*(AN106-Y106)/12000),0),0)","v":110.75399999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ106*AA106*(Z106-MIN(Y106,AN106))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ106+$W$78*AQ106^2+$W$79*AQ106^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR106+$Y$78*AR106^2+$Y$79*AR106^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,112,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C107,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C107,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C107,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q5-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C107>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},84,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG107*(AD107-Y107)/12000),0),0)","v":156.59999999999997},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG107*AA107*(Z107-MIN(Y107,AD107))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG107+$W$78*AG107^2+$W$79*AG107^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH107+$Y$78*AH107^2+$Y$79*AH107^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C107>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},84,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ107*(AN107-Y107)/12000),0),0)","v":109.61999999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ107*AA107*(Z107-MIN(Y107,AN107))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ107+$W$78*AQ107^2+$W$79*AQ107^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR107+$Y$78*AR107^2+$Y$79*AR107^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,111,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C108,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C108,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C108,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q6-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C108>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},83.699999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG108*(AD108-Y108)/12000),0),0)","v":154.97999999999993},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG108*AA108*(Z108-MIN(Y108,AD108))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG108+$W$78*AG108^2+$W$79*AG108^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH108+$Y$78*AH108^2+$Y$79*AH108^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C108>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},83.699999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ108*(AN108-Y108)/12000),0),0)","v":108.48599999999996},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ108*AA108*(Z108-MIN(Y108,AN108))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ108+$W$78*AQ108^2+$W$79*AQ108^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR108+$Y$78*AR108^2+$Y$79*AR108^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,110,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C109,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C109,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C109,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q7-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C109>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},83.4,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG109*(AD109-Y109)/12000),0),0)","v":153.36000000000001},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG109*AA109*(Z109-MIN(Y109,AD109))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG109+$W$78*AG109^2+$W$79*AG109^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH109+$Y$78*AH109^2+$Y$79*AH109^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C109>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},83.4,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ109*(AN109-Y109)/12000),0),0)","v":107.352},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ109*AA109*(Z109-MIN(Y109,AN109))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ109+$W$78*AQ109^2+$W$79*AQ109^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR109+$Y$78*AR109^2+$Y$79*AR109^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,109,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C110,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C110,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C110,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q8-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C110>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},83.1,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG110*(AD110-Y110)/12000),0),0)","v":151.73999999999995},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG110*AA110*(Z110-MIN(Y110,AD110))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG110+$W$78*AG110^2+$W$79*AG110^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH110+$Y$78*AH110^2+$Y$79*AH110^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C110>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},83.1,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ110*(AN110-Y110)/12000),0),0)","v":106.21799999999996},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ110*AA110*(Z110-MIN(Y110,AN110))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ110+$W$78*AQ110^2+$W$79*AQ110^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR110+$Y$78*AR110^2+$Y$79*AR110^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,108,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C111,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C111,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C111,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q9-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C111>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},82.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG111*(AD111-Y111)/12000),0),0)","v":150.11999999999995},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG111*AA111*(Z111-MIN(Y111,AD111))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG111+$W$78*AG111^2+$W$79*AG111^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH111+$Y$78*AH111^2+$Y$79*AH111^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C111>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},82.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ111*(AN111-Y111)/12000),0),0)","v":105.08399999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ111*AA111*(Z111-MIN(Y111,AN111))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ111+$W$78*AQ111^2+$W$79*AQ111^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR111+$Y$78*AR111^2+$Y$79*AR111^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,107,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C112,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C112,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C112,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q10-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C112>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},82.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG112*(AD112-Y112)/12000),0),0)","v":148.5},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG112*AA112*(Z112-MIN(Y112,AD112))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG112+$W$78*AG112^2+$W$79*AG112^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH112+$Y$78*AH112^2+$Y$79*AH112^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C112>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},82.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ112*(AN112-Y112)/12000),0),0)","v":103.94999999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ112*AA112*(Z112-MIN(Y112,AN112))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ112+$W$78*AQ112^2+$W$79*AQ112^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR112+$Y$78*AR112^2+$Y$79*AR112^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,106,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C113,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C113,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C113,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q11-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C113>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},82.199999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG113*(AD113-Y113)/12000),0),0)","v":146.87999999999991},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG113*AA113*(Z113-MIN(Y113,AD113))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG113+$W$78*AG113^2+$W$79*AG113^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH113+$Y$78*AH113^2+$Y$79*AH113^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C113>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},82.199999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ113*(AN113-Y113)/12000),0),0)","v":102.81599999999995},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ113*AA113*(Z113-MIN(Y113,AN113))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ113+$W$78*AQ113^2+$W$79*AQ113^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR113+$Y$78*AR113^2+$Y$79*AR113^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,105,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C114,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C114,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C114,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q12-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C114>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},81.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG114*(AD114-Y114)/12000),0),0)","v":145.26000000000002},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG114*AA114*(Z114-MIN(Y114,AD114))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG114+$W$78*AG114^2+$W$79*AG114^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH114+$Y$78*AH114^2+$Y$79*AH114^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C114>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},81.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ114*(AN114-Y114)/12000),0),0)","v":101.682},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ114*AA114*(Z114-MIN(Y114,AN114))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ114+$W$78*AQ114^2+$W$79*AQ114^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR114+$Y$78*AR114^2+$Y$79*AR114^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,104,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C115,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C115,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C115,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q13-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C115>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},81.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG115*(AD115-Y115)/12000),0),0)","v":143.63999999999993},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG115*AA115*(Z115-MIN(Y115,AD115))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG115+$W$78*AG115^2+$W$79*AG115^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH115+$Y$78*AH115^2+$Y$79*AH115^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C115>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},81.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ115*(AN115-Y115)/12000),0),0)","v":100.54799999999996},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ115*AA115*(Z115-MIN(Y115,AN115))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ115+$W$78*AQ115^2+$W$79*AQ115^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR115+$Y$78*AR115^2+$Y$79*AR115^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,103,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C116,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C116,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C116,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q14-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C116>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},81.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG116*(AD116-Y116)/12000),0),0)","v":142.01999999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG116*AA116*(Z116-MIN(Y116,AD116))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG116+$W$78*AG116^2+$W$79*AG116^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH116+$Y$78*AH116^2+$Y$79*AH116^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C116>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},81.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ116*(AN116-Y116)/12000),0),0)","v":99.413999999999973},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ116*AA116*(Z116-MIN(Y116,AN116))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ116+$W$78*AQ116^2+$W$79*AQ116^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR116+$Y$78*AR116^2+$Y$79*AR116^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,102,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C117,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C117,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C117,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q15-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C117>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},81,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG117*(AD117-Y117)/12000),0),0)","v":140.39999999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG117*AA117*(Z117-MIN(Y117,AD117))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG117+$W$78*AG117^2+$W$79*AG117^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH117+$Y$78*AH117^2+$Y$79*AH117^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C117>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},81,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ117*(AN117-Y117)/12000),0),0)","v":98.279999999999987},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ117*AA117*(Z117-MIN(Y117,AN117))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ117+$W$78*AQ117^2+$W$79*AQ117^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR117+$Y$78*AR117^2+$Y$79*AR117^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,101,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C118,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C118,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C118,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q16-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C118>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},80.699999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG118*(AD118-Y118)/12000),0),0)","v":138.77999999999992},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG118*AA118*(Z118-MIN(Y118,AD118))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG118+$W$78*AG118^2+$W$79*AG118^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH118+$Y$78*AH118^2+$Y$79*AH118^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C118>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},80.699999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ118*(AN118-Y118)/12000),0),0)","v":97.145999999999944},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ118*AA118*(Z118-MIN(Y118,AN118))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ118+$W$78*AQ118^2+$W$79*AQ118^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR118+$Y$78*AR118^2+$Y$79*AR118^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,100,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C119,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C119,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C119,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q17-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C119>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},80.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG119*(AD119-Y119)/12000),0),0)","v":137.16},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG119*AA119*(Z119-MIN(Y119,AD119))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG119+$W$78*AG119^2+$W$79*AG119^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH119+$Y$78*AH119^2+$Y$79*AH119^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C119>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},80.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ119*(AN119-Y119)/12000),0),0)","v":96.012000000000015},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ119*AA119*(Z119-MIN(Y119,AN119))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ119+$W$78*AQ119^2+$W$79*AQ119^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR119+$Y$78*AR119^2+$Y$79*AR119^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,99,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C120,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C120,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C120,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q18-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C120>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},80.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG120*(AD120-Y120)/12000),0),0)","v":135.53999999999996},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG120*AA120*(Z120-MIN(Y120,AD120))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG120+$W$78*AG120^2+$W$79*AG120^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH120+$Y$78*AH120^2+$Y$79*AH120^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C120>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},80.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ120*(AN120-Y120)/12000),0),0)","v":94.877999999999972},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ120*AA120*(Z120-MIN(Y120,AN120))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ120+$W$78*AQ120^2+$W$79*AQ120^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR120+$Y$78*AR120^2+$Y$79*AR120^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,98,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C121,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C121,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C121,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q19-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C121>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},79.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG121*(AD121-Y121)/12000),0),0)","v":133.91999999999996},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG121*AA121*(Z121-MIN(Y121,AD121))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG121+$W$78*AG121^2+$W$79*AG121^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH121+$Y$78*AH121^2+$Y$79*AH121^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C121>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},79.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ121*(AN121-Y121)/12000),0),0)","v":93.744},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ121*AA121*(Z121-MIN(Y121,AN121))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ121+$W$78*AQ121^2+$W$79*AQ121^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR121+$Y$78*AR121^2+$Y$79*AR121^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,97,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C122,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C122,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C122,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q20-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C122>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},79.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG122*(AD122-Y122)/12000),0),0)","v":132.29999999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG122*AA122*(Z122-MIN(Y122,AD122))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG122+$W$78*AG122^2+$W$79*AG122^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH122+$Y$78*AH122^2+$Y$79*AH122^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C122>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},79.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ122*(AN122-Y122)/12000),0),0)","v":92.609999999999985},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ122*AA122*(Z122-MIN(Y122,AN122))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ122+$W$78*AQ122^2+$W$79*AQ122^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR122+$Y$78*AR122^2+$Y$79*AR122^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,96,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C123,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C123,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C123,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q21-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C123>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},79.199999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG123*(AD123-Y123)/12000),0),0)","v":130.67999999999992},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG123*AA123*(Z123-MIN(Y123,AD123))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG123+$W$78*AG123^2+$W$79*AG123^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH123+$Y$78*AH123^2+$Y$79*AH123^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C123>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},79.199999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ123*(AN123-Y123)/12000),0),0)","v":91.475999999999942},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ123*AA123*(Z123-MIN(Y123,AN123))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ123+$W$78*AQ123^2+$W$79*AQ123^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR123+$Y$78*AR123^2+$Y$79*AR123^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,95,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C124,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C124,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C124,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q22-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C124>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},78.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG124*(AD124-Y124)/12000),0),0)","v":129.06000000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG124*AA124*(Z124-MIN(Y124,AD124))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.99999999999999978},0.8999999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG124+$W$78*AG124^2+$W$79*AG124^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH124+$Y$78*AH124^2+$Y$79*AH124^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C124>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},78.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ124*(AN124-Y124)/12000),0),0)","v":90.342000000000013},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ124*AA124*(Z124-MIN(Y124,AN124))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.69999999999999984},0.62999999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ124+$W$78*AQ124^2+$W$79*AQ124^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR124+$Y$78*AR124^2+$Y$79*AR124^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,94,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C125,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C125,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C125,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q23-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C125>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},78.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG125*(AD125-Y125)/12000),0),0)","v":125.52839999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG125*AA125*(Z125-MIN(Y125,AD125))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.98499999999999988},0.88649999999999995,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG125+$W$78*AG125^2+$W$79*AG125^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH125+$Y$78*AH125^2+$Y$79*AH125^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C125>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},78.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ125*(AN125-Y125)/12000),0),0)","v":87.933599999999956},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ125*AA125*(Z125-MIN(Y125,AN125))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.68999999999999984},0.62099999999999989,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ125+$W$78*AQ125^2+$W$79*AQ125^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR125+$Y$78*AR125^2+$Y$79*AR125^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,93,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C126,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C126,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C126,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q24-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C126>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},78.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG126*(AD126-Y126)/12000),0),0)","v":122.04539999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG126*AA126*(Z126-MIN(Y126,AD126))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.97},0.873,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG126+$W$78*AG126^2+$W$79*AG126^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH126+$Y$78*AH126^2+$Y$79*AH126^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C126>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},78.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ126*(AN126-Y126)/12000),0),0)","v":85.557599999999979},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ126*AA126*(Z126-MIN(Y126,AN126))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.67999999999999983},0.61199999999999988,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ126+$W$78*AQ126^2+$W$79*AQ126^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR126+$Y$78*AR126^2+$Y$79*AR126^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,92,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C127,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C127,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C127,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q25-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C127>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},78,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG127*(AD127-Y127)/12000),0),0)","v":118.61099999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG127*AA127*(Z127-MIN(Y127,AD127))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.95499999999999985},0.85949999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG127+$W$78*AG127^2+$W$79*AG127^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH127+$Y$78*AH127^2+$Y$79*AH127^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C127>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},78,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ127*(AN127-Y127)/12000),0),0)","v":83.213999999999984},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ127*AA127*(Z127-MIN(Y127,AN127))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.66999999999999982},0.60299999999999987,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ127+$W$78*AQ127^2+$W$79*AQ127^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR127+$Y$78*AR127^2+$Y$79*AR127^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,91,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C128,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C128,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C128,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":1},{"$f":"'CTZ2'!Q26-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C128>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},77.7,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG128*(AD128-Y128)/12000),0),0)","v":115.22520000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG128*AA128*(Z128-MIN(Y128,AD128))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.94},0.84599999999999997,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG128+$W$78*AG128^2+$W$79*AG128^3) ),0),0)","v":28.568068305863356},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH128+$Y$78*AH128^2+$Y$79*AH128^3),0),0),0)","v":5.8229397448419826},172.83780000000004,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C128>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},77.7,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ128*(AN128-Y128)/12000),0),0)","v":80.902800000000013},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ128*AA128*(Z128-MIN(Y128,AN128))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.65999999999999992},0.59399999999999997,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ128+$W$78*AQ128^2+$W$79*AQ128^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR128+$Y$78*AR128^2+$Y$79*AR128^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":34.391008050705338},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":34.391008050705338},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":172.83780000000004},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":172.83780000000004},0]
[null,null,90,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C129,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C129,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C129,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q27-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C129>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},77.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG129*(AD129-Y129)/12000),0),0)","v":111.88800000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG129*AA129*(Z129-MIN(Y129,AD129))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.92499999999999982},0.83249999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG129+$W$78*AG129^2+$W$79*AG129^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH129+$Y$78*AH129^2+$Y$79*AH129^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C129>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},77.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ129*(AN129-Y129)/12000),0),0)","v":78.624000000000024},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ129*AA129*(Z129-MIN(Y129,AN129))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.64999999999999991},0.58499999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ129+$W$78*AQ129^2+$W$79*AQ129^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR129+$Y$78*AR129^2+$Y$79*AR129^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,89,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C130,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C130,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C130,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":5},{"$f":"'CTZ2'!Q28-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C130>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},77.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG130*(AD130-Y130)/12000),0),0)","v":108.59939999999997},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG130*AA130*(Z130-MIN(Y130,AD130))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.90999999999999992},0.81899999999999995,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG130+$W$78*AG130^2+$W$79*AG130^3) ),0),0)","v":26.460852517091951},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH130+$Y$78*AH130^2+$Y$79*AH130^3),0),0),0)","v":5.424698281489567},162.89909999999998,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C130>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},77.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ130*(AN130-Y130)/12000),0),0)","v":76.377599999999973},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ130*AA130*(Z130-MIN(Y130,AN130))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.6399999999999999},0.57599999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ130+$W$78*AQ130^2+$W$79*AQ130^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR130+$Y$78*AR130^2+$Y$79*AR130^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":31.885550798581519},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":159.42775399290758},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":162.89909999999998},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":814.49549999999988},0]
[null,null,88,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C131,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C131,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C131,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":3},{"$f":"'CTZ2'!Q29-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C131>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},76.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG131*(AD131-Y131)/12000),0),0)","v":105.35939999999997},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG131*AA131*(Z131-MIN(Y131,AD131))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.8949999999999998},0.80549999999999988,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG131+$W$78*AG131^2+$W$79*AG131^3) ),0),0)","v":25.458808663500076},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH131+$Y$78*AH131^2+$Y$79*AH131^3),0),0),0)","v":5.2351260742114034},158.03909999999996,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C131>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},76.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ131*(AN131-Y131)/12000),0),0)","v":74.163599999999988},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ131*AA131*(Z131-MIN(Y131,AN131))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.62999999999999989},0.56699999999999995,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ131+$W$78*AQ131^2+$W$79*AQ131^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR131+$Y$78*AR131^2+$Y$79*AR131^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":30.69393473771148},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":92.081804213134433},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":158.03909999999996},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":474.11729999999989},0]
[null,null,87,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C132,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C132,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C132,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":5},{"$f":"'CTZ2'!Q30-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C132>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},76.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG132*(AD132-Y132)/12000),0),0)","v":102.16800000000001},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG132*AA132*(Z132-MIN(Y132,AD132))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.87999999999999989},0.79199999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG132+$W$78*AG132^2+$W$79*AG132^3) ),0),0)","v":24.490239501301492},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH132+$Y$78*AH132^2+$Y$79*AH132^3),0),0),0)","v":5.0517488575093736},153.25200000000001,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C132>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},76.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ132*(AN132-Y132)/12000),0),0)","v":71.981999999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ132*AA132*(Z132-MIN(Y132,AN132))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.61999999999999988},0.55799999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ132+$W$78*AQ132^2+$W$79*AQ132^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR132+$Y$78*AR132^2+$Y$79*AR132^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":29.541988358810865},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":147.70994179405432},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":153.25200000000001},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":766.26},0]
[null,null,86,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C133,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C133,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C133,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":10},{"$f":"'CTZ2'!Q31-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C133>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},76.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG133*(AD133-Y133)/12000),0),0)","v":99.025200000000027},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG133*AA133*(Z133-MIN(Y133,AD133))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.86499999999999999},0.77849999999999997,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG133+$W$78*AG133^2+$W$79*AG133^3) ),0),0)","v":23.554469028644231},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH133+$Y$78*AH133^2+$Y$79*AH133^3),0),0),0)","v":4.8744386121165597},148.53780000000003,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C133>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},76.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ133*(AN133-Y133)/12000),0),0)","v":69.832799999999992},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ133*AA133*(Z133-MIN(Y133,AN133))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.60999999999999988},0.54899999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ133+$W$78*AQ133^2+$W$79*AQ133^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR133+$Y$78*AR133^2+$Y$79*AR133^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":28.428907640760791},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":284.28907640760792},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":148.53780000000003},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":1485.3780000000004},0]
[null,null,85,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C134,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C134,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C134,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":6},{"$f":"'CTZ2'!Q32-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10000000000000009},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C134>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},75.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG134*(AD134-Y134)/12000),0),0)","v":95.931000000000012},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG134*AA134*(Z134-MIN(Y134,AD134))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.84999999999999987},0.7649999999999999,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG134+$W$78*AG134^2+$W$79*AG134^3) ),0),0)","v":22.650821243676305},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH134+$Y$78*AH134^2+$Y$79*AH134^3),0),0),0)","v":4.7030673187660392},143.8965,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C134>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},75.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ134*(AN134-Y134)/12000),0),0)","v":67.716000000000022},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ134*AA134*(Z134-MIN(Y134,AN134))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.59999999999999987},0.53999999999999992,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ134+$W$78*AQ134^2+$W$79*AQ134^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR134+$Y$78*AR134^2+$Y$79*AR134^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":27.353888562442343},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":164.12333137465407},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":143.8965},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":863.37900000000002},0]
[null,null,84,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C135,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C135,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C135,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":8},{"$f":"'CTZ2'!Q33-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.10666666666666669},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C135>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},75.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG135*(AD135-Y135)/12000),0),0)","v":92.885399999999976},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG135*AA135*(Z135-MIN(Y135,AD135))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.83499999999999996},0.75149999999999995,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG135+$W$78*AG135^2+$W$79*AG135^3) ),0),0)","v":21.778620144545791},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH135+$Y$78*AH135^2+$Y$79*AH135^3),0),0),0)","v":4.5375069581908942},139.32809999999995,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C135>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},75.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ135*(AN135-Y135)/12000),0),0)","v":65.631599999999992},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ135*AA135*(Z135-MIN(Y135,AN135))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.59},0.53100000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ135+$W$78*AQ135^2+$W$79*AQ135^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR135+$Y$78*AR135^2+$Y$79*AR135^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":26.316127102736687},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":210.52901682189349},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":139.32809999999995},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":1114.6247999999996},0]
[null,null,83,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C136,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C136,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C136,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":15},{"$f":"'CTZ2'!Q34-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.1133333333333334},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C136>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},{"$f":"AB136*(1-AC136)+C136*AC136","v":75.3},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG136*(AD136-Y136)/12000),0),0)","v":89.888399999999976},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG136*AA136*(Z136-MIN(Y136,AD136))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.81999999999999984},{"$f":"AG136*$C$94","v":0.73799999999999988},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG136+$W$78*AG136^2+$W$79*AG136^3) ),0),0)","v":20.937189729400686},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH136+$Y$78*AH136^2+$Y$79*AH136^3),0),0),0)","v":4.3776295111242014},{"$f":"IF(D136>0,$C$82*AE136,0)+IFERROR(IF($C$83=\"Electric\",IF(D136>0,(AF136)/$C$85,0),0),0)","v":134.83259999999996},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C136>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},{"$f":"AL136*(1-AM136)+C136*AM136","v":75.3},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ136*(AN136-Y136)/12000),0),0)","v":63.579599999999992},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ136*AA136*(Z136-MIN(Y136,AN136))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.57999999999999996},{"$f":"AQ136*$C$94","v":0.52200000000000002},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ136+$W$78*AQ136^2+$W$79*AQ136^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR136+$Y$78*AR136^2+$Y$79*AR136^3),0),0),0)","v":0},{"$f":"IF(E136>0,$C$82*AO136,0)+IFERROR(IF($C$83=\"Electric\",IF(E136>0,(AF136)/$C$85,0),0),0)","v":0},{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":25.314819240524887},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":379.72228860787328},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":134.83259999999996},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":2022.4889999999994},{"$f":"IF($C$83=\"Gas\",(AF136/100/$C$84*D136)+(AP136/100/$C$84*E136),0)","v":0}]
[null,null,82,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C137,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C137,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C137,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":15},{"$f":"'CTZ2'!Q35-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.12},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C137>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},75,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG137*(AD137-Y137)/12000),0),0)","v":86.94},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG137*AA137*(Z137-MIN(Y137,AD137))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.80499999999999994},0.72449999999999992,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG137+$W$78*AG137^2+$W$79*AG137^3) ),0),0)","v":20.125853996389068},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH137+$Y$78*AH137^2+$Y$79*AH137^3),0),0),0)","v":4.2233069582990446},130.41,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C137>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},75,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ137*(AN137-Y137)/12000),0),0)","v":61.56},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ137*AA137*(Z137-MIN(Y137,AN137))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.56999999999999995},0.51300000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ137+$W$78*AQ137^2+$W$79*AQ137^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR137+$Y$78*AR137^2+$Y$79*AR137^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":24.349160954688113},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":365.2374143203217},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":130.41},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":1956.1499999999999},0]
[null,null,81,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C138,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":10},{"$f":"'CTZ2'!Q36-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.12666666666666671},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C138>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},74.7,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG138*(AD138-Y138)/12000),0),0)","v":84.040200000000027},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG138*AA138*(Z138-MIN(Y138,AD138))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.79},0.71100000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG138+$W$78*AG138^2+$W$79*AG138^3) ),0),0)","v":19.343936943658957},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH138+$Y$78*AH138^2+$Y$79*AH138^3),0),0),0)","v":4.0744112804485022},126.06030000000004,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C138>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},74.7,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ138*(AN138-Y138)/12000),0),0)","v":59.572800000000008},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ138*AA138*(Z138-MIN(Y138,AN138))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.55999999999999994},0.504,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ138+$W$78*AQ138^2+$W$79*AQ138^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR138+$Y$78*AR138^2+$Y$79*AR138^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":23.418348224107458},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":234.18348224107459},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":126.06030000000004},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":1260.6030000000005},0]
[null,null,80,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C139,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":28},{"$f":"'CTZ2'!Q37-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.13333333333333341},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C139>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},74.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG139*(AD139-Y139)/12000),0),0)","v":81.189000000000007},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG139*AA139*(Z139-MIN(Y139,AD139))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.77499999999999991},0.6974999999999999,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG139+$W$78*AG139^2+$W$79*AG139^3) ),0),0)","v":18.590762569358386},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH139+$Y$78*AH139^2+$Y$79*AH139^3),0),0),0)","v":3.9308144583056506},121.7835,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C139>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},74.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ139*(AN139-Y139)/12000),0),0)","v":57.618000000000016},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ139*AA139*(Z139-MIN(Y139,AN139))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.54999999999999993},0.49499999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ139+$W$78*AQ139^2+$W$79*AQ139^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR139+$Y$78*AR139^2+$Y$79*AR139^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":22.521577027664037},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":630.60415677459309},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":121.7835},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":3409.9380000000001},0]
[null,null,79,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C140,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":27},{"$f":"'CTZ2'!Q38-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.14000000000000001},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C140>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},74.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG140*(AD140-Y140)/12000),0),0)","v":78.386399999999995},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG140*AA140*(Z140-MIN(Y140,AD140))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.76},0.68400000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG140+$W$78*AG140^2+$W$79*AG140^3) ),0),0)","v":17.865654871635407},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH140+$Y$78*AH140^2+$Y$79*AH140^3),0),0),0)","v":3.7923884726035753},117.5796,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C140>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},74.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ140*(AN140-Y140)/12000),0),0)","v":55.695599999999978},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ140*AA140*(Z140-MIN(Y140,AN140))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.53999999999999992},0.48599999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ140+$W$78*AQ140^2+$W$79*AQ140^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR140+$Y$78*AR140^2+$Y$79*AR140^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":21.658043344238983},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":584.76717029445251},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":117.5796},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":3174.6491999999998},0]
[null,null,78,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C141,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":33},{"$f":"'CTZ2'!Q39-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.14666666666666672},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C141>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},73.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG141*(AD141-Y141)/12000),0),0)","v":75.632399999999976},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG141*AA141*(Z141-MIN(Y141,AD141))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.74499999999999988},0.67049999999999987,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG141+$W$78*AG141^2+$W$79*AG141^3) ),0),0)","v":17.16793784863804},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH141+$Y$78*AH141^2+$Y$79*AH141^3),0),0),0)","v":3.6590053040753494},113.44859999999997,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C141>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},73.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ141*(AN141-Y141)/12000),0),0)","v":53.805599999999991},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ141*AA141*(Z141-MIN(Y141,AN141))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.52999999999999992},0.47699999999999992,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ141+$W$78*AQ141^2+$W$79*AQ141^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR141+$Y$78*AR141^2+$Y$79*AR141^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":20.82694315271339},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":687.28912403954189},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":113.44859999999997},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":3743.8037999999992},0]
[null,null,77,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C142,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":20},{"$f":"'CTZ2'!Q40-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.15333333333333332},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C142>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},73.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG142*(AD142-Y142)/12000),0),0)","v":72.926999999999992},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG142*AA142*(Z142-MIN(Y142,AD142))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.73},0.65700000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG142+$W$78*AG142^2+$W$79*AG142^3) ),0),0)","v":16.49693549851435},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH142+$Y$78*AH142^2+$Y$79*AH142^3),0),0),0)","v":3.5305369334540608},109.39049999999999,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C142>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},73.5,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ142*(AN142-Y142)/12000),0),0)","v":51.947999999999993},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ142*AA142*(Z142-MIN(Y142,AN142))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.51999999999999991},0.46799999999999992,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ142+$W$78*AQ142^2+$W$79*AQ142^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR142+$Y$78*AR142^2+$Y$79*AR142^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":20.027472431968413},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":400.54944863936828},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":109.39049999999999},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":2187.81},0]
[null,null,76,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C143,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":50},{"$f":"'CTZ2'!Q41-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.16000000000000003},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C143>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},73.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG143*(AD143-Y143)/12000),0),0)","v":70.270200000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG143*AA143*(Z143-MIN(Y143,AD143))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.71499999999999986},0.64349999999999985,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG143+$W$78*AG143^2+$W$79*AG143^3) ),0),0)","v":15.85197181941235},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH143+$Y$78*AH143^2+$Y$79*AH143^3),0),0),0)","v":3.4068553414727822},105.40530000000001,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C143>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},73.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ143*(AN143-Y143)/12000),0),0)","v":50.122800000000005},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ143*AA143*(Z143-MIN(Y143,AN143))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5099999999999999},0.45899999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ143+$W$78*AQ143^2+$W$79*AQ143^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR143+$Y$78*AR143^2+$Y$79*AR143^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":19.258827160885133},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":962.94135804425662},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":105.40530000000001},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":5270.2650000000003},0]
[null,null,75,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C144,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":46},{"$f":"'CTZ2'!Q42-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.16666666666666674},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C144>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},72.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG144*(AD144-Y144)/12000),0),0)","v":67.662000000000035},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG144*AA144*(Z144-MIN(Y144,AD144))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.7},0.63,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG144+$W$78*AG144^2+$W$79*AG144^3) ),0),0)","v":15.232370809480102},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH144+$Y$78*AH144^2+$Y$79*AH144^3),0),0),0)","v":3.2878325088645979},101.49300000000005,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C144>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},72.900000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ144*(AN144-Y144)/12000),0),0)","v":48.33000000000002},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ144*AA144*(Z144-MIN(Y144,AN144))/10^3),0)","v":0},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ144+$W$78*AQ144^2+$W$79*AQ144^3) ),0),0)","v":9.064411987052436},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR144+$Y$78*AR144^2+$Y$79*AR144^3),0),0),0)","v":2.0835077697477398},72.495000000000033,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":18.520203318344699},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":863.0772724006564},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":173.98800000000008},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":4741.1730000000025},0]
[null,null,74,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C145,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":60},{"$f":"'CTZ2'!Q43-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.17333333333333339},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C145>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},72.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG145*(AD145-Y145)/12000),0),0)","v":65.102400000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG145*AA145*(Z145-MIN(Y145,AD145))/10^3),0)","v":115.40880000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.68500000000000005},0.61650000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG145+$W$78*AG145^2+$W$79*AG145^3) ),0),0)","v":14.637456466865631},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH145+$Y$78*AH145^2+$Y$79*AH145^3),0),0),0)","v":3.1733404163625853},97.653600000000012,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C145>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},72.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ145*(AN145-Y145)/12000),0),0)","v":46.569599999999987},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ145*AA145*(Z145-MIN(Y145,AN145))/10^3),0)","v":82.555200000000042},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.49},0.441,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ145+$W$78*AQ145^2+$W$79*AQ145^3) ),0),0)","v":8.8424758961528411},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR145+$Y$78*AR145^2+$Y$79*AR145^3),0),0),0)","v":2.0389917970494276},69.854399999999984,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":17.810796883228218},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1079.5292806868954},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":167.50799999999998},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":5929.0704000000005},87.588540000000052]
[null,null,73,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C146,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":65},{"$f":"'CTZ2'!Q44-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.18000000000000005},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C146>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},72.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG146*(AD146-Y146)/12000),0),0)","v":62.591399999999993},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG146*AA146*(Z146-MIN(Y146,AD146))/10^3),0)","v":117.22320000000002},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.66999999999999993},0.60299999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG146+$W$78*AG146^2+$W$79*AG146^3) ),0),0)","v":14.066552789716967},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH146+$Y$78*AH146^2+$Y$79*AH146^3),0),0),0)","v":3.0632510446998249},93.88709999999999,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C146>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},72.3,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ146*(AN146-Y146)/12000),0),0)","v":44.8416},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ146*AA146*(Z146-MIN(Y146,AN146))/10^3),0)","v":83.980800000000031},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.48},0.432,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ146+$W$78*AQ146^2+$W$79*AQ146^3) ),0),0)","v":8.6273054236489486},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR146+$Y$78*AR146^2+$Y$79*AR146^3),0),0),0)","v":1.9956929222930233},67.2624,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":17.129803834416791},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1145.3062442749174},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":161.14949999999999},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":6304.448699999999},98.393130000000014]
[null,null,72,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C147,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":77},{"$f":"'CTZ2'!Q45-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.1866666666666667},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C147>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},72,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG147*(AD147-Y147)/12000),0),0)","v":60.129000000000005},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG147*AA147*(Z147-MIN(Y147,AD147))/10^3),0)","v":118.84320000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.65500000000000003},0.58950000000000002,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG147+$W$78*AG147^2+$W$79*AG147^3) ),0),0)","v":13.51898377618217},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH147+$Y$78*AH147^2+$Y$79*AH147^3),0),0),0)","v":2.9574363746093972},90.1935,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":72},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C147>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},72,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ147*(AN147-Y147)/12000),0),0)","v":43.146000000000001},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ147*AA147*(Z147-MIN(Y147,AN147))/10^3),0)","v":85.276800000000023},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.47},0.42299999999999999,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ147+$W$78*AQ147^2+$W$79*AQ147^3) ),0),0)","v":8.4187002726957232},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR147+$Y$78*AR147^2+$Y$79*AR147^3),0),0),0)","v":1.9535732138438817},64.718999999999994,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":16.476420150791569},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1299.8011720705695},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":154.91249999999999},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":7139.0565000000006},117.58446000000002]
[null,null,71,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C148,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":133},{"$f":"'CTZ2'!Q46-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.19333333333333336},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":71},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C148>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},71,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG148*(AD148-Y148)/12000),0),0)","v":55.295999999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG148*AA148*(Z148-MIN(Y148,AD148))/10^3),0)","v":120.26880000000001},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.6399999999999999},0.57599999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG148+$W$78*AG148^2+$W$79*AG148^3) ),0),0)","v":12.994073424409253},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH148+$Y$78*AH148^2+$Y$79*AH148^3),0),0),0)","v":2.8557683868243808},82.944000000000003,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":71},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C148>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},71,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ148*(AN148-Y148)/12000),0),0)","v":39.744},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ148*AA148*(Z148-MIN(Y148,AN148))/10^3),0)","v":86.443200000000019},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.45999999999999996},0.41399999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ148+$W$78*AQ148^2+$W$79*AQ148^3) ),0),0)","v":8.2164601464481475},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR148+$Y$78*AR148^2+$Y$79*AR148^3),0),0),0)","v":1.9125947400673606},59.616,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":15.849841811233635},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2148.5451804401355},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":142.56},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":11270.016},204.26904000000002]
[null,null,70,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C149,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":103},{"$f":"'CTZ2'!Q47-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.20000000000000007},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":70},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C149>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},70,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG149*(AD149-Y149)/12000),0),0)","v":50.625000000000007},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG149*AA149*(Z149-MIN(Y149,AD149))/10^3),0)","v":121.50000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.625},0.5625,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG149+$W$78*AG149^2+$W$79*AG149^3) ),0),0)","v":12.491145732546283},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH149+$Y$78*AH149^2+$Y$79*AH149^3),0),0),0)","v":2.758119062077856},75.937500000000014,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":70},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C149>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},70,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ149*(AN149-Y149)/12000),0),0)","v":36.450000000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ149*AA149*(Z149-MIN(Y149,AN149))/10^3),0)","v":87.480000000000032},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.44999999999999996},0.40499999999999997,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ149+$W$78*AQ149^2+$W$79*AQ149^3) ),0),0)","v":8.0203847480611898},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR149+$Y$78*AR149^2+$Y$79*AR149^3),0),0),0)","v":1.8727195693288172},54.675000000000004,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":15.249264794624139},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1649.8191083854063},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":130.61250000000001},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":8258.9625000000015},165.17925000000008]
[null,null,69,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C150,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":124},{"$f":"'CTZ2'!Q48-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":11},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.20666666666666672},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":69},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C150>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},69,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG150*(AD150-Y150)/12000),0),0)","v":46.116000000000014},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG150*AA150*(Z150-MIN(Y150,AD150))/10^3),0)","v":122.53680000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.6100000000000001},0.54900000000000015,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG150+$W$78*AG150^2+$W$79*AG150^3) ),0),0)","v":12.009524698741281},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH150+$Y$78*AH150^2+$Y$79*AH150^3),0),0),0)","v":2.6643603811029042},69.174000000000021,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":69},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C150>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},69,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ150*(AN150-Y150)/12000),0),0)","v":33.264000000000003},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ150*AA150*(Z150-MIN(Y150,AN150))/10^3),0)","v":88.387200000000021},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.43999999999999995},0.39599999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ150+$W$78*AQ150^2+$W$79*AQ150^3) ),0),0)","v":7.8302737806898275},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR150+$Y$78*AR150^2+$Y$79*AR150^3),0),0),0)","v":1.8339097699936084},49.896000000000001,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":14.673885079844185},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1925.8677689581968},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":119.07000000000002},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":9126.4320000000025},202.08528000000007]
[null,null,68,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C151,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":131},{"$f":"'CTZ2'!Q49-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":7},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.21333333333333337},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C151>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},68,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG151*(AD151-Y151)/12000),0),0)","v":41.768999999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG151*AA151*(Z151-MIN(Y151,AD151))/10^3),0)","v":123.37920000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.59499999999999997},0.53549999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG151+$W$78*AG151^2+$W$79*AG151^3) ),0),0)","v":11.548534321142283},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH151+$Y$78*AH151^2+$Y$79*AH151^3),0),0),0)","v":2.5743643246326009},62.653499999999994,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C151>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},68,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ151*(AN151-Y151)/12000),0),0)","v":30.186000000000007},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ151*AA151*(Z151-MIN(Y151,AN151))/10^3),0)","v":89.164800000000028},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.43000000000000005},0.38700000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ151+$W$78*AQ151^2+$W$79*AQ151^3) ),0),0)","v":7.6459269474890377},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR151+$Y$78*AR151^2+$Y$79*AR151^3),0),0),0)","v":1.7961274104270917},45.279000000000011,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":14.122898645774884},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1916.1941031019226},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":107.9325},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":8524.561499999998},209.83536000000007]
[null,null,67,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C152,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":157},{"$f":"'CTZ2'!Q50-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":23},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.22000000000000003},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C152>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},67.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG152*(AD152-Y152)/12000),0),0)","v":38.210400000000014},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG152*AA152*(Z152-MIN(Y152,AD152))/10^3),0)","v":124.02720000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.58000000000000007},0.52200000000000013,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG152+$W$78*AG152^2+$W$79*AG152^3) ),0),0)","v":11.107498597897338},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH152+$Y$78*AH152^2+$Y$79*AH152^3),0),0),0)","v":2.4880028734000308},57.315600000000018,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C152>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},67.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ152*(AN152-Y152)/12000),0),0)","v":27.669600000000013},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ152*AA152*(Z152-MIN(Y152,AN152))/10^3),0)","v":89.812800000000038},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.42000000000000004},0.37800000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ152+$W$78*AQ152^2+$W$79*AQ152^3) ),0),0)","v":7.4671439516137879},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR152+$Y$78*AR152^2+$Y$79*AR152^3),0),0),0)","v":1.7593345589946221},41.504400000000018,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":13.59550147129737},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2346.7027367376804},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":98.820000000000036},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":9953.1504000000041},269.22456000000005]
[null,null,66,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C153,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":149},{"$f":"'CTZ2'!Q51-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":16},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.22666666666666674},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C153>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},66.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG153*(AD153-Y153)/12000),0),0)","v":34.781400000000026},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG153*AA153*(Z153-MIN(Y153,AD153))/10^3),0)","v":124.48080000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.56500000000000006},0.50850000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG153+$W$78*AG153^2+$W$79*AG153^3) ),0),0)","v":10.685741527154482},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH153+$Y$78*AH153^2+$Y$79*AH153^3),0),0),0)","v":2.4051480081382706},52.172100000000043,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C153>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},66.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ153*(AN153-Y153)/12000),0),0)","v":25.239600000000021},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ153*AA153*(Z153-MIN(Y153,AN153))/10^3),0)","v":90.331200000000038},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.41000000000000003},0.36900000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ153+$W$78*AQ153^2+$W$79*AQ153^3) ),0),0)","v":7.2937244962190562},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR153+$Y$78*AR153^2+$Y$79*AR153^3),0),0),0)","v":1.7234932840615584},37.859400000000029,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":13.090889535292753},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2094.8180252431098},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":90.031500000000079},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":8379.393300000007},249.91173000000015]
[null,null,65,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C154,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":177},{"$f":"'CTZ2'!Q52-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":42},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.23333333333333339},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C154>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},65.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG154*(AD154-Y154)/12000),0),0)","v":31.481999999999989},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG154*AA154*(Z154-MIN(Y154,AD154))/10^3),0)","v":124.74000000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.55000000000000004},0.49500000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG154+$W$78*AG154^2+$W$79*AG154^3) ),0),0)","v":10.282587107061747},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH154+$Y$78*AH154^2+$Y$79*AH154^3),0),0),0)","v":2.3256717095804014},47.222999999999985,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C154>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},65.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ154*(AN154-Y154)/12000),0),0)","v":22.895999999999987},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ154*AA154*(Z154-MIN(Y154,AN154))/10^3),0)","v":90.720000000000041},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ154+$W$78*AQ154^2+$W$79*AQ154^3) ),0),0)","v":7.1254682844598172},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR154+$Y$78*AR154^2+$Y$79*AR154^3),0),0),0)","v":1.6885656539932572},34.34399999999998,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":12.608258816642149},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2601.8512359606898},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":81.566999999999965},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":9800.9189999999962},323.61525000000012]
[null,null,64,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C155,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":187},{"$f":"'CTZ2'!Q53-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":58},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.24000000000000005},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C155>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},64.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG155*(AD155-Y155)/12000),0),0)","v":28.312199999999997},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG155*AA155*(Z155-MIN(Y155,AD155))/10^3),0)","v":124.80480000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.53500000000000003},0.48150000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG155+$W$78*AG155^2+$W$79*AG155^3) ),0),0)","v":9.8973593357671774},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH155+$Y$78*AH155^2+$Y$79*AH155^3),0),0),0)","v":2.2494459584595026},42.468299999999999,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C155>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},64.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ155*(AN155-Y155)/12000),0),0)","v":20.6388},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ155*AA155*(Z155-MIN(Y155,AN155))/10^3),0)","v":90.979200000000034},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.39},0.35100000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ155+$W$78*AQ155^2+$W$79*AQ155^3) ),0),0)","v":6.9621750194910454},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR155+$Y$78*AR155^2+$Y$79*AR155^3),0),0),0)","v":1.6545137371550758},30.958199999999998,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":12.146805294226681},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2771.2205379058646},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":73.426500000000004},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":9737.1476999999995},357.69114000000008]
[null,null,63,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C156,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":153},{"$f":"'CTZ2'!Q54-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":47},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.2466666666666667},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C156>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},64,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG156*(AD156-Y156)/12000),0),0)","v":25.272000000000002},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG156*AA156*(Z156-MIN(Y156,AD156))/10^3),0)","v":124.67520000000003},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.52},0.46800000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG156+$W$78*AG156^2+$W$79*AG156^3) ),0),0)","v":9.5293822114188131},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH156+$Y$78*AH156^2+$Y$79*AH156^3),0),0),0)","v":2.1763427355086549},37.908000000000001,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C156>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},64,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ156*(AN156-Y156)/12000),0),0)","v":18.468},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ156*AA156*(Z156-MIN(Y156,AN156))/10^3),0)","v":91.108800000000031},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.38},0.34200000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ156+$W$78*AQ156^2+$W$79*AQ156^3) ),0),0)","v":6.8036444044677138},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR156+$Y$78*AR156^2+$Y$79*AR156^3),0),0),0)","v":1.6212996019123704},27.701999999999998,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":11.705724946927468},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2186.9482851797666},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":65.61},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":7101.9179999999997},291.96774000000005]
[null,null,62,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C157,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":202},{"$f":"'CTZ2'!Q55-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":110},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.25333333333333335},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C157>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},63.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG157*(AD157-Y157)/12000),0),0)","v":22.36140000000001},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG157*AA157*(Z157-MIN(Y157,AD157))/10^3),0)","v":124.35120000000002},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.505},0.45450000000000002,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG157+$W$78*AG157^2+$W$79*AG157^3) ),0),0)","v":9.1779797321646885},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH157+$Y$78*AH157^2+$Y$79*AH157^3),0),0),0)","v":2.1062340214609363},33.542100000000019,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C157>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},63.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ157*(AN157-Y157)/12000),0),0)","v":16.383600000000008},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ157*AA157*(Z157-MIN(Y157,AN157))/10^3),0)","v":91.108800000000016},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.37},0.33300000000000002,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ157+$W$78*AQ157^2+$W$79*AQ157^3) ),0),0)","v":6.6496761425447968},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR157+$Y$78*AR157^2+$Y$79*AR157^3),0),0),0)","v":1.5888853166304981},24.575400000000013,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":11.284213753625625},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":3185.6529387416585},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":58.117500000000035},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":9478.7982000000047},439.26138000000003]
[null,null,61,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C158,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":218},{"$f":"'CTZ2'!Q56-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":125},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.26000000000000006},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C158>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},62.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG158*(AD158-Y158)/12000),0),0)","v":19.580400000000019},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG158*AA158*(Z158-MIN(Y158,AD158))/10^3),0)","v":123.83280000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4900000000000001},0.44100000000000011,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG158+$W$78*AG158^2+$W$79*AG158^3) ),0),0)","v":8.8424758961528465},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH158+$Y$78*AH158^2+$Y$79*AH158^3),0),0),0)","v":2.0389917970494289},29.370600000000028,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C158>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},62.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ158*(AN158-Y158)/12000),0),0)","v":14.385600000000013},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ158*AA158*(Z158-MIN(Y158,AN158))/10^3),0)","v":90.97920000000002},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.36},0.32400000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ158+$W$78*AQ158^2+$W$79*AQ158^3) ),0),0)","v":6.5000699368772716},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR158+$Y$78*AR158^2+$Y$79*AR158^3),0),0),0)","v":1.5572329496748165},21.57840000000002,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":10.881467693202275},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":3379.3228179371072},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":50.949000000000048},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":9100.090800000009},479.59938000000011]
[null,null,60,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C159,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":268},{"$f":"'CTZ2'!Q57-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":199},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.26666666666666672},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C159>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},61.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG159*(AD159-Y159)/12000),0),0)","v":16.928999999999991},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG159*AA159*(Z159-MIN(Y159,AD159))/10^3),0)","v":123.12000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.47500000000000009},0.4275000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG159+$W$78*AG159^2+$W$79*AG159^3) ),0),0)","v":8.5221947015313173},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH159+$Y$78*AH159^2+$Y$79*AH159^3),0),0),0)","v":1.9744880430072098},25.393499999999989,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C159>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},61.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ159*(AN159-Y159)/12000),0),0)","v":12.47399999999999},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ159*AA159*(Z159-MIN(Y159,AN159))/10^3),0)","v":90.720000000000013},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.35},0.315,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ159+$W$78*AQ159^2+$W$79*AQ159^3) ),0),0)","v":6.3546254906201103},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR159+$Y$78*AR159^2+$Y$79*AR159^3),0),0),0)","v":1.526304569410682},18.710999999999984,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":10.496682744538527},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":4381.4160574824527},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":44.104499999999973},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":10528.946999999993},638.11800000000017]
[null,null,59,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C160,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":243},{"$f":"'CTZ2'!Q58-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":212},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.27333333333333337},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C160>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},60.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG160*(AD160-Y160)/12000),0),0)","v":14.407199999999998},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG160*AA160*(Z160-MIN(Y160,AD160))/10^3),0)","v":122.21280000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.46000000000000008},0.41400000000000009,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG160+$W$78*AG160^2+$W$79*AG160^3) ),0),0)","v":8.216460146448151},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH160+$Y$78*AH160^2+$Y$79*AH160^3),0),0),0)","v":1.9125947400673613},21.610799999999998,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C160>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},60.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ160*(AN160-Y160)/12000),0),0)","v":10.6488},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ160*AA160*(Z160-MIN(Y160,AN160))/10^3),0)","v":90.331200000000038},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.34000000000000008},0.30600000000000011,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ160+$W$78*AQ160^2+$W$79*AQ160^3) ),0),0)","v":6.2131425069282855},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR160+$Y$78*AR160^2+$Y$79*AR160^3),0),0),0)","v":1.4960622442034524},15.973199999999999,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":10.129054886515512},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":4095.7117446631978},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":37.583999999999996},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":8637.7427999999982},610.59906000000024]
[null,null,58,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C161,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":297},{"$f":"'CTZ2'!Q59-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":248},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.28000000000000003},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C161>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},60,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG161*(AD161-Y161)/12000),0),0)","v":12.015000000000004},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG161*AA161*(Z161-MIN(Y161,AD161))/10^3),0)","v":121.11120000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.44500000000000006},0.40050000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG161+$W$78*AG161^2+$W$79*AG161^3) ),0),0)","v":7.9245962290513763},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH161+$Y$78*AH161^2+$Y$79*AH161^3),0),0),0)","v":1.8531838689629616},18.022500000000008,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C161>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},60,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ161*(AN161-Y161)/12000),0),0)","v":8.9100000000000037},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ161*AA161*(Z161-MIN(Y161,AN161))/10^3),0)","v":89.812800000000038},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.33000000000000007},0.2970000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ161+$W$78*AQ161^2+$W$79*AQ161^3) ),0),0)","v":6.0754206889567763},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR161+$Y$78*AR161^2+$Y$79*AR161^3),0),0),0)","v":1.4664680424184835},13.365000000000006,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.7777800980143379},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":4774.3890944913228},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":31.387500000000014},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":8667.2025000000031},728.04501000000027]
[null,null,57,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C162,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":234},{"$f":"'CTZ2'!Q60-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":230},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.28666666666666674},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C162>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},59.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG162*(AD162-Y162)/12000),0),0)","v":9.7524000000000086},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG162*AA162*(Z162-MIN(Y162,AD162))/10^3),0)","v":119.81520000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.43000000000000005},0.38700000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG162+$W$78*AG162^2+$W$79*AG162^3) ),0),0)","v":7.6459269474890377},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH162+$Y$78*AH162^2+$Y$79*AH162^3),0),0),0)","v":1.7961274104270917},14.628600000000013,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C162>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},59.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ162*(AN162-Y162)/12000),0),0)","v":7.2576000000000072},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ162*AA162*(Z162-MIN(Y162,AN162))/10^3),0)","v":89.164800000000042},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.32000000000000006},0.28800000000000009,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ162+$W$78*AQ162^2+$W$79*AQ162^3) ),0),0)","v":5.9412597398605538},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR162+$Y$78*AR162^2+$Y$79*AR162^3),0),0),0)","v":1.4374840324211327},10.886400000000011,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.4420543579161293},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":3906.5517873771623},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":25.515000000000022},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":5926.9644000000062},606.80826000000025]
[null,null,56,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C163,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":264},{"$f":"'CTZ2'!Q61-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":254},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.29333333333333339},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C163>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},58.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG163*(AD163-Y163)/12000),0),0)","v":7.6194000000000139},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG163*AA163*(Z163-MIN(Y163,AD163))/10^3),0)","v":118.32480000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.41500000000000004},0.37350000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG163+$W$78*AG163^2+$W$79*AG163^3) ),0),0)","v":7.3797762999091709},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH163+$Y$78*AH163^2+$Y$79*AH163^3),0),0),0)","v":1.7412973451928302},11.429100000000021,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C163>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},58.400000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ163*(AN163-Y163)/12000),0),0)","v":5.6916000000000118},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ163*AA163*(Z163-MIN(Y163,AN163))/10^3),0)","v":88.387200000000036},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.31000000000000005},0.27900000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ163+$W$78*AQ163^2+$W$79*AQ163^3) ),0),0)","v":5.8104593627945942},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR163+$Y$78*AR163^2+$Y$79*AR163^3),0),0),0)","v":1.4090722825767572},8.5374000000000176,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.1210736451020011},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":4241.7244802312516},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":19.966500000000039},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":5185.7820000000102},671.10120000000006]
[null,null,55,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C164,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":214},{"$f":"'CTZ2'!Q62-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":247},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.30000000000000004},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C164>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},57.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG164*(AD164-Y164)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG164*AA164*(Z164-MIN(Y164,AD164))/10^3),0)","v":116.64000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.40000000000000013},0.36000000000000015,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG164+$W$78*AG164^2+$W$79*AG164^3) ),0),0)","v":7.1254682844598189},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH164+$Y$78*AH164^2+$Y$79*AH164^3),0),0),0)","v":1.6885656539932581},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C164>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},57.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ164*(AN164-Y164)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ164*AA164*(Z164-MIN(Y164,AN164))/10^3),0)","v":87.480000000000032},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},0.27000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ164+$W$78*AQ164^2+$W$79*AQ164^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR164+$Y$78*AR164^2+$Y$79*AR164^3),0),0),0)","v":1.3811948612507141},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530773},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":3631.0147510036104},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},582.10650000000032]
[null,null,54,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C165,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":187},{"$f":"'CTZ2'!Q63-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":241},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.3066666666666667},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C165>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},56.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG165*(AD165-Y165)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG165*AA165*(Z165-MIN(Y165,AD165))/10^3),0)","v":119.23200000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.40000000000000013},0.36000000000000015,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG165+$W$78*AG165^2+$W$79*AG165^3) ),0),0)","v":7.1254682844598189},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH165+$Y$78*AH165^2+$Y$79*AH165^3),0),0),0)","v":1.6885656539932581},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C165>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},56.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ165*(AN165-Y165)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ165*AA165*(Z165-MIN(Y165,AN165))/10^3),0)","v":89.424000000000035},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},0.27000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ165+$W$78*AQ165^2+$W$79*AQ165^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR165+$Y$78*AR165^2+$Y$79*AR165^3),0),0),0)","v":1.3811948612507141},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530773},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":3350.6517499323895},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},548.09460000000013]
[null,null,53,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C166,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":185},{"$f":"'CTZ2'!Q64-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":234},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.31333333333333341},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C166>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},56,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG166*(AD166-Y166)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG166*AA166*(Z166-MIN(Y166,AD166))/10^3),0)","v":121.82400000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.40000000000000013},0.36000000000000015,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG166+$W$78*AG166^2+$W$79*AG166^3) ),0),0)","v":7.1254682844598189},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH166+$Y$78*AH166^2+$Y$79*AH166^3),0),0),0)","v":1.6885656539932581},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C166>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},56,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ166*(AN166-Y166)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ166*AA166*(Z166-MIN(Y166,AN166))/10^3),0)","v":91.368000000000038},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},0.27000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ166+$W$78*AQ166^2+$W$79*AQ166^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR166+$Y$78*AR166^2+$Y$79*AR166^3),0),0),0)","v":1.3811948612507141},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530773},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":3283.5755832003315},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},548.96940000000018]
[null,null,52,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C167,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":152},{"$f":"'CTZ2'!Q65-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":206},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.32000000000000006},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C167>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.8},55.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG167*(AD167-Y167)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG167*AA167*(Z167-MIN(Y167,AD167))/10^3),0)","v":124.41600000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.40000000000000013},0.36000000000000015,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG167+$W$78*AG167^2+$W$79*AG167^3) ),0),0)","v":7.1254682844598189},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH167+$Y$78*AH167^2+$Y$79*AH167^3),0),0),0)","v":1.6885656539932581},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C167>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.8},55.2,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ167*(AN167-Y167)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ167*AA167*(Z167-MIN(Y167,AN167))/10^3),0)","v":93.312000000000026},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},0.27000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ167+$W$78*AQ167^2+$W$79*AQ167^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR167+$Y$78*AR167^2+$Y$79*AR167^3),0),0),0)","v":1.3811948612507141},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530773},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2794.9200678107718},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},476.66880000000015]
[null,null,51,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C168,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":160},{"$f":"'CTZ2'!Q66-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":196},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.32666666666666672},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C168>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.76470588235294112},{"$f":"AB168*(1-AC168)+C168*AC168","v":55},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG168*(AD168-Y168)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG168*AA168*(Z168-MIN(Y168,AD168))/10^3),0)","v":127.00800000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.40000000000000013},{"$f":"AG168*$C$94","v":0.36000000000000015},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG168+$W$78*AG168^2+$W$79*AG168^3) ),0),0)","v":7.1254682844598189},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH168+$Y$78*AH168^2+$Y$79*AH168^3),0),0),0)","v":1.6885656539932581},{"$f":"IF(D168>0,$C$82*AE168,0)+IFERROR(IF($C$83=\"Electric\",IF(D168>0,(AF168)/$C$85,0),0),0)","v":0},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C168>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.76470588235294112},{"$f":"AL168*(1-AM168)+C168*AM168","v":55},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ168*(AN168-Y168)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ168*AA168*(Z168-MIN(Y168,AN168))/10^3),0)","v":95.256000000000029},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},{"$f":"AQ168*$C$94","v":0.27000000000000007},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ168+$W$78*AQ168^2+$W$79*AQ168^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR168+$Y$78*AR168^2+$Y$79*AR168^3),0),0),0)","v":1.3811948612507141},{"$f":"IF(E168>0,$C$82*AO168,0)+IFERROR(IF($C$83=\"Electric\",IF(E168>0,(AF168)/$C$85,0),0),0)","v":0},{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530773},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":2794.7921980967503},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},{"$f":"IF($C$83=\"Gas\",(AF168/100/$C$84*D168)+(AP168/100/$C$84*E168),0)","v":487.39320000000015}]
[null,null,50,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C169,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":98},{"$f":"'CTZ2'!Q67-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":147},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.33333333333333337},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C169>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.72222222222222221},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG169*(AD169-Y169)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG169*AA169*(Z169-MIN(Y169,AD169))/10^3),0)","v":129.60000000000008},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.40000000000000013},0.36000000000000015,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG169+$W$78*AG169^2+$W$79*AG169^3) ),0),0)","v":7.1254682844598189},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH169+$Y$78*AH169^2+$Y$79*AH169^3),0),0),0)","v":1.6885656539932581},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C169>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.72222222222222221},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ169*(AN169-Y169)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ169*AA169*(Z169-MIN(Y169,AN169))/10^3),0)","v":97.200000000000031},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},0.27000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ169+$W$78*AQ169^2+$W$79*AQ169^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR169+$Y$78*AR169^2+$Y$79*AR169^3),0),0),0)","v":1.3811948612507141},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530773},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1902.1854019265952},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},337.36500000000012]
[null,null,49,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C170,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":106},{"$f":"'CTZ2'!Q68-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":160},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.34000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C170>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.68421052631578949},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG170*(AD170-Y170)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG170*AA170*(Z170-MIN(Y170,AD170))/10^3),0)","v":102.44880000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.31000000000000005},0.27900000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG170+$W$78*AG170^2+$W$79*AG170^3) ),0),0)","v":5.8104593627945942},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH170+$Y$78*AH170^2+$Y$79*AH170^3),0),0),0)","v":1.4090722825767572},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C170>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.68421052631578949},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ170*(AN170-Y170)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ170*AA170*(Z170-MIN(Y170,AN170))/10^3),0)","v":69.400800000000061},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.21000000000000008},0.18900000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ170+$W$78*AQ170^2+$W$79*AQ170^3) ),0),0)","v":4.6432217478937527},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR170+$Y$78*AR170^2+$Y$79*AR170^3),0),0),0)","v":1.1480841329251767},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":7.2195316453713509},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1691.8792953403918},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},274.54626000000019]
[null,null,48,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C171,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":86},{"$f":"'CTZ2'!Q69-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":113},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.34666666666666673},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C171>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.65},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG171*(AD171-Y171)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG171*AA171*(Z171-MIN(Y171,AD171))/10^3),0)","v":107.82720000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.32000000000000006},0.28800000000000009,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG171+$W$78*AG171^2+$W$79*AG171^3) ),0),0)","v":5.9412597398605538},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH171+$Y$78*AH171^2+$Y$79*AH171^3),0),0),0)","v":1.4374840324211327},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C171>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.65},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ171*(AN171-Y171)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ171*AA171*(Z171-MIN(Y171,AN171))/10^3),0)","v":74.131200000000049},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.22000000000000008},0.19800000000000009,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ171+$W$78*AQ171^2+$W$79*AQ171^3) ),0),0)","v":4.7514327311335034},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR171+$Y$78*AR171^2+$Y$79*AR171^3),0),0),0)","v":1.1728595211451658},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":7.3787437722816867},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1304.0169889237145},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},220.62456000000012]
[null,null,47,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C172,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":80},{"$f":"'CTZ2'!Q70-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":120},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.35333333333333339},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C172>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.61904761904761907},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG172*(AD172-Y172)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG172*AA172*(Z172-MIN(Y172,AD172))/10^3),0)","v":113.33520000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.33000000000000007},0.2970000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG172+$W$78*AG172^2+$W$79*AG172^3) ),0),0)","v":6.0754206889567763},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH172+$Y$78*AH172^2+$Y$79*AH172^3),0),0),0)","v":1.4664680424184835},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C172>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.61904761904761907},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ172*(AN172-Y172)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ172*AA172*(Z172-MIN(Y172,AN172))/10^3),0)","v":78.991200000000049},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.23000000000000009},0.2070000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ172+$W$78*AQ172^2+$W$79*AQ172^3) ),0),0)","v":4.8610013179532601},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR172+$Y$78*AR172^2+$Y$79*AR172^3),0),0),0)","v":1.1978278531716997},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":7.5418887313752601},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":1330.4105990450162},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},231.82200000000012]
[null,null,46,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C173,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":64},{"$f":"'CTZ2'!Q71-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":79},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.36000000000000004},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C173>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.59090909090909094},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG173*(AD173-Y173)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG173*AA173*(Z173-MIN(Y173,AD173))/10^3),0)","v":118.97280000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.34000000000000008},0.30600000000000011,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG173+$W$78*AG173^2+$W$79*AG173^3) ),0),0)","v":6.2131425069282855},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH173+$Y$78*AH173^2+$Y$79*AH173^3),0),0),0)","v":1.4960622442034524},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C173>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.59090909090909094},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ173*(AN173-Y173)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ173*AA173*(Z173-MIN(Y173,AN173))/10^3),0)","v":83.980800000000059},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.2400000000000001},0.21600000000000011,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ173+$W$78*AQ173^2+$W$79*AQ173^3) ),0),0)","v":4.9721278051980491},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR173+$Y$78*AR173^2+$Y$79*AR173^3),0),0),0)","v":1.2230270606394218},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":7.7092047511317379},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":982.80633847359138},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},178.1092800000001]
[null,null,45,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C174,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":54},{"$f":"'CTZ2'!Q72-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":63},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.3666666666666667},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C174>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.56521739130434778},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG174*(AD174-Y174)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG174*AA174*(Z174-MIN(Y174,AD174))/10^3),0)","v":124.74000000000002},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.35000000000000003},0.31500000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG174+$W$78*AG174^2+$W$79*AG174^3) ),0),0)","v":6.3546254906201094},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH174+$Y$78*AH174^2+$Y$79*AH174^3),0),0),0)","v":1.5263045694106823},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C174>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.56521739130434778},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ174*(AN174-Y174)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ174*AA174*(Z174-MIN(Y174,AN174))/10^3),0)","v":89.100000000000037},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.25000000000000006},0.22500000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ174+$W$78*AQ174^2+$W$79*AQ174^3) ),0),0)","v":5.0850124897128923},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR174+$Y$78*AR174^2+$Y$79*AR174^3),0),0),0)","v":1.2484950751829753},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":7.8809300600307921},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":824.58119983010249},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},154.36575000000005]
[null,null,44,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C175,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":46},{"$f":"'CTZ2'!Q73-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":63},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.37333333333333341},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C175>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.54166666666666663},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG175*(AD175-Y175)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG175*AA175*(Z175-MIN(Y175,AD175))/10^3),0)","v":130.63680000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.36000000000000004},0.32400000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG175+$W$78*AG175^2+$W$79*AG175^3) ),0),0)","v":6.5000699368772699},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH175+$Y$78*AH175^2+$Y$79*AH175^3),0),0),0)","v":1.557232949674817},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C175>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.54166666666666663},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ175*(AN175-Y175)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ175*AA175*(Z175-MIN(Y175,AN175))/10^3),0)","v":94.348800000000068},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.26000000000000006},0.23400000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ175+$W$78*AQ175^2+$W$79*AQ175^3) ),0),0)","v":5.1998556683428205},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR175+$Y$78*AR175^2+$Y$79*AR175^3),0),0),0)","v":1.2742698284370026},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.0573028865520868},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":778.50583907852479},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},149.41584000000006]
[null,null,43,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C176,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":28},{"$f":"'CTZ2'!Q74-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":53},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.38000000000000006},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C176>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.52},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG176*(AD176-Y176)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG176*AA176*(Z176-MIN(Y176,AD176))/10^3),0)","v":136.66320000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.37000000000000005},0.33300000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG176+$W$78*AG176^2+$W$79*AG176^3) ),0),0)","v":6.6496761425447968},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH176+$Y$78*AH176^2+$Y$79*AH176^3),0),0),0)","v":1.5888853166304986},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C176>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.52},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ176*(AN176-Y176)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ176*AA176*(Z176-MIN(Y176,AN176))/10^3),0)","v":99.727200000000053},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.27000000000000007},0.24300000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ176+$W$78*AQ176^2+$W$79*AQ176^3) ),0),0)","v":5.3168576379328565},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR176+$Y$78*AR176^2+$Y$79*AR176^3),0),0),0)","v":1.3003892520361475},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.2385614591752958},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":581.39380602526546},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},113.90139000000005]
[null,null,42,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C177,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":40},{"$f":"'CTZ2'!Q75-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":31},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.38666666666666671},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C177>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.5},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG177*(AD177-Y177)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG177*AA177*(Z177-MIN(Y177,AD177))/10^3),0)","v":142.81920000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.38},0.34200000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG177+$W$78*AG177^2+$W$79*AG177^3) ),0),0)","v":6.8036444044677138},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH177+$Y$78*AH177^2+$Y$79*AH177^3),0),0),0)","v":1.6212996019123704},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C177>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.5},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ177*(AN177-Y177)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ177*AA177*(Z177-MIN(Y177,AN177))/10^3),0)","v":105.23520000000002},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.28000000000000003},0.25200000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ177+$W$78*AQ177^2+$W$79*AQ177^3) ),0),0)","v":5.4362186953280265},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR177+$Y$78*AR177^2+$Y$79*AR177^3),0),0),0)","v":1.3268912776150521},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.424944006380084},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":546.65416941643889},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},112.18824000000004]
[null,null,41,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C178,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":17},{"$f":"'CTZ2'!Q76-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":22},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.39333333333333337},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C178>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.48148148148148145},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG178*(AD178-Y178)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG178*AA178*(Z178-MIN(Y178,AD178))/10^3),0)","v":149.10480000000001},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.39},0.35100000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG178+$W$78*AG178^2+$W$79*AG178^3) ),0),0)","v":6.9621750194910454},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH178+$Y$78*AH178^2+$Y$79*AH178^3),0),0),0)","v":1.6545137371550758},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C178>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.48148148148148145},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ178*(AN178-Y178)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ178*AA178*(Z178-MIN(Y178,AN178))/10^3),0)","v":110.87280000000003},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.29000000000000004},0.26100000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ178+$W$78*AQ178^2+$W$79*AQ178^3) ),0),0)","v":5.5581391373733542},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR178+$Y$78*AR178^2+$Y$79*AR178^3),0),0),0)","v":1.3538138368083603},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.6166887566461217},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":298.54667429498181},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},62.174790000000009]
[null,null,40,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C179,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":28},{"$f":"'CTZ2'!Q77-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":25},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C179>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.4642857142857143},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG179*(AD179-Y179)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG179*AA179*(Z179-MIN(Y179,AD179))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG179+$W$78*AG179^2+$W$79*AG179^3) ),0),0)","v":7.1254682844598172},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH179+$Y$78*AH179^2+$Y$79*AH179^3),0),0),0)","v":1.6885656539932572},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C179>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.4642857142857143},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ179*(AN179-Y179)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ179*AA179*(Z179-MIN(Y179,AN179))/10^3),0)","v":116.64000000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.30000000000000004},0.27000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ179+$W$78*AQ179^2+$W$79*AQ179^3) ),0),0)","v":5.6828192609138677},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR179+$Y$78*AR179^2+$Y$79*AR179^3),0),0),0)","v":1.3811948612507141},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":8.8140339384530737},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":423.39330333080062},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},90.882000000000033]
[null,null,39,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C180,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":16},{"$f":"'CTZ2'!Q78-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":14},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C180>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.44827586206896552},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG180*(AD180-Y180)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG180*AA180*(Z180-MIN(Y180,AD180))/10^3),0)","v":159.40800000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.41000000000000003},0.36900000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG180+$W$78*AG180^2+$W$79*AG180^3) ),0),0)","v":7.2937244962190562},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH180+$Y$78*AH180^2+$Y$79*AH180^3),0),0),0)","v":1.7234932840615584},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C180>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.44827586206896552},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ180*(AN180-Y180)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ180*AA180*(Z180-MIN(Y180,AN180))/10^3),0)","v":120.52800000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.31000000000000005},0.27900000000000008,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ180+$W$78*AQ180^2+$W$79*AQ180^3) ),0),0)","v":5.8104593627945942},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR180+$Y$78*AR180^2+$Y$79*AR180^3),0),0),0)","v":1.4090722825767572},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.0172177802806139},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":245.34892751968874},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},52.974000000000025]
[null,null,38,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C181,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":6},{"$f":"'CTZ2'!Q79-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":15},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C181>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.43333333333333335},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG181*(AD181-Y181)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG181*AA181*(Z181-MIN(Y181,AD181))/10^3),0)","v":163.29600000000008},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.42000000000000004},0.37800000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG181+$W$78*AG181^2+$W$79*AG181^3) ),0),0)","v":7.4671439516137879},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH181+$Y$78*AH181^2+$Y$79*AH181^3),0),0),0)","v":1.7593345589946221},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C181>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.43333333333333335},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ181*(AN181-Y181)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ181*AA181*(Z181-MIN(Y181,AN181))/10^3),0)","v":124.41600000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.32000000000000006},0.28800000000000009,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ181+$W$78*AQ181^2+$W$79*AQ181^3) ),0),0)","v":5.9412597398605538},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR181+$Y$78*AR181^2+$Y$79*AR181^3),0),0),0)","v":1.4374840324211327},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.2264785106084091},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":166.04002764787577},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},35.575200000000017]
[null,null,37,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C182,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":7},{"$f":"'CTZ2'!Q80-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C182>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.41935483870967744},54.999999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG182*(AD182-Y182)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG182*AA182*(Z182-MIN(Y182,AD182))/10^3),0)","v":167.18400000000014},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.43},0.38700000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG182+$W$78*AG182^2+$W$79*AG182^3) ),0),0)","v":7.6459269474890359},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH182+$Y$78*AH182^2+$Y$79*AH182^3),0),0),0)","v":1.7961274104270912},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C182>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.41935483870967744},54.999999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ182*(AN182-Y182)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ182*AA182*(Z182-MIN(Y182,AN182))/10^3),0)","v":128.30400000000012},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.33},0.29700000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ182+$W$78*AQ182^2+$W$79*AQ182^3) ),0),0)","v":6.0754206889567763},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR182+$Y$78*AR182^2+$Y$79*AR182^3),0),0),0)","v":1.4664680424184831},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.4420543579161276},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":111.34571289366444},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},24.251400000000018]
[null,null,36,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C183,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":8},{"$f":"'CTZ2'!Q81-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":4},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C183>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.40625},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG183*(AD183-Y183)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG183*AA183*(Z183-MIN(Y183,AD183))/10^3),0)","v":171.07200000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.44},0.39600000000000002,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG183+$W$78*AG183^2+$W$79*AG183^3) ),0),0)","v":7.8302737806898284},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH183+$Y$78*AH183^2+$Y$79*AH183^3),0),0),0)","v":1.8339097699936084},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C183>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.40625},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ183*(AN183-Y183)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ183*AA183*(Z183-MIN(Y183,AN183))/10^3),0)","v":132.19200000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.34},0.30600000000000005,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ183+$W$78*AQ183^2+$W$79*AQ183^3) ),0),0)","v":6.2131425069282855},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR183+$Y$78*AR183^2+$Y$79*AR183^3),0),0),0)","v":1.4960622442034519},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.6641835506834362},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":108.15028740999443},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},23.71680000000001]
[null,null,35,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C184,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":4},{"$f":"'CTZ2'!Q82-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":6},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C184>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.39393939393939392},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG184*(AD184-Y184)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG184*AA184*(Z184-MIN(Y184,AD184))/10^3),0)","v":174.96000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.45},0.40500000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG184+$W$78*AG184^2+$W$79*AG184^3) ),0),0)","v":8.0203847480611916},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH184+$Y$78*AH184^2+$Y$79*AH184^3),0),0),0)","v":1.8727195693288179},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C184>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.39393939393939392},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ184*(AN184-Y184)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ184*AA184*(Z184-MIN(Y184,AN184))/10^3),0)","v":136.08000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.35000000000000003},0.31500000000000006,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ184+$W$78*AQ184^2+$W$79*AQ184^3) ),0),0)","v":6.3546254906201094},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR184+$Y$78*AR184^2+$Y$79*AR184^3),0),0),0)","v":1.5263045694106823},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":9.8931043173900086},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":86.857997629744787},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},18.954000000000008]
[null,null,34,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C185,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q83-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":3},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C185>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.38235294117647056},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG185*(AD185-Y185)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG185*AA185*(Z185-MIN(Y185,AD185))/10^3),0)","v":178.84800000000004},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.45999999999999996},0.41399999999999998,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG185+$W$78*AG185^2+$W$79*AG185^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH185+$Y$78*AH185^2+$Y$79*AH185^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C185>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.38235294117647056},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ185*(AN185-Y185)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ185*AA185*(Z185-MIN(Y185,AN185))/10^3),0)","v":139.96800000000002},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.36},0.32400000000000001,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ185+$W$78*AQ185^2+$W$79*AQ185^3) ),0),0)","v":6.5000699368772716},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR185+$Y$78*AR185^2+$Y$79*AR185^3),0),0),0)","v":1.5572329496748165},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":24.171908659656268},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},5.248800000000001]
[null,null,33,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C186,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q84-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C186>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.37142857142857144},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG186*(AD186-Y186)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG186*AA186*(Z186-MIN(Y186,AD186))/10^3),0)","v":182.73600000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.47},0.42299999999999999,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG186+$W$78*AG186^2+$W$79*AG186^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH186+$Y$78*AH186^2+$Y$79*AH186^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C186>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.37142857142857144},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ186*(AN186-Y186)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ186*AA186*(Z186-MIN(Y186,AN186))/10^3),0)","v":143.85600000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.37},0.33300000000000002,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ186+$W$78*AQ186^2+$W$79*AQ186^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR186+$Y$78*AR186^2+$Y$79*AR186^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,32,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C187,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q85-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C187>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3611111111111111},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG187*(AD187-Y187)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG187*AA187*(Z187-MIN(Y187,AD187))/10^3),0)","v":186.62400000000005},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.48},0.432,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG187+$W$78*AG187^2+$W$79*AG187^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH187+$Y$78*AH187^2+$Y$79*AH187^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C187>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3611111111111111},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ187*(AN187-Y187)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ187*AA187*(Z187-MIN(Y187,AN187))/10^3),0)","v":147.74400000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.38},0.34200000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ187+$W$78*AQ187^2+$W$79*AQ187^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR187+$Y$78*AR187^2+$Y$79*AR187^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,31,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C188,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q86-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C188>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.35135135135135137},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG188*(AD188-Y188)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG188*AA188*(Z188-MIN(Y188,AD188))/10^3),0)","v":190.51200000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.49},0.441,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG188+$W$78*AG188^2+$W$79*AG188^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH188+$Y$78*AH188^2+$Y$79*AH188^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C188>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.35135135135135137},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ188*(AN188-Y188)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ188*AA188*(Z188-MIN(Y188,AN188))/10^3),0)","v":151.63200000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.39},0.35100000000000003,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ188+$W$78*AQ188^2+$W$79*AQ188^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR188+$Y$78*AR188^2+$Y$79*AR188^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,30,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C189,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q87-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C189>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.34210526315789475},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG189*(AD189-Y189)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG189*AA189*(Z189-MIN(Y189,AD189))/10^3),0)","v":194.40000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG189+$W$78*AG189^2+$W$79*AG189^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH189+$Y$78*AH189^2+$Y$79*AH189^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C189>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.34210526315789475},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ189*(AN189-Y189)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ189*AA189*(Z189-MIN(Y189,AN189))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ189+$W$78*AQ189^2+$W$79*AQ189^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR189+$Y$78*AR189^2+$Y$79*AR189^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,29,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C190,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q88-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C190>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.33333333333333331},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG190*(AD190-Y190)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG190*AA190*(Z190-MIN(Y190,AD190))/10^3),0)","v":194.40000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG190+$W$78*AG190^2+$W$79*AG190^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH190+$Y$78*AH190^2+$Y$79*AH190^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C190>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.33333333333333331},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ190*(AN190-Y190)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ190*AA190*(Z190-MIN(Y190,AN190))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ190+$W$78*AQ190^2+$W$79*AQ190^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR190+$Y$78*AR190^2+$Y$79*AR190^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,28,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C191,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q89-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C191>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.32500000000000001},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG191*(AD191-Y191)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG191*AA191*(Z191-MIN(Y191,AD191))/10^3),0)","v":194.40000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG191+$W$78*AG191^2+$W$79*AG191^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH191+$Y$78*AH191^2+$Y$79*AH191^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C191>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.32500000000000001},55.000000000000007,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ191*(AN191-Y191)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ191*AA191*(Z191-MIN(Y191,AN191))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ191+$W$78*AQ191^2+$W$79*AQ191^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR191+$Y$78*AR191^2+$Y$79*AR191^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,27,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C192,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q90-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C192>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.31707317073170732},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG192*(AD192-Y192)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG192*AA192*(Z192-MIN(Y192,AD192))/10^3),0)","v":194.40000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG192+$W$78*AG192^2+$W$79*AG192^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH192+$Y$78*AH192^2+$Y$79*AH192^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C192>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.31707317073170732},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ192*(AN192-Y192)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ192*AA192*(Z192-MIN(Y192,AN192))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ192+$W$78*AQ192^2+$W$79*AQ192^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR192+$Y$78*AR192^2+$Y$79*AR192^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,26,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C193,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q91-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C193>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.30952380952380953},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG193*(AD193-Y193)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG193*AA193*(Z193-MIN(Y193,AD193))/10^3),0)","v":194.40000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG193+$W$78*AG193^2+$W$79*AG193^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH193+$Y$78*AH193^2+$Y$79*AH193^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C193>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.30952380952380953},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ193*(AN193-Y193)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ193*AA193*(Z193-MIN(Y193,AN193))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ193+$W$78*AQ193^2+$W$79*AQ193^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR193+$Y$78*AR193^2+$Y$79*AR193^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,25,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C194,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C194,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C194,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q92-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C194>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.30232558139534882},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG194*(AD194-Y194)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG194*AA194*(Z194-MIN(Y194,AD194))/10^3),0)","v":194.40000000000006},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG194+$W$78*AG194^2+$W$79*AG194^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH194+$Y$78*AH194^2+$Y$79*AH194^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C194>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.30232558139534882},55,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ194*(AN194-Y194)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ194*AA194*(Z194-MIN(Y194,AN194))/10^3),0)","v":155.52000000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ194+$W$78*AQ194^2+$W$79*AQ194^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR194+$Y$78*AR194^2+$Y$79*AR194^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,24,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C195,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C195,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C195,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q93-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C195>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},54.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG195*(AD195-Y195)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG195*AA195*(Z195-MIN(Y195,AD195))/10^3),0)","v":196.99200000000008},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG195+$W$78*AG195^2+$W$79*AG195^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH195+$Y$78*AH195^2+$Y$79*AH195^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C195>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},54.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ195*(AN195-Y195)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ195*AA195*(Z195-MIN(Y195,AN195))/10^3),0)","v":157.59360000000009},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ195+$W$78*AQ195^2+$W$79*AQ195^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR195+$Y$78*AR195^2+$Y$79*AR195^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,23,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C196,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C196,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C196,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q94-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C196>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},54.499999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG196*(AD196-Y196)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG196*AA196*(Z196-MIN(Y196,AD196))/10^3),0)","v":200.88000000000014},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG196+$W$78*AG196^2+$W$79*AG196^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH196+$Y$78*AH196^2+$Y$79*AH196^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C196>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},54.499999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ196*(AN196-Y196)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ196*AA196*(Z196-MIN(Y196,AN196))/10^3),0)","v":160.70400000000012},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ196+$W$78*AQ196^2+$W$79*AQ196^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR196+$Y$78*AR196^2+$Y$79*AR196^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,22,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C197,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C197,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C197,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q95-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C197>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},54.199999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG197*(AD197-Y197)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG197*AA197*(Z197-MIN(Y197,AD197))/10^3),0)","v":204.76800000000011},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG197+$W$78*AG197^2+$W$79*AG197^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH197+$Y$78*AH197^2+$Y$79*AH197^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C197>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},54.199999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ197*(AN197-Y197)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ197*AA197*(Z197-MIN(Y197,AN197))/10^3),0)","v":163.81440000000012},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ197+$W$78*AQ197^2+$W$79*AQ197^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR197+$Y$78*AR197^2+$Y$79*AR197^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,21,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C198,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C198,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C198,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q96-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C198>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},53.899999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG198*(AD198-Y198)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG198*AA198*(Z198-MIN(Y198,AD198))/10^3),0)","v":208.65600000000018},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG198+$W$78*AG198^2+$W$79*AG198^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH198+$Y$78*AH198^2+$Y$79*AH198^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C198>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},53.899999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ198*(AN198-Y198)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ198*AA198*(Z198-MIN(Y198,AN198))/10^3),0)","v":166.92480000000015},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ198+$W$78*AQ198^2+$W$79*AQ198^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR198+$Y$78*AR198^2+$Y$79*AR198^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,20,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C199,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C199,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C199,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q97-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C199>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},53.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG199*(AD199-Y199)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG199*AA199*(Z199-MIN(Y199,AD199))/10^3),0)","v":212.54400000000015},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG199+$W$78*AG199^2+$W$79*AG199^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH199+$Y$78*AH199^2+$Y$79*AH199^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C199>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},53.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ199*(AN199-Y199)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ199*AA199*(Z199-MIN(Y199,AN199))/10^3),0)","v":170.03520000000012},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ199+$W$78*AQ199^2+$W$79*AQ199^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR199+$Y$78*AR199^2+$Y$79*AR199^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,19,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C200,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C200,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C200,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q98-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C200>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},{"$f":"AB200*(1-AC200)+C200*AC200","v":53.3},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG200*(AD200-Y200)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG200*AA200*(Z200-MIN(Y200,AD200))/10^3),0)","v":216.43200000000007},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},{"$f":"AG200*$C$94","v":0.45},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG200+$W$78*AG200^2+$W$79*AG200^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH200+$Y$78*AH200^2+$Y$79*AH200^3),0),0),0)","v":0},{"$f":"IF(D200>0,$C$82*AE200,0)+IFERROR(IF($C$83=\"Electric\",IF(D200>0,(AF200)/$C$85,0),0),0)","v":0},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C200>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},{"$f":"AL200*(1-AM200)+C200*AM200","v":53.3},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ200*(AN200-Y200)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ200*AA200*(Z200-MIN(Y200,AN200))/10^3),0)","v":173.14560000000009},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},{"$f":"AQ200*$C$94","v":0.36000000000000004},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ200+$W$78*AQ200^2+$W$79*AQ200^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR200+$Y$78*AR200^2+$Y$79*AR200^3),0),0),0)","v":0},{"$f":"IF(E200>0,$C$82*AO200,0)+IFERROR(IF($C$83=\"Electric\",IF(E200>0,(AF200)/$C$85,0),0),0)","v":0},{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},{"$f":"IF($C$83=\"Gas\",(AF200/100/$C$84*D200)+(AP200/100/$C$84*E200),0)","v":0}]
[null,null,18,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C201,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C201,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C201,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q99-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C201>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},52.999999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG201*(AD201-Y201)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG201*AA201*(Z201-MIN(Y201,AD201))/10^3),0)","v":220.32000000000014},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG201+$W$78*AG201^2+$W$79*AG201^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH201+$Y$78*AH201^2+$Y$79*AH201^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C201>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},52.999999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ201*(AN201-Y201)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ201*AA201*(Z201-MIN(Y201,AN201))/10^3),0)","v":176.25600000000014},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ201+$W$78*AQ201^2+$W$79*AQ201^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR201+$Y$78*AR201^2+$Y$79*AR201^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,17,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C202,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C202,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C202,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q100-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C202>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},52.699999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG202*(AD202-Y202)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG202*AA202*(Z202-MIN(Y202,AD202))/10^3),0)","v":224.20800000000011},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG202+$W$78*AG202^2+$W$79*AG202^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH202+$Y$78*AH202^2+$Y$79*AH202^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C202>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},52.699999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ202*(AN202-Y202)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ202*AA202*(Z202-MIN(Y202,AN202))/10^3),0)","v":179.36640000000011},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ202+$W$78*AQ202^2+$W$79*AQ202^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR202+$Y$78*AR202^2+$Y$79*AR202^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,16,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C203,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C203,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C203,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q101-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C203>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},52.399999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG203*(AD203-Y203)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG203*AA203*(Z203-MIN(Y203,AD203))/10^3),0)","v":228.09600000000017},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG203+$W$78*AG203^2+$W$79*AG203^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH203+$Y$78*AH203^2+$Y$79*AH203^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C203>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},52.399999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ203*(AN203-Y203)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ203*AA203*(Z203-MIN(Y203,AN203))/10^3),0)","v":182.47680000000017},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ203+$W$78*AQ203^2+$W$79*AQ203^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR203+$Y$78*AR203^2+$Y$79*AR203^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,15,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C204,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C204,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C204,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q102-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C204>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},52.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG204*(AD204-Y204)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG204*AA204*(Z204-MIN(Y204,AD204))/10^3),0)","v":231.98400000000015},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG204+$W$78*AG204^2+$W$79*AG204^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH204+$Y$78*AH204^2+$Y$79*AH204^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C204>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},52.099999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ204*(AN204-Y204)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ204*AA204*(Z204-MIN(Y204,AN204))/10^3),0)","v":185.58720000000014},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ204+$W$78*AQ204^2+$W$79*AQ204^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR204+$Y$78*AR204^2+$Y$79*AR204^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,14,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C205,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C205,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C205,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q103-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C205>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},51.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG205*(AD205-Y205)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG205*AA205*(Z205-MIN(Y205,AD205))/10^3),0)","v":235.87200000000013},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG205+$W$78*AG205^2+$W$79*AG205^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH205+$Y$78*AH205^2+$Y$79*AH205^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C205>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},51.8,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ205*(AN205-Y205)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ205*AA205*(Z205-MIN(Y205,AN205))/10^3),0)","v":188.69760000000008},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ205+$W$78*AQ205^2+$W$79*AQ205^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR205+$Y$78*AR205^2+$Y$79*AR205^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,13,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C206,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C206,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C206,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q104-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C206>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},51.499999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG206*(AD206-Y206)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG206*AA206*(Z206-MIN(Y206,AD206))/10^3),0)","v":239.76000000000013},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG206+$W$78*AG206^2+$W$79*AG206^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH206+$Y$78*AH206^2+$Y$79*AH206^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C206>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},51.499999999999993,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ206*(AN206-Y206)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ206*AA206*(Z206-MIN(Y206,AN206))/10^3),0)","v":191.80800000000013},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ206+$W$78*AQ206^2+$W$79*AQ206^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR206+$Y$78*AR206^2+$Y$79*AR206^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,12,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C207,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C207,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C207,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q105-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C207>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},51.199999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG207*(AD207-Y207)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG207*AA207*(Z207-MIN(Y207,AD207))/10^3),0)","v":243.64800000000011},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG207+$W$78*AG207^2+$W$79*AG207^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH207+$Y$78*AH207^2+$Y$79*AH207^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C207>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},51.199999999999996,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ207*(AN207-Y207)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ207*AA207*(Z207-MIN(Y207,AN207))/10^3),0)","v":194.9184000000001},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ207+$W$78*AQ207^2+$W$79*AQ207^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR207+$Y$78*AR207^2+$Y$79*AR207^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,11,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C208,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C208,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C208,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q106-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C208>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},50.899999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG208*(AD208-Y208)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG208*AA208*(Z208-MIN(Y208,AD208))/10^3),0)","v":247.53600000000017},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG208+$W$78*AG208^2+$W$79*AG208^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH208+$Y$78*AH208^2+$Y$79*AH208^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C208>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},50.899999999999991,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ208*(AN208-Y208)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ208*AA208*(Z208-MIN(Y208,AN208))/10^3),0)","v":198.02880000000016},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ208+$W$78*AQ208^2+$W$79*AQ208^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR208+$Y$78*AR208^2+$Y$79*AR208^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]
[null,null,10,{"$f":"SUM(\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C209,tbl_Climate_Zone[Weekday],$J$83,tbl_Climate_Zone[Hour],\">\"&$H$83,tbl_Climate_Zone[Hour],\"<=\"&$I$83),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C209,tbl_Climate_Zone[Weekday],$J$84,tbl_Climate_Zone[Hour],\">\"&$H$84,tbl_Climate_Zone[Hour],\"<=\"&$I$84),\nCOUNTIFS(tbl_Climate_Zone[Dry_Bulb],C209,tbl_Climate_Zone[Weekday],$J$85,tbl_Climate_Zone[Hour],\">\"&$H$85,tbl_Climate_Zone[Hour],\"<=\"&$I$85))","v":0},{"$f":"'CTZ2'!Q107-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(IF($C$96=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 1]]),\nFORECAST(MEDIAN($C$44,$D$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$C$43:$D$43,$C$44:$D$44)),0)","v":55},{"$f":"IF($J$40 = \"Disable\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],IFERROR(IF($C$96=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[SAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F])),\nFORECAST(MEDIAN($H$44,$I$44,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$43:$I$43,$H$44:$I$44)),0))","v":55},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]]","v":0},{"$f":"IFERROR(IF($C$74=\"Baseline\",tbl_HVAC_Airside_Calc_Engine[[#This Row],[Base SAT]],tbl_HVAC_Airside_Calc_Engine[[#This Row],[Proposed SAT]]),0)","v":55},{"$f":"IFERROR(IF($H$94=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 1]]),IF($H$94=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[DAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[DAT °F 2]]),\nFORECAST(MEDIAN($H$96,$I$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]),$H$95:$I$95,$H$96:$I$96))),0)","v":70},{"$f":"IFERROR(MAX(0,MIN(1,IF($H$94=\"Baseline Trend Data\", IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 1]]),\n IF($H$94=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[RH Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[RH Flow % 2]]),\nTREND($H$98:$I$98,$H$96:$I$96,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$H$96,$I$96)))))),0)","v":0.40000000000000008},{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[[ Occ RAT °F 1]],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),IF($L$87=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F 2]]),\nMEDIAN($M$96,$L$96,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C209>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RAT °F]])))),$H$90)))","v":0.3},50.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AG209*(AD209-Y209)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AG209*AA209*(Z209-MIN(Y209,AD209))/10^3),0)","v":251.42400000000015},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Occ SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$92:$M$92,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$89:$M$89,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.5},0.45,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AG209+$W$78*AG209^2+$W$79*AG209^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AH209+$Y$78*AH209^2+$Y$79*AH209^3),0),0),0)","v":0},0,{"$f":"IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[ Occ RAT °F 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[UnOcc RAT °F 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F 2]]),\n\nMEDIAN($M$97,$L$97,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]])))","v":68},{"$f":"IF($H$88=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 1]]),IF($H$88=\"Proposed Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[OA Flow % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[OA Flow % 2]]),\nIFERROR(IF((C209>$H$91),$H$90,MAX($H$90,MIN($I$90,(tbl_HVAC_Airside_Calc_Engine[[#This Row],[SAT]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])/(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]-tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc RAT °F]])))),$H$90)))","v":0.3},50.599999999999994,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]>$C$87,MAX(1.08*$C$89*(AQ209*(AN209-Y209)/12000),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$C$86,(1.08*$C$89*AQ209*AA209*(Z209-MIN(Y209,AN209))/10^3),0)","v":201.13920000000013},{"$f":"MIN(100,IF($C$74=\"Proposed\",1+(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Delta SAT]]*$U$75),1)*MAX(0,MIN(1,IF($L$87=\"Baseline Trend Data\",\nIF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 1],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 1]]),\nIF($L$87=\"Proposed Trend Data\",IF(ISBLANK(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),FORECAST(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],tbl_HVAC_Airside_Calc_Engine[Unocc SF Speed % 2],tbl_HVAC_Airside_Calc_Engine[OAT °F]),tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed % 2]]),\nIF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]<$L$94,TREND($L$93:$M$93,$L$94:$M$94,MEDIAN(tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]],$L$94,$M$94)),TREND($L$90:$M$90,$L$91:$M$91,MEDIAN($M$91,$L$91,tbl_HVAC_Airside_Calc_Engine[[#This Row],[OAT °F]]))))))))","v":0.4},0.36000000000000004,{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$88*0.746/$T$78/IF($C$90=\"VFD\",$U$79,1)*(($W$76+$W$77*AQ209+$W$78*AQ209^2+$W$79*AQ209^3) ),0),0)","v":0},{"$f":"IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF Speed %]]>0,IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]],IF(tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]>0,$C$91*0.746/$T$79/IF($C$93=\"VFD\",$U$79,1)*($Y$76+$Y$77*AR209+$Y$78*AR209^2+$Y$79*AR209^3),0),0),0)","v":0},0,{"$f":"SUM((tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]),(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]]))","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ RF kW]])+tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]*(tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc SF kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc RF kW]])","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]","v":0},{"$f":"tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[Occ Hr]]+tbl_HVAC_Airside_Calc_Engine[[#This Row],[Unocc Load kW]]*tbl_HVAC_Airside_Calc_Engine[[#This Row],[UnOcc Hr]]","v":0},0]

{"sheet":"Engineering Report","index":4,"n_rows":96,"n_cols":15,"rows_kept":96,"cut":false,"hidden":true,"merged":[[87,13,87,14],[47,1,47,2],[34,1,34,2],[39,1,39,2],[43,1,43,2],[51,1,51,2],[48,1,48,2],[71,10,71,12],[73,1,73,2],[73,3,73,4],[79,1,79,3],[79,5,79,6],[71,6,72,6],[71,1,72,2],[71,3,72,4],[71,5,72,5],[6,1,6,10],[9,1,9,10],[13,1,13,10],[20,1,20,2],[29,1,29,2],[71,7,71,9],[87,11,87,12],[95,1,96,2],[95,3,96,4],[95,5,96,6],[95,7,96,9],[87,5,88,5],[87,6,88,6],[87,7,87,8],[87,9,87,10],[97,5,97,6],[97,7,97,9],[89,1,89,2],[89,3,89,4],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[87,1,88,2],[87,3,88,4],[97,1,97,2],[97,3,97,4]]}
[]
[null,"Engineering Report"]
[]
[null,", "]
[]
[null,"Assumptions"]
[]
[]
[null,"Governing Equations"]
[null," \n"]
[]
[]
[null,"Project Notes"]
[null," \nPlease write down any influence documentation or any other relevant project information. "]
[]
[]
[]
[]
[null,"Summary of Systems"]
[null,"Air Side Systems"]
[null,"Input"]
[null,"Equipment Vintage"]
[null,"Supply Fan HP"]
[null,"Supply Fan CFM"]
[null,"Supply Fan Control"]
[null,"Return Fan HP"]
[null,"Return Fan CFM"]
[null,"Return Fan Control"]
[null,"Chilled Water System"]
[null,"Input"]
[null,"Capacity (tons)"]
[null,"Design kW/ton"]
[null,"Design CHWT"]
[null,"Cooling Tower System"]
[null,"Input"]
[null,"Capacity (tons)"]
[null,"Fan HP"]
[null,"Motor Efficiency (%)"]
[null,"Secondary Chilled Water Pump"]
[null,"Input"]
[null,"# on Pumps"]
[null,"Baseline Controls"]
[null,"Condenser Water Pumps"]
[null,"Input"]
[null,"# on Pumps"]
[null,"Baseline Controls"]
[1,"Hot Water System"]
[2,"Input"]
[null,"Capacity (kBtu/h)"]
[null,"Efficiency (%)"]
[null,"Seconday Hot Water Pumps"]
[null,"Input"]
[null,"# on Pumps"]
[null,"Baseline Controls"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Energy Savings"]
[]
[null,"Equipment/System Name",null,"Measure Name",null,"Measure Type","Measure EUL","Savings with Existing Baseline ",null,null,"Savings with Title 24/Code Baseline"]
[null,null,null,null,null,null,null,"Total kW","Total kWh","Therms","Energy Usage\n(kWh)","Peak Demand\n(kW)","Energy Usage\n(Therms)"]
[]
[]
[]
[]
[null,"Financial Analysis"]
[]
[null,"Incentive Rates",null,null,null,"Utility Cost"]
[null,"Basic Non Lighting",null,0.08,null,"$/kWh",{"$error":"#DIV/0!"}]
[null,"Target Non Lighting",null,0.15,null,"$/therm",{"$error":"#DIV/0!"}]
[null,"Peak Demand",null,150]
[null,"Natural Gas",null,1]
[null,"To Code/ISP Electric",null,0.03]
[null,"To Code/ISP Gas",null,0.4]
[]
[null,"Equipment/System Name",null,"Measure Name",null,"Yearly Utility Cost Savings\n($)","Estimated Incentives\n($)","Implementation Cost",null,"Payback",null,"Measure Lifetime ROI",null,"Savings to Investment Ratio (SIR)"]
[null,null,null,null,null,null,null,"Measure Cost","w/ Incentives\n($)","w/o\nIncentives \n(years)","w/ Incentives\n(years)","w/o\nIncentives \n(%)","w/ Incentives\n(%)","w/o\nIncentives ","w/ Incentives"]
[]
[]
[]
[]
[null,"M&V Requirements"]
[]
[null,"Equipment/System Name",null,"Measure Name",null,"M&V Type ",null,"Parameters"]

{"sheet":"Report Look Up Tables","index":5,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":true,"merged":[[5,2,6,2],[5,3,6,3],[5,4,6,4],[5,5,6,5],[5,6,6,6],[5,9,5,11],[7,7,7,8],[8,7,8,8],[9,7,9,8],[11,7,11,8],[10,7,10,8],[5,7,6,8],[12,7,12,8],[13,7,13,8],[22,2,23,2],[22,3,22,4],[22,5,22,6],[22,7,22,8],[48,2,49,2],[48,3,48,4],[48,5,48,6],[48,7,48,8],[36,7,37,8],[38,7,38,8],[39,7,39,8],[40,7,40,8],[41,7,41,8],[42,7,42,8],[36,2,37,2],[36,3,37,3],[36,4,37,4],[36,5,37,5],[36,6,37,6],[61,2,62,2],[61,3,62,3],[61,4,62,4],[61,5,62,5],[61,6,62,6],[61,7,62,8],[63,7,63,8],[64,7,64,8],[65,7,65,8],[66,7,66,8],[67,7,67,8],[78,2,79,2],[78,3,78,4],[78,5,78,6],[78,7,78,8],[68,7,68,8],[69,7,69,8],[70,7,70,8],[71,7,71,8],[72,7,72,8]]}
[]
[]
[]
[null,null,"Air Side Measure - Measure Type - Incentive Cap - EUL"]
[]
[null,null,"Measure Name","Measure Type","Incentives Cap","Measure Cost","EUL","Reference",null,"Incentive Rates"]
[null,null,null,null,null,null,null,null,null,"$/kW","$/kWh","$/Therms"]
[null,null,"Equipment Replacements","N/A",0,"TMC",15,"DEER",null,0,0,0]
[null,null,"Scheduling Optimization","BRO",0.5,"TMC",3,"E-4818 Resolution",null,150,0.08,1]
[null,null,"Economizer Optimization","BRO",0.5,"TMC",3,"E-4818 Resolution",null,150,0.08,1]
[null,null,"Static Pressure Reset","BRO",0.5,"TMC",3,"E-4818 Resolution",null,150,0.08,1]
[null,null,"Supply Air Temperature Reset","BRO",0.5,"TMC",3,"E-4818 Resolution",null,150,0.08,1]
[null,null,"Temperature And Fan Setback","BRO",0.5,"TMC",3,"E-4818 Resolution",null,150,0.08,1]
[null,null,"VAV Flow and Reheat Flow Adjustment","BRO",0.5,"TMC",3,"E-4818 Resolution",null,150,0.08,1]
[null,null,"*TMC = Total Measure Cost, IMC = Incremental Measure Cost"]
[]
[]
[]
[]
[null,null,"AirSide M&V Requirements"]
[]
[]
[null,null,"Measure Name","Definition of small & Big Projects",null,"Small Projects",null,"Big Projects"]
[null,null,null,"kWh","Therms","Type of Documentation","Parameters","Type of Documentation","Parameters"]
[null,null,"Equipment Replacements",75000,7500,"N/A","N/A","N/A","N/A"]
[null,null,"Scheduling Optimization",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Fan Schedule","Minimum Two Weeks Trend Data","Fan On/Off Status or Fan Speed"]
[null,null,"Economizer Optimization",75000,7500,"Spot Measurement/EMS Snapshot/Photo","AHU Diagram and Economizer Control Sequence","Minimum Two Weeks Trend Data","MAT, OAT, RAT, SAT"]
[null,null,"Static Pressure Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","AHU Diagram and SAT Reset Logic","Minimum Two Weeks Trend Data","MAT, OAT, RAT, SAT, SAT-SP"]
[null,null,"Supply Air Temperature Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","AHU Diagram and SP Reset Logic","Minimum Two Weeks Trend Data","OAT or RAT, Fan Speed, SP setpoint and SP"]
[null,null,"Temperature And Fan Setback",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Occ and Unocc Temp Setpoint","Minimum Two Weeks Trend Data","OAT, MAT, RAT, SAT, Fan Speed, DAT"]
[null,null,"VAV Flow and Reheat Flow Adjustment",75000,7500,"Spot Measurement/EMS Snapshot/Photo","VAV Heating and Cooling Flow Setpoint, VAV Control Logic","Minimum Two Weeks Trend Data","OAT, MAT, RAT, SAT, Fan Speed, DAT"]
[]
[]
[]
[null,null,"Hot Water Side Measure - Measure Type - Incentive Cap - EUL"]
[]
[null,null,"Measure Name","Measure Type","Incentives Cap","Measure Cost","EUL","Reference"]
[]
[null,null,"HW Lockout Control","BRO",0,"TMC",3,"DEER"]
[null,null,"Boiler Staging Sequence","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"HW Temp Reset","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"SHWP VFD And Speed Control","AOE",0.5,"TMC",15,"DEER"]
[null,null,"HW Differential Pressure Reset","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"*TMC = Total Measure Cost, IMC = Incremental Measure Cost"]
[]
[null,null,"Hot Water M&V Requirements"]
[]
[]
[null,null,"Measure Name","Definition of small & Big Projects",null,"Small Projects",null,"Big Projects"]
[null,null,null,"kWh","Therms","Type of Documentation","Parameters","Type of Documentation","Parameters"]
[null,null,"HW Lockout Control",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Lockout Outside Air Temperature","Minimum Two Weeks Trend Data","Boiler and HWPs On/Off Status, OAT"]
[null,null,"Boiler Staging Sequence",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Control Logic for Boilers Staging","Minimum Two Weeks Trend Data","Boiler and HWPs On/Off Status, Boiler Load in Btu/h, OAT"]
[null,null,"HW Temp Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","HWST Min and Max Setpoints, HWST Reset Control Logic","Minimum Two Weeks Trend Data"," OAT, HWST Setpoint, HWST, HWRT"]
[null,null,"SHWP VFD And Speed Control",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Amp/Power Measurement, Pumps Status","Minimum Two Weeks Trend Data","OAT, SCHWP Speed"]
[null,null,"HW Differential Pressure Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Pump Status & DP Setpoint (if any)","Minimum Two Weeks Trend Data","OAT, SCHWP Speed, DP Set Point, Actual DP"]
[]
[]
[]
[]
[null,null,"Chilled Water Side Measure - Measure Type - Incentive Cap - EUL"]
[]
[null,null,"Measure Name","Measure Type","Incentives Cap","Measure Cost","EUL","Reference"]
[]
[null,null,"Chiller Replacement (or Load Change)","ER/NR",1,"IMC",20,"DEER"]
[null,null,"Chilled Water Plant Lockout Control","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Chiller Staging Sequence Optimization","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Chilled Water Temperature Reset","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Condenser Water Temperature Reset","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Water Side Economizer Optimization","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Cooling Tower Staging Sequence Optimization","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Secondary Chilled Water Pump VFD","AOE",0.5,"TMC",15,"DEER"]
[null,null,"Chilled Water Differential Pressure Reset","BRO",0.5,"TMC",3,"E-4818 Resolution"]
[null,null,"Condenser Water Pump VFD","AOE",0.5,"TMC",15,"DEER"]
[null,null,"*TMC = Total Measure Cost, IMC = Incremental Measure Cost"]
[]
[null,null,"Chilled Water M&V Requirements"]
[]
[]
[null,null,"Measure Name","Definition of small & Big Projects",null,"Small Projects",null,"Big Projects"]
[null,null,null,"kWh","Therms","Type of Documentation","Parameters","Type of Documentation","Parameters"]
[null,null,"Chiller Replacement (or Load Change)",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Chiller nameplate, as-built or submittals for chiller efficiency","Minimum Two Weeks Trend Data","Cooling load, chiller status, amps or kW, OAT db "]
[null,null,"Chilled Water Plant Lockout Control",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Chilled water plant graphics or control logic showing cooling lockout ","Minimum Two Weeks Trend Data","OAT db, chiller status (amps or kW), cooling load"]
[null,null,"Chiller Staging Sequence Optimization",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Chiller staging sequence","Minimum Two Weeks Trend Data","OAT db, Chiller Status (amps or kW), Cooling Load, PCHWP Status or Speed, CWP Status or Speed, CT Fan Status or Speed (CWP & CT Fan points requirement will depend on sequencing)"]
[null,null,"Chilled Water Temperature Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Chilled water reset control logic and chilled water plant graphic","Minimum Two Weeks Trend Data","OAT db, CHWST, CHWST Set Point, Cooling Load"]
[null,null,"Condenser Water Temperature Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Condenser water reset control logic","Minimum Two Weeks Trend Data","OAT wb, CWST, CWST Set Point, Cooling Load"]
[null,null,"Water Side Economizer Optimization",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Economizer and chiller staging sequence","Minimum Two Weeks Trend Data","OAT db, OAT wb, Water Temperature Entering and Leaving Heat Exchanger, Water Flow (gpm)"]
[null,null,"Cooling Tower Staging Sequence Optimization",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Cooling tower staging sequence","Minimum Two Weeks Trend Data","OAT db, OAT wb, CWP Status or Speed, CT Fan Status or Speed"]
[null,null,"Secondary Chilled Water Pump VFD",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Pump speed and OAT, and minimum pump speed. Photo of VFD.","Minimum Two Weeks Trend Data","OAT, SCHWP Speed"]
[null,null,"Chilled Water Differential Pressure Reset",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Pump speed, OAT, minimum pump speed, differential pressure, and DP reset logic","Minimum Two Weeks Trend Data","OAT, SCHWP Speed, DP, DP Set Point"]
[null,null,"Condenser Water Pump VFD",75000,7500,"Spot Measurement/EMS Snapshot/Photo","Pump speed and OAT, and minimum pump speed.  Photo of VFD.","Minimum Two Weeks Trend Data","OAT, CWP Speed"]

{"sheet":"CTZ2","index":6,"n_rows":140161,"n_cols":21,"rows_kept":4500,"cut":true,"hidden":true,"merged":[],"bounds":{"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0}}
["Climate_Zone","Date","Month","Day","Hour","Weekday","Wet_Bulb","Dry_Bulb",null,"First_Line","Hour","Weekday","Wet_Bulb","Dry_Bulb",null,"Dry_Bulb","Hours",null,null,"Peak Demand for this facility"]
[1,{"$f":"DATE(2009,C2,D2)","v":39814},1,1,1,{"$f":"IF(AND(WEEKDAY(DATE(2009,C2,D2),1)>1,WEEKDAY(DATE(2009,C2,D2))<7),\"Weekday\",IF(WEEKDAY(DATE(2009,C2,D2),1)=1,\"Sunday\",\"Saturday\"))","v":"Weekday"},36,37,null,{"$f":"MATCH(nr_Climate_Zone,tbl_Climate_Zones[Climate_Zone],0)","v":17521},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,115,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,"Climate Zone","Start Date","Average T"]
[1,39814,1,1,2,"Weekday",36,37,null,{"$f":"J2+1","v":17522},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,114,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,{"$f":"nr_Climate_Zone","v":3},{"$f":"INDEX($T$6:$T$21,$S$3)","v":"2017-07-08"},{"$f":"ROUNDDOWN(INDEX($U$6:$U$21,$S$3),0)","v":69}]
[1,39814,1,1,3,"Weekday",36,37,null,{"$f":"J3+1","v":17523},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},null,113,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,null,"Peak Demand DEER Temperatures"]
[1,39814,1,1,4,"Weekday",36,38,null,17524,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},null,112,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,"Climate Zone","Start Date","Average T"]
[1,39814,1,1,5,"Weekday",36,38,null,17525,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},null,111,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,1,"2017-09-16",59.8]
[1,39814,1,1,6,"Weekday",37,39,null,17526,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,110,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,{"$f":"S6+1","v":2},"2017-07-08",75.900000000000006]
[1,39814,1,1,7,"Weekday",37,40,null,17527,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,109,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,{"$f":"S7+1","v":3},"2017-07-08",69.2]
[1,39814,1,1,8,"Weekday",38,41,null,17528,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,108,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,4,"2017-09-01",77.5]
[1,39814,1,1,9,"Weekday",39,42,null,17529,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,107,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,5,"2017-09-08",64.8]
[1,39814,1,1,10,"Weekday",40,43,null,17530,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},null,106,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,6,"2017-09-01",77.099999999999994]
[1,39814,1,1,11,"Weekday",41,44,null,17531,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},null,105,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,7,"2017-09-01",73.900000000000006]
[1,39814,1,1,12,"Weekday",43,46,null,17532,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},null,104,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,8,"2017-09-01",79.8]
[1,39814,1,1,13,"Weekday",45,48,null,17533,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},null,103,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,9,"2017-09-01",86.6]
[1,39814,1,1,14,"Weekday",45,48,null,17534,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},null,102,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,10,"2017-09-01",86.3]
[1,39814,1,1,15,"Weekday",45,48,null,17535,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},null,101,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,11,"2017-07-08",88.3]
[1,39814,1,1,16,"Weekday",45,48,null,17536,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},null,100,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,12,"2017-07-08",82.4]
[1,39814,1,1,17,"Weekday",45,48,null,17537,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},null,99,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,13,"2017-07-08",86.7]
[1,39814,1,1,18,"Weekday",45,48,null,17538,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},null,98,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,14,"2017-08-26",86.8]
[1,39814,1,1,19,"Weekday",45,48,null,17539,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},null,97,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,15,"2017-08-25",97.5]
[1,39814,1,1,20,"Weekday",45,48,null,17540,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,96,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0},null,16,"2017-07-08",78.8]
[1,39814,1,1,21,"Weekday",45,48,null,17541,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,95,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39814,1,1,22,"Weekday",45,48,null,17542,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,94,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39814,1,1,23,"Weekday",45,48,null,17543,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,93,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39814,1,1,24,"Weekday",44,47,null,17544,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,92,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39815,1,2,1,"Weekday",44,47,null,17545,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,91,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":1}]
[1,39815,1,2,2,"Weekday",44,47,null,17546,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,90,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39815,1,2,3,"Weekday",44,47,null,17547,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,89,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":5}]
[1,39815,1,2,4,"Weekday",44,48,null,17548,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,88,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":3}]
[1,39815,1,2,5,"Weekday",45,48,null,17549,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,87,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":5}]
[1,39815,1,2,6,"Weekday",45,48,null,17550,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,86,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":10}]
[1,39815,1,2,7,"Weekday",45,48,null,17551,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":32},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},null,85,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":6}]
[1,39815,1,2,8,"Weekday",45,48,null,17552,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,84,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":8}]
[1,39815,1,2,9,"Weekday",45,48,null,17553,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,83,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":15}]
[1,39815,1,2,10,"Weekday",46,48,null,17554,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,82,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":15}]
[1,39815,1,2,11,"Weekday",46,48,null,17555,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,81,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":10}]
[1,39815,1,2,12,"Weekday",48,49,null,17556,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,80,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":28}]
[1,39815,1,2,13,"Weekday",48,49,null,17557,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,79,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":27}]
[1,39815,1,2,14,"Weekday",49,49,null,17558,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,78,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":33}]
[1,39815,1,2,15,"Weekday",49,50,null,17559,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},null,77,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":20}]
[1,39815,1,2,16,"Weekday",49,50,null,17560,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},null,76,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":50}]
[1,39815,1,2,17,"Weekday",49,50,null,17561,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,75,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":47}]
[1,39815,1,2,18,"Weekday",49,50,null,17562,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},null,74,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":61}]
[1,39815,1,2,19,"Weekday",49,50,null,17563,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,73,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":68}]
[1,39815,1,2,20,"Weekday",49,50,null,17564,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,72,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":80}]
[1,39815,1,2,21,"Weekday",49,49,null,17565,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,71,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":137}]
[1,39815,1,2,22,"Weekday",48,49,null,17566,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,70,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":111}]
[1,39815,1,2,23,"Weekday",48,48,null,17567,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,69,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":135}]
[1,39815,1,2,24,"Weekday",48,48,null,17568,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,68,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":138}]
[1,39816,1,3,1,"Saturday",47,47,null,17569,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,67,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":180}]
[1,39816,1,3,2,"Saturday",47,47,null,17570,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,66,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":165}]
[1,39816,1,3,3,"Saturday",47,48,null,17571,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,65,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":219}]
[1,39816,1,3,4,"Saturday",48,48,null,17572,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},null,64,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":245}]
[1,39816,1,3,5,"Saturday",49,49,null,17573,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},null,63,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":200}]
[1,39816,1,3,6,"Saturday",50,51,null,17574,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},null,62,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":312}]
[1,39816,1,3,7,"Saturday",50,51,null,17575,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},null,61,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":343}]
[1,39816,1,3,8,"Saturday",51,51,null,17576,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},null,60,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":467}]
[1,39816,1,3,9,"Saturday",51,51,null,17577,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},null,59,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":455}]
[1,39816,1,3,10,"Saturday",51,51,null,17578,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},null,58,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":545}]
[1,39816,1,3,11,"Saturday",51,52,null,17579,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,57,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":464}]
[1,39816,1,3,12,"Saturday",51,52,null,17580,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,56,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":518}]
[1,39816,1,3,13,"Saturday",52,53,null,17581,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,55,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":461}]
[1,39816,1,3,14,"Saturday",52,53,null,17582,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,54,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":428}]
[1,39816,1,3,15,"Saturday",52,53,null,17583,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,53,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":419}]
[1,39816,1,3,16,"Saturday",52,53,null,17584,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},null,52,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":358}]
[1,{"$f":"DATE(2009,C66,D66)","v":39816},1,3,17,"Saturday",53,54,null,17585,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},null,51,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":356}]
[1,39816,1,3,18,"Saturday",54,54,null,17586,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,50,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":245}]
[1,39816,1,3,19,"Saturday",55,55,null,{"$f":"J67+1","v":17587},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,49,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":266}]
[1,39816,1,3,20,"Saturday",55,55,null,17588,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,48,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":199}]
[1,39816,1,3,21,"Saturday",55,55,null,17589,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,47,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":200}]
[1,39816,1,3,22,"Saturday",55,55,null,17590,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,46,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":143}]
[1,39816,1,3,23,"Saturday",55,55,null,17591,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,45,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":117}]
[1,39816,1,3,24,"Saturday",55,55,null,17592,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,44,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":109}]
[1,39817,1,4,1,"Sunday",55,55,null,17593,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,43,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":81}]
[1,39817,1,4,2,"Sunday",54,55,null,17594,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,42,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":71}]
[1,39817,1,4,3,"Sunday",54,54,null,17595,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,41,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":39}]
[1,39817,1,4,4,"Sunday",53,53,null,17596,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,40,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":53}]
[1,39817,1,4,5,"Sunday",53,53,null,17597,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,39,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":30}]
[1,39817,1,4,6,"Sunday",52,53,null,17598,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,38,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":21}]
[1,39817,1,4,7,"Sunday",51,52,null,17599,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,37,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":13}]
[1,39817,1,4,8,"Sunday",51,52,null,17600,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,36,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":12}]
[1,39817,1,4,9,"Sunday",51,51,null,17601,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},null,35,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":10}]
[1,39817,1,4,10,"Sunday",51,51,null,17602,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},null,34,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":3}]
[1,39817,1,4,11,"Sunday",51,51,null,17603,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,33,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,12,"Sunday",51,52,null,17604,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,32,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,13,"Sunday",51,52,null,17605,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},null,31,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,14,"Sunday",52,53,null,17606,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},null,30,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,15,"Sunday",52,54,null,17607,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,29,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,16,"Sunday",53,55,null,17608,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,28,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,17,"Sunday",53,54,null,17609,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,27,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,18,"Sunday",53,53,null,17610,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,26,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,19,"Sunday",52,52,null,17611,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,25,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,20,"Sunday",53,53,null,17612,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,24,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,21,"Sunday",53,54,null,17613,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,23,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,22,"Sunday",54,55,null,17614,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,22,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,23,"Sunday",55,55,null,17615,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,21,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39817,1,4,24,"Sunday",55,56,null,17616,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,20,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,1,"Weekday",55,56,null,17617,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,19,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,2,"Weekday",55,56,null,17618,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},null,18,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,3,"Weekday",55,56,null,17619,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},null,17,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,4,"Weekday",55,56,null,17620,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,16,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,5,"Weekday",54,55,null,17621,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,15,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,6,"Weekday",54,55,null,17622,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,14,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,7,"Weekday",54,55,null,17623,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},null,13,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,8,"Weekday",54,56,null,17624,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},null,12,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,9,"Weekday",55,57,null,17625,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},null,11,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,10,"Weekday",56,58,null,17626,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},null,10,{"$f":"COUNTIF(tbl_Climate_Zone[Dry_Bulb],tbl_Bin_Data[[#This Row],[Dry_Bulb]])","v":0}]
[1,39818,1,5,11,"Weekday",57,59,null,17627,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39818,1,5,12,"Weekday",58,59,null,17628,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39818,1,5,13,"Weekday",58,60,null,17629,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39818,1,5,14,"Weekday",58,60,null,17630,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39818,1,5,15,"Weekday",58,60,null,17631,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39818,1,5,16,"Weekday",58,60,null,17632,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,17,"Weekday",58,59,null,17633,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,18,"Weekday",58,59,null,17634,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,19,"Weekday",58,58,null,17635,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,20,"Weekday",57,58,null,17636,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,21,"Weekday",57,58,null,17637,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,22,"Weekday",57,57,null,17638,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39818,1,5,23,"Weekday",56,57,null,17639,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39818,1,5,24,"Weekday",56,57,null,17640,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39819,1,6,1,"Weekday",57,57,null,17641,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39819,1,6,2,"Weekday",57,57,null,17642,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39819,1,6,3,"Weekday",57,57,null,17643,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39819,1,6,4,"Weekday",57,57,null,17644,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39819,1,6,5,"Weekday",57,58,null,17645,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39819,1,6,6,"Weekday",57,58,null,17646,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39819,1,6,7,"Weekday",57,58,null,17647,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39819,1,6,8,"Weekday",58,60,null,17648,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,{"$f":"DATE(2009,C130,D130)","v":39819},1,6,9,"Weekday",59,62,null,17649,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39819,1,6,10,"Weekday",61,63,null,17650,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39819,1,6,11,"Weekday",60,62,null,{"$f":"J131+1","v":17651},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39819,1,6,12,"Weekday",59,62,null,17652,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39819,1,6,13,"Weekday",58,61,null,17653,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39819,1,6,14,"Weekday",58,61,null,17654,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39819,1,6,15,"Weekday",58,61,null,17655,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39819,1,6,16,"Weekday",58,61,null,17656,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39819,1,6,17,"Weekday",58,60,null,17657,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39819,1,6,18,"Weekday",57,59,null,17658,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39819,1,6,19,"Weekday",57,58,null,17659,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39819,1,6,20,"Weekday",55,56,null,17660,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39819,1,6,21,"Weekday",54,55,null,17661,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39819,1,6,22,"Weekday",53,53,null,17662,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39819,1,6,23,"Weekday",52,52,null,17663,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39819,1,6,24,"Weekday",51,51,null,17664,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39820,1,7,1,"Weekday",51,51,null,17665,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39820,1,7,2,"Weekday",50,50,null,17666,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39820,1,7,3,"Weekday",50,50,null,17667,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39820,1,7,4,"Weekday",49,49,null,17668,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38}]
[1,39820,1,7,5,"Weekday",49,50,null,17669,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39820,1,7,6,"Weekday",50,50,null,17670,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39820,1,7,7,"Weekday",51,51,null,17671,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39820,1,7,8,"Weekday",51,52,null,17672,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39820,1,7,9,"Weekday",52,53,null,17673,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39820,1,7,10,"Weekday",52,55,null,17674,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39820,1,7,11,"Weekday",54,55,null,17675,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39820,1,7,12,"Weekday",55,56,null,17676,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39820,1,7,13,"Weekday",56,57,null,17677,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39820,1,7,14,"Weekday",56,57,null,17678,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39820,1,7,15,"Weekday",56,57,null,17679,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39820,1,7,16,"Weekday",56,57,null,17680,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39820,1,7,17,"Weekday",56,56,null,17681,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39820,1,7,18,"Weekday",56,56,null,17682,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39820,1,7,19,"Weekday",55,56,null,17683,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39820,1,7,20,"Weekday",55,56,null,17684,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39820,1,7,21,"Weekday",55,56,null,17685,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39820,1,7,22,"Weekday",55,57,null,17686,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39820,1,7,23,"Weekday",55,57,null,17687,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39820,1,7,24,"Weekday",55,56,null,17688,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39821,1,8,1,"Weekday",54,55,null,17689,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39821,1,8,2,"Weekday",53,54,null,17690,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39821,1,8,3,"Weekday",52,53,null,17691,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38}]
[1,39821,1,8,4,"Weekday",51,52,null,17692,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39821,1,8,5,"Weekday",50,51,null,17693,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39821,1,8,6,"Weekday",48,49,null,17694,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39821,1,8,7,"Weekday",47,47,null,17695,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39821,1,8,8,"Weekday",48,49,null,17696,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39821,1,8,9,"Weekday",50,51,null,17697,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39821,1,8,10,"Weekday",52,52,null,17698,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39821,1,8,11,"Weekday",52,53,null,17699,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39821,1,8,12,"Weekday",52,55,null,17700,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39821,1,8,13,"Weekday",53,56,null,17701,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39821,1,8,14,"Weekday",52,55,null,17702,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39821,1,8,15,"Weekday",52,55,null,17703,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39821,1,8,16,"Weekday",52,55,null,17704,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39821,1,8,17,"Weekday",50,52,null,17705,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39821,1,8,18,"Weekday",47,49,null,17706,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39821,1,8,19,"Weekday",45,46,null,17707,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39821,1,8,20,"Weekday",43,44,null,17708,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39821,1,8,21,"Weekday",41,42,null,17709,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39821,1,8,22,"Weekday",39,39,null,17710,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39821,1,8,23,"Weekday",38,39,null,17711,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39821,1,8,24,"Weekday",39,40,null,17712,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,{"$f":"DATE(2009,C194,D194)","v":39822},1,9,1,"Weekday",40,41,null,17713,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39822,1,9,2,"Weekday",40,40,null,17714,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39822,1,9,3,"Weekday",38,39,null,{"$f":"J195+1","v":17715},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39822,1,9,4,"Weekday",36,37,null,17716,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35}]
[1,39822,1,9,5,"Weekday",37,38,null,17717,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38}]
[1,39822,1,9,6,"Weekday",37,38,null,17718,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39822,1,9,7,"Weekday",38,39,null,17719,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39822,1,9,8,"Weekday",41,42,null,17720,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39822,1,9,9,"Weekday",43,45,null,17721,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39822,1,9,10,"Weekday",46,47,null,17722,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39822,1,9,11,"Weekday",48,50,null,17723,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39822,1,9,12,"Weekday",50,53,null,17724,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39822,1,9,13,"Weekday",52,55,null,17725,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39822,1,9,14,"Weekday",51,54,null,17726,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39822,1,9,15,"Weekday",50,53,null,17727,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39822,1,9,16,"Weekday",50,53,null,17728,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39822,1,9,17,"Weekday",47,49,null,17729,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39822,1,9,18,"Weekday",44,46,null,17730,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39822,1,9,19,"Weekday",41,42,null,17731,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39822,1,9,20,"Weekday",40,41,null,17732,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39822,1,9,21,"Weekday",40,40,null,17733,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39822,1,9,22,"Weekday",39,39,null,17734,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39822,1,9,23,"Weekday",38,38,null,17735,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39822,1,9,24,"Weekday",38,38,null,17736,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39823,1,10,1,"Saturday",38,38,null,17737,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39823,1,10,2,"Saturday",38,38,null,17738,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39823,1,10,3,"Saturday",38,38,null,17739,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39823,1,10,4,"Saturday",38,39,null,17740,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39823,1,10,5,"Saturday",39,39,null,17741,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39823,1,10,6,"Saturday",39,40,null,17742,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39823,1,10,7,"Saturday",39,40,null,17743,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39823,1,10,8,"Saturday",41,42,null,17744,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39823,1,10,9,"Saturday",43,44,null,17745,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39823,1,10,10,"Saturday",44,46,null,17746,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39823,1,10,11,"Saturday",46,49,null,17747,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39823,1,10,12,"Saturday",48,52,null,17748,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39823,1,10,13,"Saturday",50,55,null,17749,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39823,1,10,14,"Saturday",50,53,null,17750,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39823,1,10,15,"Saturday",50,52,null,17751,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39823,1,10,16,"Saturday",49,51,null,17752,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39823,1,10,17,"Saturday",50,51,null,17753,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39823,1,10,18,"Saturday",50,51,null,17754,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39823,1,10,19,"Saturday",50,51,null,17755,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39823,1,10,20,"Saturday",50,50,null,17756,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39823,1,10,21,"Saturday",49,50,null,17757,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39823,1,10,22,"Saturday",49,49,null,17758,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39823,1,10,23,"Saturday",48,49,null,17759,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39823,1,10,24,"Saturday",48,48,null,17760,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39824,1,11,1,"Sunday",47,47,null,17761,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39824,1,11,2,"Sunday",47,47,null,17762,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39824,1,11,3,"Sunday",47,47,null,17763,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39824,1,11,4,"Sunday",47,47,null,17764,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39824,1,11,5,"Sunday",46,46,null,17765,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39824,1,11,6,"Sunday",46,46,null,17766,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39824,1,11,7,"Sunday",45,46,null,17767,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39824,1,11,8,"Sunday",47,47,null,17768,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39824,1,11,9,"Sunday",48,49,null,17769,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39824,1,11,10,"Sunday",50,51,null,17770,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39824,1,11,11,"Sunday",51,53,null,17771,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39824,1,11,12,"Sunday",53,55,null,17772,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39824,1,11,13,"Sunday",54,57,null,17773,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,14,"Sunday",54,56,null,17774,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,15,"Sunday",54,55,null,17775,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,16,"Sunday",53,55,null,17776,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,{"$f":"DATE(2009,C258,D258)","v":39824},1,11,17,"Sunday",51,53,null,17777,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,18,"Sunday",49,51,null,17778,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,19,"Sunday",47,49,null,{"$f":"J259+1","v":17779},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,20,"Sunday",45,47,null,17780,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,21,"Sunday",43,44,null,17781,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,22,"Sunday",40,42,null,17782,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39824,1,11,23,"Sunday",39,41,null,17783,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39824,1,11,24,"Sunday",39,40,null,17784,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39825,1,12,1,"Weekday",39,40,null,17785,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39825,1,12,2,"Weekday",40,40,null,17786,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39825,1,12,3,"Weekday",41,41,null,17787,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39825,1,12,4,"Weekday",41,42,null,17788,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39825,1,12,5,"Weekday",41,42,null,17789,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39825,1,12,6,"Weekday",41,42,null,17790,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39825,1,12,7,"Weekday",41,41,null,17791,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39825,1,12,8,"Weekday",43,44,null,17792,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39825,1,12,9,"Weekday",46,47,null,17793,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39825,1,12,10,"Weekday",48,50,null,17794,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39825,1,12,11,"Weekday",50,53,null,17795,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39825,1,12,12,"Weekday",51,55,null,17796,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39825,1,12,13,"Weekday",53,58,null,17797,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39825,1,12,14,"Weekday",52,58,null,17798,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39825,1,12,15,"Weekday",51,58,null,17799,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39825,1,12,16,"Weekday",50,58,null,17800,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39825,1,12,17,"Weekday",49,55,null,17801,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39825,1,12,18,"Weekday",49,52,null,17802,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39825,1,12,19,"Weekday",48,49,null,17803,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39825,1,12,20,"Weekday",47,48,null,17804,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39825,1,12,21,"Weekday",45,46,null,17805,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39825,1,12,22,"Weekday",44,45,null,17806,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39825,1,12,23,"Weekday",43,44,null,17807,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39825,1,12,24,"Weekday",42,43,null,17808,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39826,1,13,1,"Weekday",41,42,null,17809,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39826,1,13,2,"Weekday",41,41,null,17810,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39826,1,13,3,"Weekday",40,41,null,17811,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39826,1,13,4,"Weekday",40,40,null,17812,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39826,1,13,5,"Weekday",40,40,null,17813,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39826,1,13,6,"Weekday",40,40,null,17814,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39826,1,13,7,"Weekday",40,40,null,17815,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39826,1,13,8,"Weekday",43,44,null,17816,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39826,1,13,9,"Weekday",46,47,null,17817,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39826,1,13,10,"Weekday",50,51,null,17818,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39826,1,13,11,"Weekday",52,54,null,17819,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39826,1,13,12,"Weekday",53,57,null,17820,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39826,1,13,13,"Weekday",55,60,null,17821,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39826,1,13,14,"Weekday",55,58,null,17822,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39826,1,13,15,"Weekday",54,56,null,17823,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39826,1,13,16,"Weekday",54,54,null,17824,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39826,1,13,17,"Weekday",54,54,null,17825,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39826,1,13,18,"Weekday",54,54,null,17826,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39826,1,13,19,"Weekday",54,54,null,17827,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39826,1,13,20,"Weekday",54,54,null,17828,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39826,1,13,21,"Weekday",53,53,null,17829,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39826,1,13,22,"Weekday",52,52,null,17830,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39826,1,13,23,"Weekday",51,51,null,17831,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39826,1,13,24,"Weekday",50,50,null,17832,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39827,1,14,1,"Weekday",49,49,null,17833,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39827,1,14,2,"Weekday",49,49,null,17834,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39827,1,14,3,"Weekday",49,49,null,17835,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39827,1,14,4,"Weekday",49,49,null,17836,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39827,1,14,5,"Weekday",48,49,null,17837,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39827,1,14,6,"Weekday",48,49,null,17838,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39827,1,14,7,"Weekday",48,48,null,17839,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39827,1,14,8,"Weekday",49,50,null,17840,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,{"$f":"DATE(2009,C322,D322)","v":39827},1,14,9,"Weekday",50,51,null,17841,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39827,1,14,10,"Weekday",51,53,null,17842,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39827,1,14,11,"Weekday",52,53,null,{"$f":"J323+1","v":17843},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39827,1,14,12,"Weekday",53,54,null,17844,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39827,1,14,13,"Weekday",55,55,null,17845,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39827,1,14,14,"Weekday",54,55,null,17846,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39827,1,14,15,"Weekday",54,54,null,17847,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39827,1,14,16,"Weekday",54,54,null,17848,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39827,1,14,17,"Weekday",54,54,null,17849,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39827,1,14,18,"Weekday",54,54,null,17850,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39827,1,14,19,"Weekday",54,54,null,17851,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39827,1,14,20,"Weekday",54,54,null,17852,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39827,1,14,21,"Weekday",54,54,null,17853,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39827,1,14,22,"Weekday",54,54,null,17854,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39827,1,14,23,"Weekday",53,54,null,17855,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39827,1,14,24,"Weekday",53,53,null,17856,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39828,1,15,1,"Weekday",52,53,null,17857,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39828,1,15,2,"Weekday",52,53,null,17858,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39828,1,15,3,"Weekday",52,53,null,17859,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39828,1,15,4,"Weekday",52,53,null,17860,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39828,1,15,5,"Weekday",52,53,null,17861,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39828,1,15,6,"Weekday",52,53,null,17862,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39828,1,15,7,"Weekday",52,53,null,17863,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39828,1,15,8,"Weekday",53,54,null,17864,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39828,1,15,9,"Weekday",54,55,null,17865,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39828,1,15,10,"Weekday",55,56,null,17866,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39828,1,15,11,"Weekday",56,57,null,17867,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39828,1,15,12,"Weekday",56,58,null,17868,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39828,1,15,13,"Weekday",57,60,null,17869,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39828,1,15,14,"Weekday",57,59,null,17870,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39828,1,15,15,"Weekday",57,59,null,17871,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39828,1,15,16,"Weekday",56,58,null,17872,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39828,1,15,17,"Weekday",53,55,null,17873,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39828,1,15,18,"Weekday",50,51,null,17874,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39828,1,15,19,"Weekday",47,47,null,17875,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39828,1,15,20,"Weekday",45,46,null,17876,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39828,1,15,21,"Weekday",43,44,null,17877,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39828,1,15,22,"Weekday",41,42,null,17878,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39828,1,15,23,"Weekday",41,42,null,17879,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39828,1,15,24,"Weekday",43,45,null,17880,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39829,1,16,1,"Weekday",45,47,null,17881,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39829,1,16,2,"Weekday",46,48,null,17882,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39829,1,16,3,"Weekday",44,47,null,17883,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39829,1,16,4,"Weekday",43,46,null,17884,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39829,1,16,5,"Weekday",41,43,null,17885,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39829,1,16,6,"Weekday",39,40,null,17886,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39829,1,16,7,"Weekday",37,38,null,17887,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39829,1,16,8,"Weekday",41,43,null,17888,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39829,1,16,9,"Weekday",44,49,null,17889,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39829,1,16,10,"Weekday",48,54,null,17890,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39829,1,16,11,"Weekday",50,59,null,17891,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39829,1,16,12,"Weekday",52,63,null,17892,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39829,1,16,13,"Weekday",55,67,null,17893,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39829,1,16,14,"Weekday",54,66,null,17894,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39829,1,16,15,"Weekday",53,64,null,17895,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39829,1,16,16,"Weekday",53,63,null,17896,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39829,1,16,17,"Weekday",50,59,null,17897,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39829,1,16,18,"Weekday",48,56,null,17898,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39829,1,16,19,"Weekday",46,52,null,17899,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39829,1,16,20,"Weekday",44,49,null,17900,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39829,1,16,21,"Weekday",43,46,null,17901,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39829,1,16,22,"Weekday",41,43,null,17902,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39829,1,16,23,"Weekday",39,42,null,17903,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39829,1,16,24,"Weekday",39,41,null,17904,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,{"$f":"DATE(2009,C386,D386)","v":39830},1,17,1,"Saturday",39,40,null,17905,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39830,1,17,2,"Saturday",38,39,null,17906,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39830,1,17,3,"Saturday",37,38,null,{"$f":"J387+1","v":17907},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39830,1,17,4,"Saturday",36,37,null,17908,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39830,1,17,5,"Saturday",36,36,null,17909,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39830,1,17,6,"Saturday",35,35,null,17910,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39830,1,17,7,"Saturday",34,34,null,17911,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39830,1,17,8,"Saturday",38,39,null,17912,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39830,1,17,9,"Saturday",41,44,null,17913,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39830,1,17,10,"Saturday",44,49,null,17914,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39830,1,17,11,"Saturday",47,52,null,17915,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39830,1,17,12,"Saturday",50,55,null,17916,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39830,1,17,13,"Saturday",54,57,null,17917,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39830,1,17,14,"Saturday",53,57,null,17918,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39830,1,17,15,"Saturday",53,56,null,17919,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39830,1,17,16,"Saturday",52,56,null,17920,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39830,1,17,17,"Saturday",49,51,null,17921,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39830,1,17,18,"Saturday",45,46,null,17922,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39830,1,17,19,"Saturday",41,42,null,17923,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39830,1,17,20,"Saturday",40,41,null,17924,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39830,1,17,21,"Saturday",39,39,null,17925,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39830,1,17,22,"Saturday",38,38,null,17926,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39830,1,17,23,"Saturday",38,38,null,17927,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39830,1,17,24,"Saturday",38,38,null,17928,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39831,1,18,1,"Sunday",38,38,null,17929,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39831,1,18,2,"Sunday",37,37,null,17930,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39831,1,18,3,"Sunday",36,36,null,17931,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39831,1,18,4,"Sunday",35,35,null,17932,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39831,1,18,5,"Sunday",35,35,null,17933,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39831,1,18,6,"Sunday",35,35,null,17934,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39831,1,18,7,"Sunday",35,35,null,17935,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39831,1,18,8,"Sunday",38,39,null,17936,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39831,1,18,9,"Sunday",41,42,null,17937,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39831,1,18,10,"Sunday",44,46,null,17938,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39831,1,18,11,"Sunday",46,49,null,17939,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39831,1,18,12,"Sunday",47,52,null,17940,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39831,1,18,13,"Sunday",49,55,null,17941,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39831,1,18,14,"Sunday",50,56,null,17942,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39831,1,18,15,"Sunday",50,56,null,17943,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39831,1,18,16,"Sunday",51,57,null,17944,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39831,1,18,17,"Sunday",49,55,null,17945,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39831,1,18,18,"Sunday",47,53,null,17946,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39831,1,18,19,"Sunday",45,51,null,17947,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39831,1,18,20,"Sunday",43,49,null,17948,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39831,1,18,21,"Sunday",42,47,null,17949,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39831,1,18,22,"Sunday",40,46,null,17950,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39831,1,18,23,"Sunday",39,43,null,17951,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39831,1,18,24,"Sunday",37,39,null,17952,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39832,1,19,1,"Weekday",35,36,null,17953,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39832,1,19,2,"Weekday",33,35,null,17954,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,3,"Weekday",33,35,null,17955,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,4,"Weekday",33,35,null,17956,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,5,"Weekday",35,38,null,17957,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,6,"Weekday",37,41,null,17958,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,7,"Weekday",39,45,null,17959,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,8,"Weekday",39,46,null,17960,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39832,1,19,9,"Weekday",39,48,null,17961,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39832,1,19,10,"Weekday",39,49,null,17962,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39832,1,19,11,"Weekday",42,51,null,17963,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39832,1,19,12,"Weekday",45,53,null,17964,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39832,1,19,13,"Weekday",48,55,null,17965,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39832,1,19,14,"Weekday",48,55,null,17966,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39832,1,19,15,"Weekday",48,55,null,17967,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39832,1,19,16,"Weekday",48,55,null,17968,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,{"$f":"DATE(2009,C450,D450)","v":39832},1,19,17,"Weekday",46,52,null,17969,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39832,1,19,18,"Weekday",45,49,null,17970,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39832,1,19,19,"Weekday",44,46,null,{"$f":"J451+1","v":17971},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39832,1,19,20,"Weekday",41,42,null,17972,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39832,1,19,21,"Weekday",39,39,null,17973,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39832,1,19,22,"Weekday",36,36,null,17974,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39832,1,19,23,"Weekday",33,33,null,17975,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39832,1,19,24,"Weekday",33,33,null,17976,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39833,1,20,1,"Weekday",33,33,null,17977,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39833,1,20,2,"Weekday",33,33,null,17978,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39833,1,20,3,"Weekday",33,33,null,17979,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39833,1,20,4,"Weekday",32,32,null,17980,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39833,1,20,5,"Weekday",32,32,null,17981,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39833,1,20,6,"Weekday",32,32,null,17982,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39833,1,20,7,"Weekday",32,32,null,17983,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39833,1,20,8,"Weekday",35,36,null,17984,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39833,1,20,9,"Weekday",39,40,null,17985,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39833,1,20,10,"Weekday",42,44,null,17986,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39833,1,20,11,"Weekday",43,47,null,17987,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39833,1,20,12,"Weekday",44,50,null,17988,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39833,1,20,13,"Weekday",45,53,null,17989,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39833,1,20,14,"Weekday",46,54,null,17990,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39833,1,20,15,"Weekday",47,54,null,17991,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39833,1,20,16,"Weekday",49,54,null,17992,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39833,1,20,17,"Weekday",45,49,null,17993,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39833,1,20,18,"Weekday",41,44,null,17994,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39833,1,20,19,"Weekday",38,38,null,17995,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39833,1,20,20,"Weekday",37,37,null,17996,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39833,1,20,21,"Weekday",36,37,null,17997,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39833,1,20,22,"Weekday",35,36,null,17998,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39833,1,20,23,"Weekday",35,35,null,17999,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39833,1,20,24,"Weekday",35,35,null,18000,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39834,1,21,1,"Weekday",35,35,null,18001,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39834,1,21,2,"Weekday",34,35,null,18002,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39834,1,21,3,"Weekday",35,35,null,18003,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39834,1,21,4,"Weekday",35,36,null,18004,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39834,1,21,5,"Weekday",36,38,null,18005,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39834,1,21,6,"Weekday",37,40,null,18006,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39834,1,21,7,"Weekday",39,42,null,18007,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39834,1,21,8,"Weekday",40,44,null,18008,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39834,1,21,9,"Weekday",41,45,null,18009,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39834,1,21,10,"Weekday",43,47,null,18010,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39834,1,21,11,"Weekday",44,49,null,18011,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39834,1,21,12,"Weekday",45,51,null,18012,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39834,1,21,13,"Weekday",46,53,null,18013,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39834,1,21,14,"Weekday",47,52,null,18014,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39834,1,21,15,"Weekday",47,52,null,18015,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39834,1,21,16,"Weekday",47,51,null,18016,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39834,1,21,17,"Weekday",47,50,null,18017,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39834,1,21,18,"Weekday",47,48,null,18018,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39834,1,21,19,"Weekday",46,47,null,18019,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39834,1,21,20,"Weekday",46,47,null,18020,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39834,1,21,21,"Weekday",46,47,null,18021,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39834,1,21,22,"Weekday",46,47,null,18022,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39834,1,21,23,"Weekday",45,47,null,18023,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39834,1,21,24,"Weekday",44,46,null,18024,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39835,1,22,1,"Weekday",43,46,null,18025,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39835,1,22,2,"Weekday",43,46,null,18026,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38}]
[1,39835,1,22,3,"Weekday",44,46,null,18027,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36}]
[1,39835,1,22,4,"Weekday",44,46,null,18028,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":32},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34}]
[1,39835,1,22,5,"Weekday",44,46,null,18029,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36}]
[1,39835,1,22,6,"Weekday",44,46,null,18030,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39835,1,22,7,"Weekday",45,46,null,18031,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38}]
[1,39835,1,22,8,"Weekday",45,46,null,18032,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,{"$f":"DATE(2009,C514,D514)","v":39835},1,22,9,"Weekday",46,47,null,18033,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39835,1,22,10,"Weekday",47,48,null,18034,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39835,1,22,11,"Weekday",48,49,null,{"$f":"J515+1","v":18035},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39835,1,22,12,"Weekday",49,50,null,18036,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39835,1,22,13,"Weekday",51,51,null,18037,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39835,1,22,14,"Weekday",50,51,null,18038,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39835,1,22,15,"Weekday",50,50,null,18039,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39835,1,22,16,"Weekday",50,50,null,18040,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39835,1,22,17,"Weekday",48,49,null,18041,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39835,1,22,18,"Weekday",47,48,null,18042,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39835,1,22,19,"Weekday",46,47,null,18043,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39835,1,22,20,"Weekday",45,46,null,18044,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39835,1,22,21,"Weekday",45,45,null,18045,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39835,1,22,22,"Weekday",44,44,null,18046,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39835,1,22,23,"Weekday",43,44,null,18047,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39835,1,22,24,"Weekday",43,44,null,18048,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39836,1,23,1,"Weekday",43,44,null,18049,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39836,1,23,2,"Weekday",42,44,null,18050,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39836,1,23,3,"Weekday",40,42,null,18051,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39836,1,23,4,"Weekday",38,40,null,18052,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39836,1,23,5,"Weekday",39,41,null,18053,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39836,1,23,6,"Weekday",41,42,null,18054,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39836,1,23,7,"Weekday",42,43,null,18055,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39836,1,23,8,"Weekday",43,45,null,18056,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39836,1,23,9,"Weekday",45,47,null,18057,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39836,1,23,10,"Weekday",46,48,null,18058,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39836,1,23,11,"Weekday",47,49,null,18059,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39836,1,23,12,"Weekday",48,50,null,18060,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39836,1,23,13,"Weekday",49,51,null,18061,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39836,1,23,14,"Weekday",49,51,null,18062,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39836,1,23,15,"Weekday",48,51,null,18063,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39836,1,23,16,"Weekday",48,51,null,18064,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39836,1,23,17,"Weekday",48,50,null,18065,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39836,1,23,18,"Weekday",47,49,null,18066,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39836,1,23,19,"Weekday",47,48,null,18067,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39836,1,23,20,"Weekday",46,48,null,18068,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39836,1,23,21,"Weekday",46,47,null,18069,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39836,1,23,22,"Weekday",45,46,null,18070,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39836,1,23,23,"Weekday",45,46,null,18071,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39836,1,23,24,"Weekday",45,46,null,18072,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39837,1,24,1,"Saturday",45,46,null,18073,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39837,1,24,2,"Saturday",45,46,null,18074,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39837,1,24,3,"Saturday",45,46,null,18075,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39837,1,24,4,"Saturday",45,45,null,18076,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39837,1,24,5,"Saturday",45,46,null,18077,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39837,1,24,6,"Saturday",45,47,null,18078,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39837,1,24,7,"Saturday",46,47,null,18079,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39837,1,24,8,"Saturday",47,49,null,18080,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39837,1,24,9,"Saturday",49,50,null,18081,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39837,1,24,10,"Saturday",50,52,null,18082,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39837,1,24,11,"Saturday",52,54,null,18083,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39837,1,24,12,"Saturday",53,56,null,18084,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39837,1,24,13,"Saturday",55,59,null,18085,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39837,1,24,14,"Saturday",54,57,null,18086,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39837,1,24,15,"Saturday",53,56,null,18087,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39837,1,24,16,"Saturday",52,55,null,18088,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39837,1,24,17,"Saturday",50,52,null,18089,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39837,1,24,18,"Saturday",47,49,null,18090,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39837,1,24,19,"Saturday",45,46,null,18091,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39837,1,24,20,"Saturday",44,45,null,18092,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39837,1,24,21,"Saturday",44,44,null,18093,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39837,1,24,22,"Saturday",43,43,null,18094,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39837,1,24,23,"Saturday",42,42,null,18095,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39837,1,24,24,"Saturday",42,42,null,18096,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,{"$f":"DATE(2009,C578,D578)","v":39838},1,25,1,"Sunday",42,42,null,18097,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39838,1,25,2,"Sunday",42,42,null,18098,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39838,1,25,3,"Sunday",42,42,null,{"$f":"J579+1","v":18099},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39838,1,25,4,"Sunday",42,42,null,18100,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,5,"Sunday",41,41,null,18101,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,6,"Sunday",40,40,null,18102,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,7,"Sunday",38,38,null,18103,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,8,"Sunday",42,42,null,18104,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,9,"Sunday",45,46,null,18105,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,10,"Sunday",49,50,null,18106,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39838,1,25,11,"Sunday",50,53,null,18107,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39838,1,25,12,"Sunday",51,56,null,18108,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39838,1,25,13,"Sunday",52,59,null,18109,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39838,1,25,14,"Sunday",52,59,null,18110,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39838,1,25,15,"Sunday",53,60,null,18111,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39838,1,25,16,"Sunday",53,60,null,18112,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39838,1,25,17,"Sunday",51,57,null,18113,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39838,1,25,18,"Sunday",49,54,null,18114,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39838,1,25,19,"Sunday",48,51,null,18115,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39838,1,25,20,"Sunday",47,50,null,18116,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39838,1,25,21,"Sunday",46,48,null,18117,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39838,1,25,22,"Sunday",45,47,null,18118,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39838,1,25,23,"Sunday",44,45,null,18119,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39838,1,25,24,"Sunday",43,43,null,18120,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39839,1,26,1,"Weekday",42,42,null,18121,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39839,1,26,2,"Weekday",40,41,null,18122,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39839,1,26,3,"Weekday",41,42,null,18123,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39839,1,26,4,"Weekday",41,43,null,18124,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39839,1,26,5,"Weekday",43,47,null,18125,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39839,1,26,6,"Weekday",45,52,null,18126,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39839,1,26,7,"Weekday",46,56,null,18127,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39839,1,26,8,"Weekday",47,56,null,18128,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39839,1,26,9,"Weekday",48,55,null,18129,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39839,1,26,10,"Weekday",50,55,null,18130,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39839,1,26,11,"Weekday",51,58,null,18131,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39839,1,26,12,"Weekday",52,62,null,18132,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39839,1,26,13,"Weekday",53,65,null,18133,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39839,1,26,14,"Weekday",52,64,null,18134,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39839,1,26,15,"Weekday",50,62,null,18135,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39839,1,26,16,"Weekday",49,60,null,18136,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39839,1,26,17,"Weekday",48,60,null,18137,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39839,1,26,18,"Weekday",47,60,null,18138,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39839,1,26,19,"Weekday",46,59,null,18139,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39839,1,26,20,"Weekday",45,57,null,18140,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39839,1,26,21,"Weekday",43,55,null,18141,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39839,1,26,22,"Weekday",42,53,null,18142,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39839,1,26,23,"Weekday",42,50,null,18143,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39839,1,26,24,"Weekday",41,47,null,18144,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39840,1,27,1,"Weekday",41,44,null,18145,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39840,1,27,2,"Weekday",40,42,null,18146,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39840,1,27,3,"Weekday",39,40,null,18147,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39840,1,27,4,"Weekday",38,39,null,18148,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39840,1,27,5,"Weekday",39,40,null,18149,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39840,1,27,6,"Weekday",39,41,null,18150,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39840,1,27,7,"Weekday",40,42,null,18151,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39840,1,27,8,"Weekday",42,46,null,18152,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39840,1,27,9,"Weekday",45,50,null,18153,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39840,1,27,10,"Weekday",47,54,null,18154,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39840,1,27,11,"Weekday",49,57,null,18155,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39840,1,27,12,"Weekday",51,59,null,18156,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39840,1,27,13,"Weekday",52,61,null,18157,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39840,1,27,14,"Weekday",53,60,null,18158,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39840,1,27,15,"Weekday",53,60,null,18159,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39840,1,27,16,"Weekday",54,59,null,18160,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,{"$f":"DATE(2009,C642,D642)","v":39840},1,27,17,"Weekday",51,55,null,18161,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39840,1,27,18,"Weekday",48,51,null,18162,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39840,1,27,19,"Weekday",45,47,null,{"$f":"J643+1","v":18163},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39840,1,27,20,"Weekday",44,46,null,18164,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39840,1,27,21,"Weekday",44,45,null,18165,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39840,1,27,22,"Weekday",43,43,null,18166,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39840,1,27,23,"Weekday",42,43,null,18167,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39840,1,27,24,"Weekday",42,44,null,18168,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39841,1,28,1,"Weekday",42,44,null,18169,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39841,1,28,2,"Weekday",41,43,null,18170,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39841,1,28,3,"Weekday",40,40,null,18171,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39841,1,28,4,"Weekday",38,38,null,18172,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39841,1,28,5,"Weekday",38,38,null,18173,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39841,1,28,6,"Weekday",38,39,null,18174,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39841,1,28,7,"Weekday",39,40,null,18175,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39841,1,28,8,"Weekday",42,44,null,18176,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39841,1,28,9,"Weekday",45,49,null,18177,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39841,1,28,10,"Weekday",48,53,null,18178,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39841,1,28,11,"Weekday",49,58,null,18179,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39841,1,28,12,"Weekday",51,63,null,18180,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39841,1,28,13,"Weekday",52,67,null,18181,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39841,1,28,14,"Weekday",53,66,null,18182,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39841,1,28,15,"Weekday",53,66,null,18183,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39841,1,28,16,"Weekday",54,65,null,18184,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39841,1,28,17,"Weekday",53,64,null,18185,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39841,1,28,18,"Weekday",53,62,null,18186,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39841,1,28,19,"Weekday",53,61,null,18187,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39841,1,28,20,"Weekday",52,58,null,18188,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39841,1,28,21,"Weekday",51,56,null,18189,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39841,1,28,22,"Weekday",51,53,null,18190,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39841,1,28,23,"Weekday",49,51,null,18191,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39841,1,28,24,"Weekday",49,50,null,18192,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39842,1,29,1,"Weekday",49,50,null,18193,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39842,1,29,2,"Weekday",49,50,null,18194,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39842,1,29,3,"Weekday",49,51,null,18195,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39842,1,29,4,"Weekday",50,51,null,18196,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39842,1,29,5,"Weekday",50,51,null,18197,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39842,1,29,6,"Weekday",50,51,null,18198,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39842,1,29,7,"Weekday",49,50,null,18199,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39842,1,29,8,"Weekday",49,52,null,18200,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39842,1,29,9,"Weekday",49,53,null,18201,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39842,1,29,10,"Weekday",49,55,null,18202,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39842,1,29,11,"Weekday",50,55,null,18203,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39842,1,29,12,"Weekday",50,54,null,18204,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39842,1,29,13,"Weekday",51,54,null,18205,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39842,1,29,14,"Weekday",51,53,null,18206,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39842,1,29,15,"Weekday",51,53,null,18207,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39842,1,29,16,"Weekday",52,53,null,18208,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39842,1,29,17,"Weekday",51,52,null,18209,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39842,1,29,18,"Weekday",51,52,null,18210,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39842,1,29,19,"Weekday",50,51,null,18211,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39842,1,29,20,"Weekday",50,50,null,18212,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39842,1,29,21,"Weekday",49,49,null,18213,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39842,1,29,22,"Weekday",48,48,null,18214,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39842,1,29,23,"Weekday",48,48,null,18215,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39842,1,29,24,"Weekday",48,49,null,18216,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39843,1,30,1,"Weekday",48,49,null,18217,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,2,"Weekday",48,49,null,18218,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,3,"Weekday",47,47,null,18219,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,4,"Weekday",46,47,null,18220,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,5,"Weekday",46,47,null,18221,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,6,"Weekday",46,47,null,18222,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,7,"Weekday",46,47,null,18223,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,8,"Weekday",46,47,null,18224,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,{"$f":"DATE(2009,C706,D706)","v":39843},1,30,9,"Weekday",47,49,null,18225,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39843,1,30,10,"Weekday",48,50,null,18226,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39843,1,30,11,"Weekday",49,51,null,{"$f":"J707+1","v":18227},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39843,1,30,12,"Weekday",50,53,null,18228,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39843,1,30,13,"Weekday",52,55,null,18229,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39843,1,30,14,"Weekday",50,53,null,18230,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39843,1,30,15,"Weekday",49,51,null,18231,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39843,1,30,16,"Weekday",48,49,null,18232,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39843,1,30,17,"Weekday",47,47,null,18233,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39843,1,30,18,"Weekday",45,47,null,18234,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39843,1,30,19,"Weekday",44,45,null,18235,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,20,"Weekday",44,45,null,18236,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39843,1,30,21,"Weekday",44,45,null,18237,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39843,1,30,22,"Weekday",43,44,null,18238,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39843,1,30,23,"Weekday",43,44,null,18239,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39843,1,30,24,"Weekday",43,44,null,18240,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39844,1,31,1,"Saturday",43,43,null,18241,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39844,1,31,2,"Saturday",43,43,null,18242,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39844,1,31,3,"Saturday",42,42,null,18243,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39844,1,31,4,"Saturday",42,42,null,18244,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39844,1,31,5,"Saturday",42,42,null,18245,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39844,1,31,6,"Saturday",43,43,null,18246,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39844,1,31,7,"Saturday",43,43,null,18247,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39844,1,31,8,"Saturday",44,45,null,18248,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39844,1,31,9,"Saturday",46,47,null,18249,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39844,1,31,10,"Saturday",47,49,null,18250,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39844,1,31,11,"Saturday",48,50,null,18251,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39844,1,31,12,"Saturday",49,52,null,18252,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39844,1,31,13,"Saturday",50,53,null,18253,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39844,1,31,14,"Saturday",49,53,null,18254,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39844,1,31,15,"Saturday",49,53,null,18255,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,16,"Saturday",49,53,null,18256,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,17,"Saturday",49,52,null,18257,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,18,"Saturday",48,50,null,18258,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,19,"Saturday",47,48,null,18259,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,20,"Saturday",48,50,null,18260,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,21,"Saturday",48,51,null,18261,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,22,"Saturday",48,52,null,18262,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39844,1,31,23,"Saturday",48,51,null,18263,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39844,1,31,24,"Saturday",46,49,null,18264,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39845,2,1,1,"Sunday",46,47,null,18265,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,2,"Sunday",44,45,null,18266,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,3,"Sunday",42,43,null,18267,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,4,"Sunday",42,43,null,18268,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,5,"Sunday",41,42,null,18269,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,6,"Sunday",40,43,null,18270,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,7,"Sunday",39,39,null,18271,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39845,2,1,8,"Sunday",44,45,null,18272,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39845,2,1,9,"Sunday",47,47,null,18273,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39845,2,1,10,"Sunday",51,53,null,18274,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39845,2,1,11,"Sunday",51,53,null,18275,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39845,2,1,12,"Sunday",51,53,null,18276,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39845,2,1,13,"Sunday",52,55,null,18277,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,14,"Sunday",54,56,null,18278,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,15,"Sunday",55,59,null,18279,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,16,"Sunday",51,53,null,18280,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,17,"Sunday",47,47,null,18281,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,18,"Sunday",47,47,null,18282,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39845,2,1,19,"Sunday",47,47,null,18283,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39845,2,1,20,"Sunday",46,46,null,18284,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39845,2,1,21,"Sunday",47,47,null,18285,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,22,"Sunday",44,45,null,18286,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39845,2,1,23,"Sunday",44,44,null,18287,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39845,2,1,24,"Sunday",43,44,null,18288,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,{"$f":"DATE(2009,C770,D770)","v":39846},2,2,1,"Weekday",44,44,null,18289,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39846,2,2,2,"Weekday",45,45,null,18290,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39846,2,2,3,"Weekday",43,43,null,{"$f":"J771+1","v":18291},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39846,2,2,4,"Weekday",39,39,null,18292,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39846,2,2,5,"Weekday",38,39,null,18293,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39846,2,2,6,"Weekday",38,38,null,18294,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39846,2,2,7,"Weekday",36,38,null,18295,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39846,2,2,8,"Weekday",38,39,null,18296,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39846,2,2,9,"Weekday",43,43,null,18297,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39846,2,2,10,"Weekday",44,45,null,18298,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39846,2,2,11,"Weekday",45,46,null,18299,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39846,2,2,12,"Weekday",47,48,null,18300,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39846,2,2,13,"Weekday",52,52,null,18301,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39846,2,2,14,"Weekday",49,49,null,18302,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39846,2,2,15,"Weekday",48,49,null,18303,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39846,2,2,16,"Weekday",49,49,null,18304,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39846,2,2,17,"Weekday",49,49,null,18305,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39846,2,2,18,"Weekday",46,47,null,18306,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39846,2,2,19,"Weekday",46,47,null,18307,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39846,2,2,20,"Weekday",47,47,null,18308,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39846,2,2,21,"Weekday",48,49,null,18309,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39846,2,2,22,"Weekday",46,46,null,18310,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39846,2,2,23,"Weekday",45,46,null,18311,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39846,2,2,24,"Weekday",49,49,null,18312,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39847,2,3,1,"Weekday",49,53,null,18313,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39847,2,3,2,"Weekday",48,51,null,18314,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39847,2,3,3,"Weekday",44,45,null,18315,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39847,2,3,4,"Weekday",44,45,null,18316,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39847,2,3,5,"Weekday",42,42,null,18317,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39847,2,3,6,"Weekday",44,46,null,18318,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39847,2,3,7,"Weekday",43,44,null,18319,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39847,2,3,8,"Weekday",46,50,null,18320,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39847,2,3,9,"Weekday",55,63,null,18321,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39847,2,3,10,"Weekday",61,67,null,18322,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39847,2,3,11,"Weekday",62,69,null,18323,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39847,2,3,12,"Weekday",59,68,null,18324,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39847,2,3,13,"Weekday",58,64,null,18325,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39847,2,3,14,"Weekday",55,60,null,18326,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39847,2,3,15,"Weekday",56,60,null,18327,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39847,2,3,16,"Weekday",53,55,null,18328,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39847,2,3,17,"Weekday",55,58,null,18329,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39847,2,3,18,"Weekday",50,51,null,18330,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39847,2,3,19,"Weekday",51,52,null,18331,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39847,2,3,20,"Weekday",50,51,null,18332,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39847,2,3,21,"Weekday",49,51,null,18333,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39847,2,3,22,"Weekday",47,47,null,18334,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39847,2,3,23,"Weekday",47,48,null,18335,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39847,2,3,24,"Weekday",51,52,null,18336,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39848,2,4,1,"Weekday",50,55,null,18337,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39848,2,4,2,"Weekday",47,53,null,18338,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39848,2,4,3,"Weekday",43,46,null,18339,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39848,2,4,4,"Weekday",41,42,null,18340,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39848,2,4,5,"Weekday",42,46,null,18341,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39848,2,4,6,"Weekday",41,42,null,18342,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39848,2,4,7,"Weekday",42,46,null,18343,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39848,2,4,8,"Weekday",43,49,null,18344,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39848,2,4,9,"Weekday",45,49,null,18345,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39848,2,4,10,"Weekday",48,49,null,18346,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39848,2,4,11,"Weekday",48,51,null,18347,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39848,2,4,12,"Weekday",46,46,null,18348,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39848,2,4,13,"Weekday",46,46,null,18349,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39848,2,4,14,"Weekday",46,47,null,18350,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39848,2,4,15,"Weekday",47,47,null,18351,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39848,2,4,16,"Weekday",47,47,null,18352,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,{"$f":"DATE(2009,C834,D834)","v":39848},2,4,17,"Weekday",46,47,null,18353,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39848,2,4,18,"Weekday",45,46,null,18354,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39848,2,4,19,"Weekday",45,46,null,{"$f":"J835+1","v":18355},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39848,2,4,20,"Weekday",46,46,null,18356,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39848,2,4,21,"Weekday",46,46,null,18357,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39848,2,4,22,"Weekday",45,46,null,18358,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39848,2,4,23,"Weekday",45,45,null,18359,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39848,2,4,24,"Weekday",42,43,null,18360,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39849,2,5,1,"Weekday",40,41,null,18361,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39849,2,5,2,"Weekday",38,38,null,18362,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39849,2,5,3,"Weekday",37,37,null,18363,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39849,2,5,4,"Weekday",38,38,null,18364,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39849,2,5,5,"Weekday",39,40,null,18365,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39849,2,5,6,"Weekday",37,37,null,18366,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39849,2,5,7,"Weekday",36,36,null,18367,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39849,2,5,8,"Weekday",38,38,null,18368,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39849,2,5,9,"Weekday",40,40,null,18369,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39849,2,5,10,"Weekday",42,42,null,18370,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39849,2,5,11,"Weekday",41,41,null,18371,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39849,2,5,12,"Weekday",45,46,null,18372,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39849,2,5,13,"Weekday",45,46,null,18373,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39849,2,5,14,"Weekday",47,49,null,18374,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39849,2,5,15,"Weekday",46,47,null,18375,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39849,2,5,16,"Weekday",46,47,null,18376,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39849,2,5,17,"Weekday",46,46,null,18377,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39849,2,5,18,"Weekday",45,45,null,18378,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39849,2,5,19,"Weekday",46,46,null,18379,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39849,2,5,20,"Weekday",45,46,null,18380,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39849,2,5,21,"Weekday",45,46,null,18381,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39849,2,5,22,"Weekday",45,46,null,18382,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39849,2,5,23,"Weekday",45,45,null,18383,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39849,2,5,24,"Weekday",44,44,null,18384,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39850,2,6,1,"Weekday",42,43,null,18385,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39850,2,6,2,"Weekday",42,42,null,18386,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39850,2,6,3,"Weekday",42,42,null,18387,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39850,2,6,4,"Weekday",42,42,null,18388,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39850,2,6,5,"Weekday",42,42,null,18389,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39850,2,6,6,"Weekday",43,44,null,18390,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39850,2,6,7,"Weekday",43,44,null,18391,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39850,2,6,8,"Weekday",43,44,null,18392,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39850,2,6,9,"Weekday",43,44,null,18393,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39850,2,6,10,"Weekday",47,50,null,18394,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39850,2,6,11,"Weekday",45,47,null,18395,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39850,2,6,12,"Weekday",48,51,null,18396,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39850,2,6,13,"Weekday",52,56,null,18397,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39850,2,6,14,"Weekday",51,56,null,18398,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39850,2,6,15,"Weekday",49,52,null,18399,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39850,2,6,16,"Weekday",49,51,null,18400,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39850,2,6,17,"Weekday",47,49,null,18401,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39850,2,6,18,"Weekday",47,48,null,18402,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39850,2,6,19,"Weekday",47,49,null,18403,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39850,2,6,20,"Weekday",47,48,null,18404,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39850,2,6,21,"Weekday",47,48,null,18405,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39850,2,6,22,"Weekday",46,47,null,18406,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39850,2,6,23,"Weekday",45,45,null,18407,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39850,2,6,24,"Weekday",43,43,null,18408,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39851,2,7,1,"Saturday",42,42,null,18409,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39851,2,7,2,"Saturday",41,42,null,18410,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39851,2,7,3,"Saturday",41,42,null,18411,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39851,2,7,4,"Saturday",40,41,null,18412,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39851,2,7,5,"Saturday",40,41,null,18413,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39851,2,7,6,"Saturday",40,41,null,18414,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39851,2,7,7,"Saturday",42,42,null,18415,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39851,2,7,8,"Saturday",44,44,null,18416,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,{"$f":"DATE(2009,C898,D898)","v":39851},2,7,9,"Saturday",45,45,null,18417,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39851,2,7,10,"Saturday",46,46,null,18418,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39851,2,7,11,"Saturday",48,48,null,{"$f":"J899+1","v":18419},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39851,2,7,12,"Saturday",47,48,null,18420,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39851,2,7,13,"Saturday",46,47,null,18421,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39851,2,7,14,"Saturday",46,47,null,18422,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39851,2,7,15,"Saturday",46,46,null,18423,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39851,2,7,16,"Saturday",47,48,null,18424,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39851,2,7,17,"Saturday",46,46,null,18425,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39851,2,7,18,"Saturday",45,45,null,18426,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39851,2,7,19,"Saturday",44,44,null,18427,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39851,2,7,20,"Saturday",44,45,null,18428,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39851,2,7,21,"Saturday",43,43,null,18429,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39851,2,7,22,"Saturday",43,44,null,18430,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39851,2,7,23,"Saturday",44,44,null,18431,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39851,2,7,24,"Saturday",43,44,null,18432,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39852,2,8,1,"Sunday",43,43,null,18433,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39852,2,8,2,"Sunday",43,43,null,18434,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39852,2,8,3,"Sunday",43,43,null,18435,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39852,2,8,4,"Sunday",40,40,null,18436,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39852,2,8,5,"Sunday",40,40,null,18437,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39852,2,8,6,"Sunday",43,43,null,18438,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39852,2,8,7,"Sunday",39,39,null,18439,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39852,2,8,8,"Sunday",40,40,null,18440,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39852,2,8,9,"Sunday",47,47,null,18441,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39852,2,8,10,"Sunday",44,45,null,18442,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39852,2,8,11,"Sunday",48,49,null,18443,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39852,2,8,12,"Sunday",48,49,null,18444,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39852,2,8,13,"Sunday",50,52,null,18445,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39852,2,8,14,"Sunday",50,52,null,18446,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39852,2,8,15,"Sunday",47,47,null,18447,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39852,2,8,16,"Sunday",46,46,null,18448,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39852,2,8,17,"Sunday",48,48,null,18449,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39852,2,8,18,"Sunday",47,47,null,18450,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39852,2,8,19,"Sunday",47,47,null,18451,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39852,2,8,20,"Sunday",45,46,null,18452,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39852,2,8,21,"Sunday",46,46,null,18453,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39852,2,8,22,"Sunday",46,46,null,18454,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39852,2,8,23,"Sunday",46,46,null,18455,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39852,2,8,24,"Sunday",45,45,null,18456,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,1,"Weekday",44,45,null,18457,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,2,"Weekday",44,44,null,18458,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,3,"Weekday",44,44,null,18459,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,4,"Weekday",44,44,null,18460,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,5,"Weekday",44,44,null,18461,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,6,"Weekday",44,44,null,18462,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,7,"Weekday",42,42,null,18463,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,8,"Weekday",42,44,null,18464,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,9,"Weekday",44,44,null,18465,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,10,"Weekday",45,46,null,18466,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39853,2,9,11,"Weekday",46,47,null,18467,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39853,2,9,12,"Weekday",43,44,null,18468,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39853,2,9,13,"Weekday",48,50,null,18469,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39853,2,9,14,"Weekday",48,52,null,18470,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39853,2,9,15,"Weekday",48,50,null,18471,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39853,2,9,16,"Weekday",48,49,null,18472,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39853,2,9,17,"Weekday",47,49,null,18473,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39853,2,9,18,"Weekday",47,49,null,18474,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39853,2,9,19,"Weekday",47,49,null,18475,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,20,"Weekday",48,48,null,18476,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,21,"Weekday",47,47,null,18477,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,22,"Weekday",47,48,null,18478,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39853,2,9,23,"Weekday",48,49,null,18479,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39853,2,9,24,"Weekday",48,49,null,18480,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,{"$f":"DATE(2009,C962,D962)","v":39854},2,10,1,"Weekday",48,49,null,18481,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39854,2,10,2,"Weekday",48,49,null,18482,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39854,2,10,3,"Weekday",47,49,null,{"$f":"J963+1","v":18483},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39854,2,10,4,"Weekday",46,48,null,18484,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39854,2,10,5,"Weekday",46,47,null,18485,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39854,2,10,6,"Weekday",46,47,null,18486,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39854,2,10,7,"Weekday",45,47,null,18487,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39854,2,10,8,"Weekday",46,47,null,18488,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39854,2,10,9,"Weekday",47,49,null,18489,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39854,2,10,10,"Weekday",50,52,null,18490,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39854,2,10,11,"Weekday",51,54,null,18491,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39854,2,10,12,"Weekday",50,53,null,18492,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39854,2,10,13,"Weekday",52,56,null,18493,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39854,2,10,14,"Weekday",52,55,null,18494,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39854,2,10,15,"Weekday",49,52,null,18495,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39854,2,10,16,"Weekday",49,52,null,18496,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39854,2,10,17,"Weekday",49,51,null,18497,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39854,2,10,18,"Weekday",49,51,null,18498,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39854,2,10,19,"Weekday",49,51,null,18499,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39854,2,10,20,"Weekday",49,51,null,18500,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39854,2,10,21,"Weekday",49,51,null,18501,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39854,2,10,22,"Weekday",49,50,null,18502,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39854,2,10,23,"Weekday",49,50,null,18503,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39854,2,10,24,"Weekday",48,50,null,18504,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39855,2,11,1,"Weekday",49,50,null,18505,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39855,2,11,2,"Weekday",49,51,null,18506,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39855,2,11,3,"Weekday",49,51,null,18507,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39855,2,11,4,"Weekday",50,51,null,18508,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39855,2,11,5,"Weekday",49,51,null,18509,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39855,2,11,6,"Weekday",48,49,null,18510,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39855,2,11,7,"Weekday",48,49,null,18511,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39855,2,11,8,"Weekday",50,51,null,18512,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39855,2,11,9,"Weekday",51,52,null,18513,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39855,2,11,10,"Weekday",51,52,null,18514,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39855,2,11,11,"Weekday",53,54,null,18515,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39855,2,11,12,"Weekday",55,56,null,18516,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39855,2,11,13,"Weekday",56,62,null,18517,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39855,2,11,14,"Weekday",56,62,null,18518,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39855,2,11,15,"Weekday",56,58,null,18519,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39855,2,11,16,"Weekday",54,58,null,18520,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39855,2,11,17,"Weekday",53,58,null,18521,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39855,2,11,18,"Weekday",54,58,null,18522,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39855,2,11,19,"Weekday",54,61,null,18523,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39855,2,11,20,"Weekday",54,58,null,18524,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39855,2,11,21,"Weekday",55,60,null,18525,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39855,2,11,22,"Weekday",54,57,null,18526,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39855,2,11,23,"Weekday",54,57,null,18527,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39855,2,11,24,"Weekday",54,58,null,18528,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39856,2,12,1,"Weekday",56,59,null,18529,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39856,2,12,2,"Weekday",55,59,null,18530,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39856,2,12,3,"Weekday",55,58,null,18531,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39856,2,12,4,"Weekday",54,59,null,18532,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39856,2,12,5,"Weekday",55,60,null,18533,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39856,2,12,6,"Weekday",55,59,null,18534,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39856,2,12,7,"Weekday",56,59,null,18535,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39856,2,12,8,"Weekday",57,59,null,18536,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39856,2,12,9,"Weekday",57,59,null,18537,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39856,2,12,10,"Weekday",57,61,null,18538,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39856,2,12,11,"Weekday",56,64,null,18539,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39856,2,12,12,"Weekday",58,65,null,18540,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39856,2,12,13,"Weekday",57,65,null,18541,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39856,2,12,14,"Weekday",57,65,null,18542,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39856,2,12,15,"Weekday",57,65,null,18543,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39856,2,12,16,"Weekday",54,61,null,18544,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,{"$f":"DATE(2009,C1026,D1026)","v":39856},2,12,17,"Weekday",54,61,null,18545,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39856,2,12,18,"Weekday",53,55,null,18546,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39856,2,12,19,"Weekday",50,55,null,{"$f":"J1027+1","v":18547},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39856,2,12,20,"Weekday",51,57,null,18548,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39856,2,12,21,"Weekday",50,55,null,18549,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39856,2,12,22,"Weekday",50,54,null,18550,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39856,2,12,23,"Weekday",49,53,null,18551,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39856,2,12,24,"Weekday",49,52,null,18552,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39857,2,13,1,"Weekday",49,51,null,18553,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39857,2,13,2,"Weekday",47,50,null,18554,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39857,2,13,3,"Weekday",47,50,null,18555,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39857,2,13,4,"Weekday",46,50,null,18556,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39857,2,13,5,"Weekday",47,52,null,18557,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39857,2,13,6,"Weekday",47,52,null,18558,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39857,2,13,7,"Weekday",46,46,null,18559,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39857,2,13,8,"Weekday",46,46,null,18560,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39857,2,13,9,"Weekday",49,49,null,18561,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39857,2,13,10,"Weekday",46,47,null,18562,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39857,2,13,11,"Weekday",47,48,null,18563,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39857,2,13,12,"Weekday",45,46,null,18564,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39857,2,13,13,"Weekday",45,46,null,18565,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39857,2,13,14,"Weekday",46,48,null,18566,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39857,2,13,15,"Weekday",45,48,null,18567,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39857,2,13,16,"Weekday",44,46,null,18568,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39857,2,13,17,"Weekday",44,46,null,18569,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39857,2,13,18,"Weekday",43,46,null,18570,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39857,2,13,19,"Weekday",44,46,null,18571,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39857,2,13,20,"Weekday",44,46,null,18572,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39857,2,13,21,"Weekday",44,46,null,18573,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39857,2,13,22,"Weekday",42,44,null,18574,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39857,2,13,23,"Weekday",41,42,null,18575,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39857,2,13,24,"Weekday",41,42,null,18576,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39858,2,14,1,"Saturday",42,43,null,18577,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39858,2,14,2,"Saturday",42,43,null,18578,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39858,2,14,3,"Saturday",42,43,null,18579,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39858,2,14,4,"Saturday",42,43,null,18580,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39858,2,14,5,"Saturday",43,44,null,18581,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39858,2,14,6,"Saturday",42,44,null,18582,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39858,2,14,7,"Saturday",42,43,null,18583,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39858,2,14,8,"Saturday",42,43,null,18584,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39858,2,14,9,"Saturday",45,46,null,18585,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39858,2,14,10,"Saturday",46,49,null,18586,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39858,2,14,11,"Saturday",48,52,null,18587,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39858,2,14,12,"Saturday",47,50,null,18588,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39858,2,14,13,"Saturday",46,49,null,18589,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39858,2,14,14,"Saturday",45,50,null,18590,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39858,2,14,15,"Saturday",44,48,null,18591,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39858,2,14,16,"Saturday",45,48,null,18592,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39858,2,14,17,"Saturday",45,49,null,18593,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39858,2,14,18,"Saturday",43,45,null,18594,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39858,2,14,19,"Saturday",42,43,null,18595,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39858,2,14,20,"Saturday",42,44,null,18596,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39858,2,14,21,"Saturday",41,44,null,18597,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39858,2,14,22,"Saturday",41,43,null,18598,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39858,2,14,23,"Saturday",40,41,null,18599,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39858,2,14,24,"Saturday",37,40,null,18600,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39859,2,15,1,"Sunday",37,40,null,18601,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39859,2,15,2,"Sunday",38,41,null,18602,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39859,2,15,3,"Sunday",39,43,null,18603,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39859,2,15,4,"Sunday",39,43,null,18604,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39859,2,15,5,"Sunday",38,42,null,18605,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39859,2,15,6,"Sunday",40,44,null,18606,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39859,2,15,7,"Sunday",40,46,null,18607,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39859,2,15,8,"Sunday",40,45,null,18608,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,{"$f":"DATE(2009,C1090,D1090)","v":39859},2,15,9,"Sunday",42,47,null,18609,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39859,2,15,10,"Sunday",44,51,null,18610,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39859,2,15,11,"Sunday",43,53,null,{"$f":"J1091+1","v":18611},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39859,2,15,12,"Sunday",47,54,null,18612,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39859,2,15,13,"Sunday",47,54,null,18613,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39859,2,15,14,"Sunday",47,55,null,18614,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39859,2,15,15,"Sunday",47,54,null,18615,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39859,2,15,16,"Sunday",46,53,null,18616,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39859,2,15,17,"Sunday",47,51,null,18617,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39859,2,15,18,"Sunday",45,51,null,18618,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39859,2,15,19,"Sunday",47,51,null,18619,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39859,2,15,20,"Sunday",45,52,null,18620,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39859,2,15,21,"Sunday",44,52,null,18621,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39859,2,15,22,"Sunday",43,53,null,18622,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39859,2,15,23,"Sunday",44,54,null,18623,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39859,2,15,24,"Sunday",45,55,null,18624,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39860,2,16,1,"Weekday",46,56,null,18625,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39860,2,16,2,"Weekday",46,55,null,18626,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39860,2,16,3,"Weekday",46,54,null,18627,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39860,2,16,4,"Weekday",47,55,null,18628,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39860,2,16,5,"Weekday",48,57,null,18629,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39860,2,16,6,"Weekday",48,58,null,18630,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39860,2,16,7,"Weekday",49,57,null,18631,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39860,2,16,8,"Weekday",49,53,null,18632,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39860,2,16,9,"Weekday",50,58,null,18633,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39860,2,16,10,"Weekday",51,61,null,18634,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39860,2,16,11,"Weekday",52,61,null,18635,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39860,2,16,12,"Weekday",54,64,null,18636,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39860,2,16,13,"Weekday",54,65,null,18637,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39860,2,16,14,"Weekday",55,65,null,18638,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39860,2,16,15,"Weekday",55,65,null,18639,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39860,2,16,16,"Weekday",56,62,null,18640,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39860,2,16,17,"Weekday",57,65,null,18641,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39860,2,16,18,"Weekday",54,61,null,18642,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39860,2,16,19,"Weekday",54,59,null,18643,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39860,2,16,20,"Weekday",55,61,null,18644,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39860,2,16,21,"Weekday",56,61,null,18645,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39860,2,16,22,"Weekday",56,61,null,18646,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39860,2,16,23,"Weekday",55,61,null,18647,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39860,2,16,24,"Weekday",56,61,null,18648,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39861,2,17,1,"Weekday",55,60,null,18649,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39861,2,17,2,"Weekday",53,60,null,18650,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39861,2,17,3,"Weekday",53,59,null,18651,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39861,2,17,4,"Weekday",52,52,null,18652,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39861,2,17,5,"Weekday",49,50,null,18653,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39861,2,17,6,"Weekday",50,51,null,18654,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39861,2,17,7,"Weekday",45,46,null,18655,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39861,2,17,8,"Weekday",45,46,null,18656,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39861,2,17,9,"Weekday",45,48,null,18657,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39861,2,17,10,"Weekday",43,46,null,18658,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39861,2,17,11,"Weekday",46,49,null,18659,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39861,2,17,12,"Weekday",46,48,null,18660,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39861,2,17,13,"Weekday",44,46,null,18661,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39861,2,17,14,"Weekday",43,46,null,18662,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39861,2,17,15,"Weekday",42,46,null,18663,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39861,2,17,16,"Weekday",41,46,null,18664,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39861,2,17,17,"Weekday",41,44,null,18665,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39861,2,17,18,"Weekday",40,42,null,18666,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39861,2,17,19,"Weekday",43,48,null,18667,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39861,2,17,20,"Weekday",40,44,null,18668,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39861,2,17,21,"Weekday",43,46,null,18669,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39861,2,17,22,"Weekday",40,43,null,18670,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39861,2,17,23,"Weekday",38,39,null,18671,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39861,2,17,24,"Weekday",35,37,null,18672,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,{"$f":"DATE(2009,C1154,D1154)","v":39862},2,18,1,"Weekday",35,37,null,18673,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39862,2,18,2,"Weekday",38,40,null,18674,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39862,2,18,3,"Weekday",40,43,null,{"$f":"J1155+1","v":18675},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39862,2,18,4,"Weekday",38,40,null,18676,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39862,2,18,5,"Weekday",36,37,null,18677,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39862,2,18,6,"Weekday",37,37,null,18678,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39862,2,18,7,"Weekday",35,36,null,18679,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39862,2,18,8,"Weekday",39,41,null,18680,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39862,2,18,9,"Weekday",42,46,null,18681,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39862,2,18,10,"Weekday",45,49,null,18682,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39862,2,18,11,"Weekday",46,53,null,18683,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39862,2,18,12,"Weekday",43,50,null,18684,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39862,2,18,13,"Weekday",45,51,null,18685,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39862,2,18,14,"Weekday",44,51,null,18686,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39862,2,18,15,"Weekday",44,51,null,18687,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39862,2,18,16,"Weekday",43,49,null,18688,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,17,"Weekday",43,49,null,18689,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,18,"Weekday",43,47,null,18690,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,19,"Weekday",42,46,null,18691,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,20,"Weekday",40,44,null,18692,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,21,"Weekday",40,44,null,18693,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,22,"Weekday",40,44,null,18694,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39862,2,18,23,"Weekday",40,44,null,18695,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39862,2,18,24,"Weekday",40,44,null,18696,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39863,2,19,1,"Weekday",41,44,null,18697,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39863,2,19,2,"Weekday",41,44,null,18698,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39863,2,19,3,"Weekday",40,44,null,18699,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39863,2,19,4,"Weekday",41,44,null,18700,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39863,2,19,5,"Weekday",41,45,null,18701,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39863,2,19,6,"Weekday",41,44,null,18702,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39863,2,19,7,"Weekday",41,45,null,18703,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39863,2,19,8,"Weekday",41,46,null,18704,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39863,2,19,9,"Weekday",43,49,null,18705,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39863,2,19,10,"Weekday",47,53,null,18706,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39863,2,19,11,"Weekday",50,57,null,18707,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39863,2,19,12,"Weekday",50,55,null,18708,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39863,2,19,13,"Weekday",50,56,null,18709,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39863,2,19,14,"Weekday",51,57,null,18710,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39863,2,19,15,"Weekday",52,55,null,18711,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39863,2,19,16,"Weekday",51,53,null,18712,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39863,2,19,17,"Weekday",50,53,null,18713,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39863,2,19,18,"Weekday",49,52,null,18714,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39863,2,19,19,"Weekday",50,52,null,18715,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39863,2,19,20,"Weekday",50,52,null,18716,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39863,2,19,21,"Weekday",49,51,null,18717,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39863,2,19,22,"Weekday",48,50,null,18718,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39863,2,19,23,"Weekday",47,49,null,18719,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39863,2,19,24,"Weekday",46,49,null,18720,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39864,2,20,1,"Weekday",45,48,null,18721,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39864,2,20,2,"Weekday",47,49,null,18722,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39864,2,20,3,"Weekday",46,49,null,18723,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39864,2,20,4,"Weekday",44,47,null,18724,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39864,2,20,5,"Weekday",45,49,null,18725,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39864,2,20,6,"Weekday",45,47,null,18726,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39864,2,20,7,"Weekday",45,49,null,18727,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39864,2,20,8,"Weekday",47,51,null,18728,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39864,2,20,9,"Weekday",50,55,null,18729,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39864,2,20,10,"Weekday",55,62,null,18730,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39864,2,20,11,"Weekday",57,63,null,18731,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39864,2,20,12,"Weekday",54,61,null,18732,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39864,2,20,13,"Weekday",53,59,null,18733,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39864,2,20,14,"Weekday",56,60,null,18734,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39864,2,20,15,"Weekday",54,58,null,18735,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39864,2,20,16,"Weekday",53,55,null,18736,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,{"$f":"DATE(2009,C1218,D1218)","v":39864},2,20,17,"Weekday",54,56,null,18737,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39864,2,20,18,"Weekday",54,56,null,18738,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39864,2,20,19,"Weekday",54,58,null,{"$f":"J1219+1","v":18739},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39864,2,20,20,"Weekday",54,55,null,18740,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39864,2,20,21,"Weekday",53,54,null,18741,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39864,2,20,22,"Weekday",53,54,null,18742,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39864,2,20,23,"Weekday",52,54,null,18743,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39864,2,20,24,"Weekday",52,54,null,18744,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39865,2,21,1,"Saturday",51,54,null,18745,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39865,2,21,2,"Saturday",51,54,null,18746,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39865,2,21,3,"Saturday",51,54,null,18747,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39865,2,21,4,"Saturday",51,54,null,18748,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39865,2,21,5,"Saturday",50,53,null,18749,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39865,2,21,6,"Saturday",51,54,null,18750,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":32},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39865,2,21,7,"Saturday",50,53,null,18751,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":31},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38}]
[1,39865,2,21,8,"Saturday",52,53,null,18752,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39865,2,21,9,"Saturday",54,55,null,18753,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39865,2,21,10,"Saturday",55,57,null,18754,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39865,2,21,11,"Saturday",56,58,null,18755,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39865,2,21,12,"Saturday",57,60,null,18756,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39865,2,21,13,"Saturday",56,59,null,18757,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39865,2,21,14,"Saturday",55,57,null,18758,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39865,2,21,15,"Saturday",55,57,null,18759,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39865,2,21,16,"Saturday",55,55,null,18760,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39865,2,21,17,"Saturday",54,55,null,18761,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39865,2,21,18,"Saturday",53,53,null,18762,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39865,2,21,19,"Saturday",53,53,null,18763,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39865,2,21,20,"Saturday",53,54,null,18764,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39865,2,21,21,"Saturday",52,53,null,18765,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39865,2,21,22,"Saturday",52,53,null,18766,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39865,2,21,23,"Saturday",51,52,null,18767,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39865,2,21,24,"Saturday",49,50,null,18768,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39866,2,22,1,"Sunday",46,48,null,18769,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39866,2,22,2,"Sunday",47,48,null,18770,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39866,2,22,3,"Sunday",46,48,null,18771,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39866,2,22,4,"Sunday",44,44,null,18772,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39866,2,22,5,"Sunday",42,42,null,18773,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39866,2,22,6,"Sunday",41,41,null,18774,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39866,2,22,7,"Sunday",41,44,null,18775,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":33},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39866,2,22,8,"Sunday",47,51,null,18776,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39866,2,22,9,"Sunday",51,56,null,18777,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39866,2,22,10,"Sunday",51,55,null,18778,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39866,2,22,11,"Sunday",51,56,null,18779,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39866,2,22,12,"Sunday",52,56,null,18780,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39866,2,22,13,"Sunday",55,62,null,18781,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39866,2,22,14,"Sunday",53,58,null,18782,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39866,2,22,15,"Sunday",51,56,null,18783,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39866,2,22,16,"Sunday",51,55,null,18784,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39866,2,22,17,"Sunday",52,55,null,18785,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39866,2,22,18,"Sunday",50,52,null,18786,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39866,2,22,19,"Sunday",49,50,null,18787,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39866,2,22,20,"Sunday",47,49,null,18788,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39866,2,22,21,"Sunday",45,46,null,18789,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39866,2,22,22,"Sunday",45,47,null,18790,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39866,2,22,23,"Sunday",46,47,null,18791,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39866,2,22,24,"Sunday",46,47,null,18792,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39867,2,23,1,"Weekday",46,47,null,18793,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39867,2,23,2,"Weekday",47,47,null,18794,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39867,2,23,3,"Weekday",48,48,null,18795,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":36},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39867,2,23,4,"Weekday",47,47,null,18796,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":34},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37}]
[1,39867,2,23,5,"Weekday",47,48,null,18797,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":35},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39867,2,23,6,"Weekday",47,47,null,18798,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39867,2,23,7,"Weekday",47,47,null,18799,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39867,2,23,8,"Weekday",48,49,null,18800,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,{"$f":"DATE(2009,C1282,D1282)","v":39867},2,23,9,"Weekday",48,49,null,18801,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39867,2,23,10,"Weekday",49,50,null,18802,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39867,2,23,11,"Weekday",49,50,null,{"$f":"J1283+1","v":18803},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39867,2,23,12,"Weekday",50,52,null,18804,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39867,2,23,13,"Weekday",50,50,null,18805,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39867,2,23,14,"Weekday",51,53,null,18806,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39867,2,23,15,"Weekday",52,54,null,18807,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39867,2,23,16,"Weekday",51,53,null,18808,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":72}]
[1,39867,2,23,17,"Weekday",52,54,null,18809,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39867,2,23,18,"Weekday",51,53,null,18810,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39867,2,23,19,"Weekday",50,52,null,18811,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39867,2,23,20,"Weekday",50,51,null,18812,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39867,2,23,21,"Weekday",50,51,null,18813,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39867,2,23,22,"Weekday",50,51,null,18814,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39867,2,23,23,"Weekday",50,51,null,18815,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39867,2,23,24,"Weekday",50,51,null,18816,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39868,2,24,1,"Weekday",49,51,null,18817,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39868,2,24,2,"Weekday",50,51,null,18818,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39868,2,24,3,"Weekday",50,51,null,18819,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39868,2,24,4,"Weekday",48,49,null,18820,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39868,2,24,5,"Weekday",48,49,null,18821,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39868,2,24,6,"Weekday",48,49,null,18822,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39868,2,24,7,"Weekday",48,49,null,18823,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39868,2,24,8,"Weekday",49,51,null,18824,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39868,2,24,9,"Weekday",50,53,null,18825,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39868,2,24,10,"Weekday",52,55,null,18826,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39868,2,24,11,"Weekday",52,54,null,18827,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39868,2,24,12,"Weekday",56,63,null,18828,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39868,2,24,13,"Weekday",57,62,null,18829,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39868,2,24,14,"Weekday",56,61,null,18830,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39868,2,24,15,"Weekday",55,60,null,18831,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39868,2,24,16,"Weekday",56,59,null,18832,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":70}]
[1,39868,2,24,17,"Weekday",54,56,null,18833,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39868,2,24,18,"Weekday",53,55,null,18834,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39868,2,24,19,"Weekday",52,53,null,18835,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39868,2,24,20,"Weekday",51,52,null,18836,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39868,2,24,21,"Weekday",53,54,null,18837,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39868,2,24,22,"Weekday",52,53,null,18838,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39868,2,24,23,"Weekday",51,52,null,18839,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39868,2,24,24,"Weekday",51,52,null,18840,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39869,2,25,1,"Weekday",51,53,null,18841,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39869,2,25,2,"Weekday",52,53,null,18842,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39869,2,25,3,"Weekday",52,53,null,18843,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39869,2,25,4,"Weekday",51,52,null,18844,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39869,2,25,5,"Weekday",50,51,null,18845,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39869,2,25,6,"Weekday",50,51,null,18846,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39869,2,25,7,"Weekday",50,51,null,18847,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39869,2,25,8,"Weekday",50,52,null,18848,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39869,2,25,9,"Weekday",53,56,null,18849,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39869,2,25,10,"Weekday",53,58,null,18850,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39869,2,25,11,"Weekday",54,58,null,18851,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39869,2,25,12,"Weekday",57,64,null,18852,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39869,2,25,13,"Weekday",55,60,null,18853,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39869,2,25,14,"Weekday",57,66,null,18854,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39869,2,25,15,"Weekday",55,66,null,18855,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39869,2,25,16,"Weekday",51,60,null,18856,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39869,2,25,17,"Weekday",49,59,null,18857,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39869,2,25,18,"Weekday",48,57,null,18858,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39869,2,25,19,"Weekday",47,55,null,18859,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39869,2,25,20,"Weekday",48,53,null,18860,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39869,2,25,21,"Weekday",48,52,null,18861,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39869,2,25,22,"Weekday",49,52,null,18862,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39869,2,25,23,"Weekday",49,52,null,18863,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39869,2,25,24,"Weekday",49,51,null,18864,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,{"$f":"DATE(2009,C1346,D1346)","v":39870},2,26,1,"Weekday",48,51,null,18865,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39870,2,26,2,"Weekday",48,50,null,18866,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39870,2,26,3,"Weekday",48,50,null,{"$f":"J1347+1","v":18867},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39870,2,26,4,"Weekday",47,49,null,18868,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39870,2,26,5,"Weekday",46,48,null,18869,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39870,2,26,6,"Weekday",45,48,null,18870,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39870,2,26,7,"Weekday",45,48,null,18871,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39870,2,26,8,"Weekday",45,50,null,18872,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39870,2,26,9,"Weekday",45,52,null,18873,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39870,2,26,10,"Weekday",45,52,null,18874,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39870,2,26,11,"Weekday",47,53,null,18875,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39870,2,26,12,"Weekday",50,54,null,18876,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39870,2,26,13,"Weekday",48,53,null,18877,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39870,2,26,14,"Weekday",46,53,null,18878,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39870,2,26,15,"Weekday",46,52,null,18879,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39870,2,26,16,"Weekday",45,50,null,18880,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39870,2,26,17,"Weekday",45,50,null,18881,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39870,2,26,18,"Weekday",45,49,null,18882,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39870,2,26,19,"Weekday",43,46,null,18883,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39870,2,26,20,"Weekday",43,46,null,18884,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39870,2,26,21,"Weekday",43,46,null,18885,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39870,2,26,22,"Weekday",42,44,null,18886,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39870,2,26,23,"Weekday",40,41,null,18887,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39870,2,26,24,"Weekday",38,39,null,18888,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39871,2,27,1,"Weekday",35,36,null,18889,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39871,2,27,2,"Weekday",34,34,null,18890,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39871,2,27,3,"Weekday",33,33,null,18891,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39871,2,27,4,"Weekday",34,36,null,18892,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39871,2,27,5,"Weekday",34,36,null,18893,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39871,2,27,6,"Weekday",33,34,null,18894,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39871,2,27,7,"Weekday",32,33,null,18895,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39871,2,27,8,"Weekday",42,46,null,18896,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39871,2,27,9,"Weekday",43,48,null,18897,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39871,2,27,10,"Weekday",45,50,null,18898,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39871,2,27,11,"Weekday",46,53,null,18899,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39871,2,27,12,"Weekday",51,59,null,18900,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39871,2,27,13,"Weekday",56,66,null,18901,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39871,2,27,14,"Weekday",54,64,null,18902,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39871,2,27,15,"Weekday",54,61,null,18903,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39871,2,27,16,"Weekday",53,59,null,18904,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39871,2,27,17,"Weekday",55,62,null,18905,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39871,2,27,18,"Weekday",50,53,null,18906,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39871,2,27,19,"Weekday",48,51,null,18907,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39871,2,27,20,"Weekday",46,48,null,18908,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39871,2,27,21,"Weekday",44,45,null,18909,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39871,2,27,22,"Weekday",45,46,null,18910,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39871,2,27,23,"Weekday",45,46,null,18911,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39871,2,27,24,"Weekday",44,45,null,18912,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39872,2,28,1,"Saturday",41,43,null,18913,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39872,2,28,2,"Saturday",42,43,null,18914,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39872,2,28,3,"Saturday",42,43,null,18915,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39872,2,28,4,"Saturday",38,39,null,18916,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39872,2,28,5,"Saturday",43,43,null,18917,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39872,2,28,6,"Saturday",41,41,null,18918,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39872,2,28,7,"Saturday",40,41,null,18919,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39872,2,28,8,"Saturday",43,44,null,18920,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39872,2,28,9,"Saturday",46,47,null,18921,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39872,2,28,10,"Saturday",49,50,null,18922,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39872,2,28,11,"Saturday",51,53,null,18923,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39872,2,28,12,"Saturday",51,53,null,18924,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39872,2,28,13,"Saturday",52,55,null,18925,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":73}]
[1,39872,2,28,14,"Saturday",51,55,null,18926,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39872,2,28,15,"Saturday",51,54,null,18927,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39872,2,28,16,"Saturday",50,53,null,18928,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,{"$f":"DATE(2009,C1410,D1410)","v":39872},2,28,17,"Saturday",49,52,null,18929,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39872,2,28,18,"Saturday",48,49,null,18930,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39872,2,28,19,"Saturday",46,47,null,{"$f":"J1411+1","v":18931},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39872,2,28,20,"Saturday",45,45,null,18932,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39872,2,28,21,"Saturday",43,44,null,18933,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39872,2,28,22,"Saturday",42,42,null,18934,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39872,2,28,23,"Saturday",42,42,null,18935,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39872,2,28,24,"Saturday",42,43,null,18936,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39873,3,1,1,"Sunday",43,43,null,18937,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39873,3,1,2,"Sunday",43,44,null,18938,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39873,3,1,3,"Sunday",43,44,null,18939,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39873,3,1,4,"Sunday",43,44,null,18940,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39873,3,1,5,"Sunday",43,44,null,18941,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39873,3,1,6,"Sunday",43,44,null,18942,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39873,3,1,7,"Sunday",43,44,null,18943,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39873,3,1,8,"Sunday",44,44,null,18944,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39873,3,1,9,"Sunday",45,45,null,18945,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39873,3,1,10,"Sunday",45,46,null,18946,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39873,3,1,11,"Sunday",46,47,null,18947,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39873,3,1,12,"Sunday",49,53,null,18948,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39873,3,1,13,"Sunday",48,49,null,18949,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39873,3,1,14,"Sunday",48,51,null,18950,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39873,3,1,15,"Sunday",48,51,null,18951,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39873,3,1,16,"Sunday",46,47,null,18952,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39873,3,1,17,"Sunday",47,49,null,18953,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39873,3,1,18,"Sunday",44,45,null,18954,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39873,3,1,19,"Sunday",44,45,null,18955,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39873,3,1,20,"Sunday",43,44,null,18956,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39873,3,1,21,"Sunday",43,44,null,18957,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39873,3,1,22,"Sunday",44,44,null,18958,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39873,3,1,23,"Sunday",44,45,null,18959,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39873,3,1,24,"Sunday",44,45,null,18960,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39874,3,2,1,"Weekday",44,45,null,18961,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39874,3,2,2,"Weekday",43,44,null,18962,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39874,3,2,3,"Weekday",41,42,null,18963,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39874,3,2,4,"Weekday",40,40,null,18964,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39874,3,2,5,"Weekday",41,41,null,18965,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39874,3,2,6,"Weekday",41,42,null,18966,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39874,3,2,7,"Weekday",41,42,null,18967,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39874,3,2,8,"Weekday",42,43,null,18968,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39874,3,2,9,"Weekday",43,45,null,18969,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39874,3,2,10,"Weekday",44,45,null,18970,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39874,3,2,11,"Weekday",44,47,null,18971,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39874,3,2,12,"Weekday",45,47,null,18972,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39874,3,2,13,"Weekday",45,47,null,18973,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39874,3,2,14,"Weekday",45,47,null,18974,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39874,3,2,15,"Weekday",46,49,null,18975,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39874,3,2,16,"Weekday",46,49,null,18976,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39874,3,2,17,"Weekday",46,47,null,18977,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39874,3,2,18,"Weekday",45,47,null,18978,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39874,3,2,19,"Weekday",46,47,null,18979,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39874,3,2,20,"Weekday",47,49,null,18980,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39874,3,2,21,"Weekday",47,49,null,18981,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39874,3,2,22,"Weekday",46,47,null,18982,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39874,3,2,23,"Weekday",46,47,null,18983,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39874,3,2,24,"Weekday",45,46,null,18984,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39875,3,3,1,"Weekday",45,45,null,18985,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39875,3,3,2,"Weekday",45,45,null,18986,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39875,3,3,3,"Weekday",45,45,null,18987,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39875,3,3,4,"Weekday",45,45,null,18988,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39875,3,3,5,"Weekday",45,45,null,18989,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39875,3,3,6,"Weekday",45,45,null,18990,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39875,3,3,7,"Weekday",45,45,null,18991,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39875,3,3,8,"Weekday",46,46,null,18992,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,{"$f":"DATE(2009,C1474,D1474)","v":39875},3,3,9,"Weekday",47,48,null,18993,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39875,3,3,10,"Weekday",50,50,null,18994,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39875,3,3,11,"Weekday",51,52,null,{"$f":"J1475+1","v":18995},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39875,3,3,12,"Weekday",50,51,null,18996,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39875,3,3,13,"Weekday",51,53,null,18997,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39875,3,3,14,"Weekday",50,52,null,18998,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39875,3,3,15,"Weekday",50,52,null,18999,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39875,3,3,16,"Weekday",50,50,null,19000,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39875,3,3,17,"Weekday",49,49,null,19001,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39875,3,3,18,"Weekday",49,49,null,19002,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39875,3,3,19,"Weekday",48,48,null,19003,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39875,3,3,20,"Weekday",48,49,null,19004,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39875,3,3,21,"Weekday",48,49,null,19005,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39875,3,3,22,"Weekday",48,49,null,19006,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39875,3,3,23,"Weekday",48,49,null,19007,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39875,3,3,24,"Weekday",48,49,null,19008,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39876,3,4,1,"Weekday",48,49,null,19009,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39876,3,4,2,"Weekday",47,49,null,19010,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39876,3,4,3,"Weekday",46,47,null,19011,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39876,3,4,4,"Weekday",46,47,null,19012,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39876,3,4,5,"Weekday",45,47,null,19013,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39876,3,4,6,"Weekday",45,47,null,19014,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39876,3,4,7,"Weekday",43,45,null,19015,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39876,3,4,8,"Weekday",45,46,null,19016,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39876,3,4,9,"Weekday",48,52,null,19017,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39876,3,4,10,"Weekday",49,53,null,19018,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39876,3,4,11,"Weekday",50,55,null,19019,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39876,3,4,12,"Weekday",51,58,null,19020,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39876,3,4,13,"Weekday",50,58,null,19021,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39876,3,4,14,"Weekday",52,60,null,19022,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39876,3,4,15,"Weekday",50,60,null,19023,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39876,3,4,16,"Weekday",49,59,null,19024,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39876,3,4,17,"Weekday",49,59,null,19025,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39876,3,4,18,"Weekday",48,55,null,19026,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39876,3,4,19,"Weekday",48,55,null,19027,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39876,3,4,20,"Weekday",48,54,null,19028,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39876,3,4,21,"Weekday",49,56,null,19029,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39876,3,4,22,"Weekday",49,56,null,19030,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39876,3,4,23,"Weekday",49,56,null,19031,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39876,3,4,24,"Weekday",49,56,null,19032,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39877,3,5,1,"Weekday",51,56,null,19033,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39877,3,5,2,"Weekday",50,56,null,19034,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39877,3,5,3,"Weekday",50,55,null,19035,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39877,3,5,4,"Weekday",50,53,null,19036,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39877,3,5,5,"Weekday",50,54,null,19037,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39877,3,5,6,"Weekday",50,58,null,19038,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39877,3,5,7,"Weekday",50,58,null,19039,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":37},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40}]
[1,39877,3,5,8,"Weekday",50,56,null,19040,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39877,3,5,9,"Weekday",50,57,null,19041,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39877,3,5,10,"Weekday",50,56,null,19042,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39877,3,5,11,"Weekday",50,55,null,19043,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39877,3,5,12,"Weekday",50,54,null,19044,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39877,3,5,13,"Weekday",51,55,null,19045,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39877,3,5,14,"Weekday",50,53,null,19046,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39877,3,5,15,"Weekday",49,51,null,19047,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39877,3,5,16,"Weekday",50,51,null,19048,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39877,3,5,17,"Weekday",49,51,null,19049,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39877,3,5,18,"Weekday",49,50,null,19050,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39877,3,5,19,"Weekday",49,50,null,19051,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39877,3,5,20,"Weekday",48,49,null,19052,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39877,3,5,21,"Weekday",48,48,null,19053,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39877,3,5,22,"Weekday",48,49,null,19054,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39877,3,5,23,"Weekday",47,49,null,19055,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39877,3,5,24,"Weekday",45,47,null,19056,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,{"$f":"DATE(2009,C1538,D1538)","v":39878},3,6,1,"Weekday",45,46,null,19057,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39878,3,6,2,"Weekday",46,47,null,19058,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39878,3,6,3,"Weekday",47,49,null,{"$f":"J1539+1","v":19059},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39878,3,6,4,"Weekday",46,47,null,19060,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39878,3,6,5,"Weekday",46,47,null,19061,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39878,3,6,6,"Weekday",47,48,null,19062,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39878,3,6,7,"Weekday",45,46,null,19063,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39878,3,6,8,"Weekday",47,47,null,19064,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39878,3,6,9,"Weekday",49,53,null,19065,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39878,3,6,10,"Weekday",53,55,null,19066,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39878,3,6,11,"Weekday",51,56,null,19067,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39878,3,6,12,"Weekday",54,58,null,19068,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39878,3,6,13,"Weekday",53,55,null,19069,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39878,3,6,14,"Weekday",53,56,null,19070,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39878,3,6,15,"Weekday",51,54,null,19071,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39878,3,6,16,"Weekday",53,56,null,19072,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39878,3,6,17,"Weekday",51,54,null,19073,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39878,3,6,18,"Weekday",51,53,null,19074,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39878,3,6,19,"Weekday",48,48,null,19075,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39878,3,6,20,"Weekday",46,46,null,19076,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39878,3,6,21,"Weekday",47,47,null,19077,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39878,3,6,22,"Weekday",48,48,null,19078,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39878,3,6,23,"Weekday",47,48,null,19079,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39878,3,6,24,"Weekday",45,46,null,19080,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39879,3,7,1,"Saturday",43,43,null,19081,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39879,3,7,2,"Saturday",42,42,null,19082,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39879,3,7,3,"Saturday",43,43,null,19083,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39879,3,7,4,"Saturday",46,47,null,19084,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39879,3,7,5,"Saturday",46,47,null,19085,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39879,3,7,6,"Saturday",48,48,null,19086,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39879,3,7,7,"Saturday",48,48,null,19087,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39879,3,7,8,"Saturday",48,48,null,19088,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39879,3,7,9,"Saturday",52,54,null,19089,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39879,3,7,10,"Saturday",52,54,null,19090,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39879,3,7,11,"Saturday",54,57,null,19091,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39879,3,7,12,"Saturday",55,58,null,19092,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39879,3,7,13,"Saturday",56,58,null,19093,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39879,3,7,14,"Saturday",55,58,null,19094,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39879,3,7,15,"Saturday",58,62,null,19095,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39879,3,7,16,"Saturday",54,56,null,19096,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":72}]
[1,39879,3,7,17,"Saturday",54,55,null,19097,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39879,3,7,18,"Saturday",53,54,null,19098,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39879,3,7,19,"Saturday",53,54,null,19099,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39879,3,7,20,"Saturday",52,54,null,19100,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39879,3,7,21,"Saturday",51,53,null,19101,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39879,3,7,22,"Saturday",49,50,null,19102,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39879,3,7,23,"Saturday",49,49,null,19103,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39879,3,7,24,"Saturday",49,49,null,19104,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39880,3,8,1,"Sunday",49,50,null,19105,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39880,3,8,2,"Sunday",50,50,null,19106,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39880,3,8,3,"Sunday",50,50,null,19107,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39880,3,8,4,"Sunday",49,49,null,19108,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39880,3,8,5,"Sunday",43,43,null,19109,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39880,3,8,6,"Sunday",46,46,null,19110,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41}]
[1,39880,3,8,7,"Sunday",47,47,null,19111,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39}]
[1,39880,3,8,8,"Sunday",47,48,null,19112,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39880,3,8,9,"Sunday",49,51,null,19113,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39880,3,8,10,"Sunday",52,55,null,19114,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39880,3,8,11,"Sunday",52,55,null,19115,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39880,3,8,12,"Sunday",52,56,null,19116,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39880,3,8,13,"Sunday",53,57,null,19117,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39880,3,8,14,"Sunday",50,53,null,19118,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39880,3,8,15,"Sunday",49,51,null,19119,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":71}]
[1,39880,3,8,16,"Sunday",50,54,null,19120,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":75}]
[1,{"$f":"DATE(2009,C1602,D1602)","v":39880},3,8,17,"Sunday",49,54,null,19121,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":71}]
[1,39880,3,8,18,"Sunday",48,50,null,19122,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39880,3,8,19,"Sunday",47,48,null,{"$f":"J1603+1","v":19123},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39880,3,8,20,"Sunday",46,47,null,19124,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39880,3,8,21,"Sunday",43,47,null,19125,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39880,3,8,22,"Sunday",42,45,null,19126,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39880,3,8,23,"Sunday",42,44,null,19127,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39880,3,8,24,"Sunday",42,44,null,19128,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39881,3,9,1,"Weekday",42,44,null,19129,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39881,3,9,2,"Weekday",41,43,null,19130,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39881,3,9,3,"Weekday",40,41,null,19131,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39881,3,9,4,"Weekday",40,41,null,19132,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39881,3,9,5,"Weekday",40,41,null,19133,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39881,3,9,6,"Weekday",41,42,null,19134,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39881,3,9,7,"Weekday",41,42,null,19135,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39881,3,9,8,"Weekday",42,43,null,19136,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39881,3,9,9,"Weekday",44,46,null,19137,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39881,3,9,10,"Weekday",46,48,null,19138,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39881,3,9,11,"Weekday",45,48,null,19139,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39881,3,9,12,"Weekday",48,52,null,19140,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39881,3,9,13,"Weekday",48,52,null,19141,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39881,3,9,14,"Weekday",48,54,null,19142,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39881,3,9,15,"Weekday",47,54,null,19143,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39881,3,9,16,"Weekday",45,50,null,19144,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39881,3,9,17,"Weekday",46,50,null,19145,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39881,3,9,18,"Weekday",46,49,null,19146,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39881,3,9,19,"Weekday",45,47,null,19147,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39881,3,9,20,"Weekday",44,46,null,19148,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39881,3,9,21,"Weekday",43,44,null,19149,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39881,3,9,22,"Weekday",43,44,null,19150,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39881,3,9,23,"Weekday",43,44,null,19151,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39881,3,9,24,"Weekday",42,43,null,19152,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39882,3,10,1,"Weekday",42,42,null,19153,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39882,3,10,2,"Weekday",41,42,null,19154,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,3,"Weekday",41,42,null,19155,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,4,"Weekday",42,42,null,19156,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,5,"Weekday",42,42,null,19157,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,6,"Weekday",42,42,null,19158,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,7,"Weekday",41,42,null,19159,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,8,"Weekday",41,42,null,19160,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39882,3,10,9,"Weekday",42,43,null,19161,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39882,3,10,10,"Weekday",43,44,null,19162,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39882,3,10,11,"Weekday",44,45,null,19163,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39882,3,10,12,"Weekday",45,46,null,19164,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39882,3,10,13,"Weekday",45,46,null,19165,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39882,3,10,14,"Weekday",45,46,null,19166,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39882,3,10,15,"Weekday",46,47,null,19167,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39882,3,10,16,"Weekday",47,49,null,19168,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39882,3,10,17,"Weekday",47,49,null,19169,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39882,3,10,18,"Weekday",46,47,null,19170,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39882,3,10,19,"Weekday",46,47,null,19171,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39882,3,10,20,"Weekday",46,47,null,19172,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39882,3,10,21,"Weekday",46,47,null,19173,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39882,3,10,22,"Weekday",46,47,null,19174,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39882,3,10,23,"Weekday",44,46,null,19175,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39882,3,10,24,"Weekday",44,45,null,19176,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39883,3,11,1,"Weekday",44,44,null,19177,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39883,3,11,2,"Weekday",44,44,null,19178,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39883,3,11,3,"Weekday",44,44,null,19179,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39883,3,11,4,"Weekday",43,44,null,19180,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39883,3,11,5,"Weekday",43,43,null,19181,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39883,3,11,6,"Weekday",43,43,null,19182,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39883,3,11,7,"Weekday",43,43,null,19183,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39883,3,11,8,"Weekday",44,45,null,19184,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,{"$f":"DATE(2009,C1666,D1666)","v":39883},3,11,9,"Weekday",48,50,null,19185,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39883,3,11,10,"Weekday",47,50,null,19186,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39883,3,11,11,"Weekday",49,53,null,{"$f":"J1667+1","v":19187},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39883,3,11,12,"Weekday",49,54,null,19188,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39883,3,11,13,"Weekday",50,56,null,19189,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39883,3,11,14,"Weekday",50,56,null,19190,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39883,3,11,15,"Weekday",48,53,null,19191,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39883,3,11,16,"Weekday",47,54,null,19192,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39883,3,11,17,"Weekday",46,52,null,19193,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39883,3,11,18,"Weekday",45,50,null,19194,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39883,3,11,19,"Weekday",43,47,null,19195,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39883,3,11,20,"Weekday",42,44,null,19196,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39883,3,11,21,"Weekday",39,40,null,19197,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39883,3,11,22,"Weekday",38,39,null,19198,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39883,3,11,23,"Weekday",38,39,null,19199,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39883,3,11,24,"Weekday",38,38,null,19200,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39884,3,12,1,"Weekday",38,38,null,19201,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39884,3,12,2,"Weekday",38,39,null,19202,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39884,3,12,3,"Weekday",38,39,null,19203,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,4,"Weekday",35,35,null,19204,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39884,3,12,5,"Weekday",36,37,null,19205,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39884,3,12,6,"Weekday",36,37,null,19206,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39884,3,12,7,"Weekday",35,36,null,19207,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,8,"Weekday",39,40,null,19208,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,9,"Weekday",43,47,null,19209,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,10,"Weekday",45,50,null,19210,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,11,"Weekday",46,52,null,19211,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39884,3,12,12,"Weekday",47,53,null,19212,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39884,3,12,13,"Weekday",47,54,null,19213,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39884,3,12,14,"Weekday",48,55,null,19214,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39884,3,12,15,"Weekday",50,56,null,19215,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,16,"Weekday",49,55,null,19216,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39884,3,12,17,"Weekday",47,52,null,19217,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39884,3,12,18,"Weekday",47,51,null,19218,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,19,"Weekday",44,47,null,19219,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,20,"Weekday",42,43,null,19220,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39884,3,12,21,"Weekday",41,41,null,19221,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39884,3,12,22,"Weekday",40,40,null,19222,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39884,3,12,23,"Weekday",38,38,null,19223,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39884,3,12,24,"Weekday",36,36,null,19224,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39885,3,13,1,"Weekday",35,35,null,19225,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39885,3,13,2,"Weekday",37,37,null,19226,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39885,3,13,3,"Weekday",39,41,null,19227,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39885,3,13,4,"Weekday",38,39,null,19228,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39885,3,13,5,"Weekday",36,37,null,19229,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39885,3,13,6,"Weekday",36,37,null,19230,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39885,3,13,7,"Weekday",36,37,null,19231,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39885,3,13,8,"Weekday",40,42,null,19232,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39885,3,13,9,"Weekday",45,51,null,19233,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39885,3,13,10,"Weekday",50,55,null,19234,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39885,3,13,11,"Weekday",49,54,null,19235,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39885,3,13,12,"Weekday",49,56,null,19236,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39885,3,13,13,"Weekday",49,53,null,19237,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39885,3,13,14,"Weekday",48,55,null,19238,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39885,3,13,15,"Weekday",51,57,null,19239,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39885,3,13,16,"Weekday",52,56,null,19240,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39885,3,13,17,"Weekday",50,53,null,19241,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39885,3,13,18,"Weekday",49,51,null,19242,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39885,3,13,19,"Weekday",47,47,null,19243,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39885,3,13,20,"Weekday",47,47,null,19244,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39885,3,13,21,"Weekday",47,47,null,19245,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39885,3,13,22,"Weekday",46,46,null,19246,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39885,3,13,23,"Weekday",44,45,null,19247,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39885,3,13,24,"Weekday",45,47,null,19248,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,{"$f":"DATE(2009,C1730,D1730)","v":39886},3,14,1,"Saturday",47,48,null,19249,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39886,3,14,2,"Saturday",44,48,null,19250,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39886,3,14,3,"Saturday",43,46,null,{"$f":"J1731+1","v":19251},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39886,3,14,4,"Saturday",42,44,null,19252,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39886,3,14,5,"Saturday",42,43,null,19253,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39886,3,14,6,"Saturday",40,41,null,19254,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39886,3,14,7,"Saturday",41,42,null,19255,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39886,3,14,8,"Saturday",48,50,null,19256,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39886,3,14,9,"Saturday",49,56,null,19257,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39886,3,14,10,"Saturday",50,57,null,19258,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39886,3,14,11,"Saturday",53,57,null,19259,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39886,3,14,12,"Saturday",52,55,null,19260,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39886,3,14,13,"Saturday",51,57,null,19261,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39886,3,14,14,"Saturday",52,57,null,19262,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39886,3,14,15,"Saturday",52,55,null,19263,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39886,3,14,16,"Saturday",51,54,null,19264,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39886,3,14,17,"Saturday",51,54,null,19265,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39886,3,14,18,"Saturday",50,53,null,19266,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39886,3,14,19,"Saturday",50,51,null,19267,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39886,3,14,20,"Saturday",50,51,null,19268,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39886,3,14,21,"Saturday",47,48,null,19269,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39886,3,14,22,"Saturday",47,47,null,19270,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39886,3,14,23,"Saturday",47,47,null,19271,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39886,3,14,24,"Saturday",48,48,null,19272,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39887,3,15,1,"Sunday",48,49,null,19273,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39887,3,15,2,"Sunday",48,49,null,19274,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39887,3,15,3,"Sunday",48,48,null,19275,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39887,3,15,4,"Sunday",48,48,null,19276,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39887,3,15,5,"Sunday",48,48,null,19277,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39887,3,15,6,"Sunday",48,48,null,19278,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39887,3,15,7,"Sunday",48,48,null,19279,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":40},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39887,3,15,8,"Sunday",48,48,null,19280,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39887,3,15,9,"Sunday",50,52,null,19281,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39887,3,15,10,"Sunday",52,57,null,19282,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39887,3,15,11,"Sunday",50,57,null,19283,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39887,3,15,12,"Sunday",52,60,null,19284,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39887,3,15,13,"Sunday",52,54,null,19285,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":74}]
[1,39887,3,15,14,"Sunday",52,55,null,19286,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":70}]
[1,39887,3,15,15,"Sunday",52,56,null,19287,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39887,3,15,16,"Sunday",51,56,null,19288,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39887,3,15,17,"Sunday",51,55,null,19289,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39887,3,15,18,"Sunday",50,53,null,19290,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39887,3,15,19,"Sunday",48,51,null,19291,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39887,3,15,20,"Sunday",47,48,null,19292,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39887,3,15,21,"Sunday",47,48,null,19293,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39887,3,15,22,"Sunday",47,48,null,19294,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39887,3,15,23,"Sunday",47,47,null,19295,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39887,3,15,24,"Sunday",45,46,null,19296,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39888,3,16,1,"Weekday",45,46,null,19297,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39888,3,16,2,"Weekday",45,46,null,19298,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39888,3,16,3,"Weekday",46,47,null,19299,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39888,3,16,4,"Weekday",46,47,null,19300,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39888,3,16,5,"Weekday",47,50,null,19301,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39888,3,16,6,"Weekday",48,51,null,19302,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39888,3,16,7,"Weekday",48,51,null,19303,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39888,3,16,8,"Weekday",50,54,null,19304,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39888,3,16,9,"Weekday",51,56,null,19305,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39888,3,16,10,"Weekday",53,59,null,19306,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39888,3,16,11,"Weekday",55,63,null,19307,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39888,3,16,12,"Weekday",56,65,null,19308,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,13,"Weekday",55,64,null,19309,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39888,3,16,14,"Weekday",54,58,null,19310,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39888,3,16,15,"Weekday",53,56,null,19311,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39888,3,16,16,"Weekday",52,54,null,19312,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,{"$f":"DATE(2009,C1794,D1794)","v":39888},3,16,17,"Weekday",52,54,null,19313,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,18,"Weekday",53,54,null,19314,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,19,"Weekday",51,51,null,{"$f":"J1795+1","v":19315},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,20,"Weekday",51,51,null,19316,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,21,"Weekday",50,51,null,19317,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,22,"Weekday",50,51,null,19318,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39888,3,16,23,"Weekday",50,51,null,19319,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39888,3,16,24,"Weekday",49,50,null,19320,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39889,3,17,1,"Weekday",48,48,null,19321,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39889,3,17,2,"Weekday",46,47,null,19322,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39889,3,17,3,"Weekday",46,46,null,19323,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39889,3,17,4,"Weekday",45,46,null,19324,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39889,3,17,5,"Weekday",41,41,null,19325,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39889,3,17,6,"Weekday",41,42,null,19326,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39889,3,17,7,"Weekday",43,44,null,19327,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39889,3,17,8,"Weekday",49,52,null,19328,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39889,3,17,9,"Weekday",56,60,null,19329,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39889,3,17,10,"Weekday",58,65,null,19330,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39889,3,17,11,"Weekday",57,62,null,19331,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39889,3,17,12,"Weekday",58,65,null,19332,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39889,3,17,13,"Weekday",59,67,null,19333,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39889,3,17,14,"Weekday",58,68,null,19334,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39889,3,17,15,"Weekday",58,68,null,19335,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39889,3,17,16,"Weekday",57,62,null,19336,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39889,3,17,17,"Weekday",56,62,null,19337,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39889,3,17,18,"Weekday",56,59,null,19338,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39889,3,17,19,"Weekday",52,53,null,19339,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39889,3,17,20,"Weekday",49,51,null,19340,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39889,3,17,21,"Weekday",48,48,null,19341,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39889,3,17,22,"Weekday",45,46,null,19342,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39889,3,17,23,"Weekday",45,45,null,19343,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39889,3,17,24,"Weekday",45,46,null,19344,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39890,3,18,1,"Weekday",46,46,null,19345,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39890,3,18,2,"Weekday",44,44,null,19346,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39890,3,18,3,"Weekday",41,41,null,19347,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39890,3,18,4,"Weekday",41,41,null,19348,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39890,3,18,5,"Weekday",40,40,null,19349,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39890,3,18,6,"Weekday",39,39,null,19350,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39890,3,18,7,"Weekday",38,38,null,19351,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39890,3,18,8,"Weekday",47,48,null,19352,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39890,3,18,9,"Weekday",52,53,null,19353,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39890,3,18,10,"Weekday",55,59,null,19354,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39890,3,18,11,"Weekday",55,59,null,19355,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39890,3,18,12,"Weekday",57,62,null,19356,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39890,3,18,13,"Weekday",59,64,null,19357,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39890,3,18,14,"Weekday",59,63,null,19358,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39890,3,18,15,"Weekday",58,62,null,19359,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39890,3,18,16,"Weekday",58,62,null,19360,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39890,3,18,17,"Weekday",55,55,null,19361,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39890,3,18,18,"Weekday",55,58,null,19362,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39890,3,18,19,"Weekday",53,54,null,19363,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39890,3,18,20,"Weekday",49,50,null,19364,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39890,3,18,21,"Weekday",53,54,null,19365,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39890,3,18,22,"Weekday",53,54,null,19366,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39890,3,18,23,"Weekday",52,53,null,19367,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39890,3,18,24,"Weekday",51,52,null,19368,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39891,3,19,1,"Weekday",50,51,null,19369,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39891,3,19,2,"Weekday",49,50,null,19370,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39891,3,19,3,"Weekday",49,50,null,19371,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39891,3,19,4,"Weekday",49,49,null,19372,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39891,3,19,5,"Weekday",49,49,null,19373,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39891,3,19,6,"Weekday",48,49,null,19374,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39891,3,19,7,"Weekday",48,48,null,19375,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45}]
[1,39891,3,19,8,"Weekday",48,48,null,19376,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,{"$f":"DATE(2009,C1858,D1858)","v":39891},3,19,9,"Weekday",50,51,null,19377,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39891,3,19,10,"Weekday",51,52,null,19378,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39891,3,19,11,"Weekday",52,53,null,{"$f":"J1859+1","v":19379},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39891,3,19,12,"Weekday",52,53,null,19380,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39891,3,19,13,"Weekday",52,53,null,19381,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39891,3,19,14,"Weekday",51,52,null,19382,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39891,3,19,15,"Weekday",51,52,null,19383,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39891,3,19,16,"Weekday",51,52,null,19384,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39891,3,19,17,"Weekday",50,50,null,19385,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39891,3,19,18,"Weekday",49,49,null,19386,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39891,3,19,19,"Weekday",48,48,null,19387,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39891,3,19,20,"Weekday",47,47,null,19388,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39891,3,19,21,"Weekday",47,47,null,19389,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39891,3,19,22,"Weekday",47,48,null,19390,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39891,3,19,23,"Weekday",48,49,null,19391,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39891,3,19,24,"Weekday",48,49,null,19392,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39892,3,20,1,"Weekday",47,48,null,19393,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39892,3,20,2,"Weekday",46,47,null,19394,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39892,3,20,3,"Weekday",46,46,null,19395,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39892,3,20,4,"Weekday",43,44,null,19396,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39892,3,20,5,"Weekday",43,43,null,19397,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39892,3,20,6,"Weekday",44,44,null,19398,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39892,3,20,7,"Weekday",45,45,null,19399,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39892,3,20,8,"Weekday",47,48,null,19400,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39892,3,20,9,"Weekday",49,50,null,19401,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39892,3,20,10,"Weekday",51,52,null,19402,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39892,3,20,11,"Weekday",51,53,null,19403,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39892,3,20,12,"Weekday",52,55,null,19404,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39892,3,20,13,"Weekday",51,55,null,19405,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,39892,3,20,14,"Weekday",51,56,null,19406,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39892,3,20,15,"Weekday",50,56,null,19407,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39892,3,20,16,"Weekday",50,55,null,19408,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39892,3,20,17,"Weekday",48,54,null,19409,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39892,3,20,18,"Weekday",48,52,null,19410,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39892,3,20,19,"Weekday",46,49,null,19411,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39892,3,20,20,"Weekday",46,50,null,19412,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39892,3,20,21,"Weekday",46,49,null,19413,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39892,3,20,22,"Weekday",44,45,null,19414,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39892,3,20,23,"Weekday",41,42,null,19415,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39892,3,20,24,"Weekday",41,41,null,19416,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39893,3,21,1,"Saturday",41,41,null,19417,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39893,3,21,2,"Saturday",40,41,null,19418,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39893,3,21,3,"Saturday",39,40,null,19419,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39893,3,21,4,"Saturday",39,40,null,19420,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39893,3,21,5,"Saturday",38,38,null,19421,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39893,3,21,6,"Saturday",39,39,null,19422,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39893,3,21,7,"Saturday",40,41,null,19423,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39893,3,21,8,"Saturday",44,46,null,19424,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39893,3,21,9,"Saturday",45,48,null,19425,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39893,3,21,10,"Saturday",46,51,null,19426,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39893,3,21,11,"Saturday",48,54,null,19427,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39893,3,21,12,"Saturday",49,52,null,19428,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39893,3,21,13,"Saturday",48,50,null,19429,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39893,3,21,14,"Saturday",49,50,null,19430,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39893,3,21,15,"Saturday",48,49,null,19431,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,39893,3,21,16,"Saturday",48,49,null,19432,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":70}]
[1,39893,3,21,17,"Saturday",47,49,null,19433,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,39893,3,21,18,"Saturday",47,48,null,19434,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39893,3,21,19,"Saturday",47,48,null,19435,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39893,3,21,20,"Saturday",47,48,null,19436,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39893,3,21,21,"Saturday",47,49,null,19437,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39893,3,21,22,"Saturday",48,50,null,19438,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39893,3,21,23,"Saturday",49,50,null,19439,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39893,3,21,24,"Saturday",49,49,null,19440,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,{"$f":"DATE(2009,C1922,D1922)","v":39894},3,22,1,"Sunday",48,48,null,19441,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39894,3,22,2,"Sunday",48,48,null,19442,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39894,3,22,3,"Sunday",47,48,null,{"$f":"J1923+1","v":19443},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39894,3,22,4,"Sunday",45,45,null,19444,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39894,3,22,5,"Sunday",45,46,null,19445,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39894,3,22,6,"Sunday",43,44,null,19446,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39894,3,22,7,"Sunday",45,45,null,19447,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39894,3,22,8,"Sunday",47,47,null,19448,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39894,3,22,9,"Sunday",45,46,null,19449,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39894,3,22,10,"Sunday",47,48,null,19450,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39894,3,22,11,"Sunday",49,50,null,19451,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39894,3,22,12,"Sunday",46,48,null,19452,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39894,3,22,13,"Sunday",48,51,null,19453,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39894,3,22,14,"Sunday",51,56,null,19454,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39894,3,22,15,"Sunday",49,54,null,19455,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39894,3,22,16,"Sunday",46,47,null,19456,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39894,3,22,17,"Sunday",47,48,null,19457,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39894,3,22,18,"Sunday",46,47,null,19458,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39894,3,22,19,"Sunday",45,45,null,19459,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39894,3,22,20,"Sunday",45,45,null,19460,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39894,3,22,21,"Sunday",45,46,null,19461,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39894,3,22,22,"Sunday",45,45,null,19462,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39894,3,22,23,"Sunday",44,44,null,19463,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39894,3,22,24,"Sunday",44,44,null,19464,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39895,3,23,1,"Weekday",44,45,null,19465,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39895,3,23,2,"Weekday",43,44,null,19466,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39895,3,23,3,"Weekday",42,43,null,19467,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39895,3,23,4,"Weekday",42,43,null,19468,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39895,3,23,5,"Weekday",43,44,null,19469,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39895,3,23,6,"Weekday",43,44,null,19470,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39895,3,23,7,"Weekday",43,44,null,19471,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39895,3,23,8,"Weekday",46,47,null,19472,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39895,3,23,9,"Weekday",48,50,null,19473,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39895,3,23,10,"Weekday",50,54,null,19474,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39895,3,23,11,"Weekday",50,56,null,19475,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39895,3,23,12,"Weekday",50,57,null,19476,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39895,3,23,13,"Weekday",51,57,null,19477,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39895,3,23,14,"Weekday",50,54,null,19478,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39895,3,23,15,"Weekday",50,55,null,19479,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39895,3,23,16,"Weekday",51,56,null,19480,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39895,3,23,17,"Weekday",50,54,null,19481,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39895,3,23,18,"Weekday",49,54,null,19482,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39895,3,23,19,"Weekday",48,53,null,19483,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39895,3,23,20,"Weekday",48,50,null,19484,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39895,3,23,21,"Weekday",48,50,null,19485,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39895,3,23,22,"Weekday",48,49,null,19486,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39895,3,23,23,"Weekday",48,49,null,19487,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39895,3,23,24,"Weekday",46,50,null,19488,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39896,3,24,1,"Weekday",46,51,null,19489,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39896,3,24,2,"Weekday",47,52,null,19490,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39896,3,24,3,"Weekday",47,52,null,19491,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39896,3,24,4,"Weekday",48,52,null,19492,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39896,3,24,5,"Weekday",48,52,null,19493,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,39896,3,24,6,"Weekday",48,52,null,19494,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43}]
[1,39896,3,24,7,"Weekday",48,54,null,19495,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":38},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42}]
[1,39896,3,24,8,"Weekday",49,54,null,19496,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39896,3,24,9,"Weekday",49,55,null,19497,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39896,3,24,10,"Weekday",51,56,null,19498,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39896,3,24,11,"Weekday",52,58,null,19499,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39896,3,24,12,"Weekday",52,58,null,19500,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39896,3,24,13,"Weekday",53,58,null,19501,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39896,3,24,14,"Weekday",52,55,null,19502,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39896,3,24,15,"Weekday",53,55,null,19503,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39896,3,24,16,"Weekday",53,55,null,19504,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,{"$f":"DATE(2009,C1986,D1986)","v":39896},3,24,17,"Weekday",54,56,null,19505,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39896,3,24,18,"Weekday",53,56,null,19506,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39896,3,24,19,"Weekday",53,55,null,{"$f":"J1987+1","v":19507},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39896,3,24,20,"Weekday",52,55,null,19508,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39896,3,24,21,"Weekday",52,55,null,19509,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,39896,3,24,22,"Weekday",53,56,null,19510,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39896,3,24,23,"Weekday",53,56,null,19511,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39896,3,24,24,"Weekday",53,56,null,19512,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39897,3,25,1,"Weekday",53,56,null,19513,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39897,3,25,2,"Weekday",54,57,null,19514,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39897,3,25,3,"Weekday",55,59,null,19515,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39897,3,25,4,"Weekday",56,59,null,19516,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50}]
[1,39897,3,25,5,"Weekday",54,56,null,19517,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,39897,3,25,6,"Weekday",56,59,null,19518,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47}]
[1,39897,3,25,7,"Weekday",56,59,null,19519,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39898,3,26,21,"Weekday",56,57,null,19557,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39901,3,29,8,"Sunday",48,48,null,19616,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":39},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,39903,3,31,5,"Weekday",46,46,null,19661,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39907,4,4,12,"Saturday",52,62,null,19764,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39909,4,6,9,"Weekday",50,54,null,19809,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39912,4,9,14,"Weekday",50,57,null,19886,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39915,4,12,12,"Sunday",52,63,null,19956,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39917,4,14,9,"Weekday",48,50,null,20001,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39921,4,18,16,"Saturday",49,52,null,20104,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,39923,4,20,13,"Weekday",54,58,null,20149,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":71}]
[1,39928,4,25,7,"Saturday",45,50,null,20263,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39929,4,26,5,"Sunday",46,47,null,20285,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":5},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,39934,5,1,10,"Weekday",54,58,null,20410,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,39936,5,3,7,"Sunday",53,56,null,20455,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39937,5,4,17,"Weekday",53,57,null,20489,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61}]
[1,39942,5,9,11,"Saturday",58,61,null,20603,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,39943,5,10,21,"Sunday",51,53,null,20637,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39946,5,13,12,"Weekday",51,54,null,20700,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":79}]
[1,39950,5,17,11,"Sunday",54,56,null,20795,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,39951,5,18,21,"Weekday",48,51,null,20829,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39956,5,23,15,"Saturday",56,60,null,20943,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63}]
[1,{"$f":"DATE(2009,C3458,D3458)","v":39958},5,25,1,"Weekday",51,53,null,20977,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,39962,5,29,19,"Weekday",51,56,null,21091,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,39963,5,30,19,"Saturday",52,56,null,21115,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39968,6,4,22,"Weekday",55,57,null,21238,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39970,6,6,19,"Saturday",55,56,null,21283,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,39972,6,8,16,"Weekday",56,62,null,21328,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":70},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":83}]
[1,39976,6,12,23,"Weekday",49,50,null,21431,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39978,6,14,20,"Sunday",56,60,null,21476,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,39983,6,19,6,"Weekday",55,55,null,21582,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,39984,6,20,23,"Saturday",51,52,null,21623,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,39986,6,22,20,"Weekday",64,65,null,21668,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,39991,6,27,3,"Saturday",49,51,null,21771,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,39992,6,28,24,"Sunday",45,46,null,21816,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,39994,6,30,21,"Weekday",54,57,null,21861,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":21},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,39997,7,3,17,"Weekday",57,61,null,21929,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":17},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,40000,7,6,24,"Weekday",48,49,null,22008,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,40005,7,11,7,"Saturday",55,58,null,22111,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,40007,7,13,4,"Weekday",54,57,null,22156,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,40011,7,17,22,"Weekday",51,53,null,22270,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,40013,7,19,8,"Sunday",56,58,null,22304,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,40014,7,20,24,"Weekday",54,56,null,22344,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,40019,7,25,11,"Saturday",55,58,null,{"$f":"J4931+1","v":22451},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,40021,7,27,8,"Weekday",55,58,null,22496,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,40026,8,1,2,"Saturday",53,53,null,22610,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,40027,8,2,12,"Sunday",60,63,null,22644,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":71}]
[1,40029,8,4,9,"Weekday",55,57,null,22689,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":9},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,40032,8,7,7,"Weekday",55,56,null,22759,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,40035,8,10,12,"Weekday",58,60,null,22836,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":70}]
[1,40040,8,15,6,"Saturday",56,57,null,22950,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,40041,8,16,16,"Sunday",61,65,null,22984,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":78}]
[1,40046,8,21,10,"Weekday",55,55,null,23098,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,40048,8,23,7,"Sunday",54,54,null,23143,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,40051,8,26,18,"Weekday",60,64,null,23226,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":61},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":71}]
[1,40054,8,29,10,"Saturday",62,66,null,23290,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,40055,8,30,20,"Sunday",56,59,null,23324,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62}]
[1,40060,9,4,14,"Weekday",59,68,null,23438,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":73}]
[1,40062,9,6,11,"Sunday",58,64,null,23483,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":74}]
[1,40065,9,9,11,"Weekday",58,62,null,23555,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":65}]
[1,40068,9,12,14,"Saturday",57,60,null,23630,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":14},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":62},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":72}]
[1,40070,9,14,11,"Weekday",59,64,null,23675,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":68}]
[1,40074,9,18,18,"Weekday",58,62,null,23778,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,40076,9,20,15,"Sunday",60,64,null,23823,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":67}]
[1,{"$f":"DATE(2009,C6338,D6338)","v":40078},9,22,1,"Weekday",49,50,null,23857,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,40082,9,26,18,"Saturday",56,56,null,23970,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":18},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":74}]
[1,40084,9,28,15,"Weekday",61,67,null,24015,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":15},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":63},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":89}]
[1,40088,10,2,22,"Weekday",50,51,null,24118,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":59}]
[1,40090,10,4,19,"Sunday",54,54,null,24163,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":19},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,40092,10,6,16,"Weekday",57,61,null,24208,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":78}]
[1,40096,10,10,23,"Saturday",50,51,null,24311,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69}]
[1,40100,10,14,1,"Weekday",52,52,null,24385,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,40103,10,17,2,"Saturday",51,51,null,24458,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,40104,10,18,23,"Sunday",55,58,null,24503,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,40106,10,20,20,"Weekday",50,51,null,24548,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":64}]
[1,40111,10,25,3,"Sunday",44,45,null,24651,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,40112,10,26,24,"Weekday",52,53,null,24696,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57}]
[1,40116,10,30,16,"Weekday",59,61,null,24784,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":69},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":85}]
[1,40119,11,2,3,"Weekday",42,43,null,24843,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":3},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,40120,11,3,24,"Weekday",42,43,null,24888,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":24},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,40125,11,8,7,"Sunday",36,40,null,24991,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":7},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,40127,11,10,4,"Weekday",39,41,null,25036,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":4},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,40131,11,14,22,"Saturday",52,56,null,25150,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":22},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":57},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":60}]
[1,40133,11,16,23,"Weekday",44,50,null,25199,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":23},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51}]
[1,40138,11,21,1,"Saturday",44,48,null,25297,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":1},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,40139,11,22,11,"Sunday",44,48,null,{"$f":"J7811+1","v":25331},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":11},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":55}]
[1,40141,11,24,8,"Weekday",39,41,null,25376,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":8},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[1,40146,11,29,2,"Sunday",45,48,null,25490,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":42},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":44}]
[1,40147,11,30,12,"Weekday",54,61,null,25524,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":43},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":56}]
[1,40151,12,4,6,"Weekday",55,59,null,25614,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":52}]
[1,40154,12,7,2,"Weekday",43,43,null,25682,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":2},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":51},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,40155,12,8,12,"Weekday",58,62,null,25716,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":12},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":50},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54}]
[1,40160,12,13,6,"Sunday",46,48,null,25830,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":6},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":48}]
[1,40161,12,14,16,"Weekday",46,55,null,25864,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":16},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":54},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":58}]
[1,40166,12,19,10,"Saturday",45,45,null,25978,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Saturday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,40168,12,21,13,"Weekday",56,56,null,26029,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":66}]
[1,40172,12,25,13,"Weekday",53,58,null,26125,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":13},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":47},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":49}]
[1,40174,12,27,10,"Sunday",50,52,null,26170,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":10},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Sunday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":45},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":53}]
[1,40175,12,28,20,"Weekday",43,44,null,26204,{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Hour]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":20},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Weekday]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":"Weekday"},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Wet_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":41},{"$f":"OFFSET(tbl_Climate_Zones[[#Headers],[Dry_Bulb]],tbl_Climate_Zone[[#This Row],[First_Line]],0)","v":46}]
[2,39815,1,2,14,"Weekday",49,57]
[2,39817,1,4,11,"Sunday",46,46]
[2,39820,1,7,4,"Weekday",40,40]
[2,39823,1,10,14,"Saturday",45,55]
[2,39825,1,12,11,"Weekday",36,41]
[2,39829,1,16,18,"Weekday",40,44]
[2,39831,1,18,15,"Sunday",45,56]
[2,39835,1,22,22,"Weekday",41,42]
[2,39837,1,24,11,"Saturday",44,44]
[2,39839,1,26,15,"Weekday",47,54]
[2,39843,1,30,22,"Weekday",61,62]
[2,39845,2,1,19,"Sunday",45,47]
[2,39850,2,6,2,"Weekday",35,36]
[2,39851,2,7,23,"Saturday",44,45]
[2,39854,2,10,18,"Weekday",50,55]
[2,39858,2,14,2,"Saturday",40,40]
[2,39859,2,15,23,"Sunday",43,45]
[2,39864,2,20,17,"Weekday",50,52]
[2,39866,2,22,3,"Sunday",49,50]
[2,39868,2,24,11,"Weekday",56,61]
[2,39872,2,28,6,"Saturday",47,48]
[2,39874,3,2,3,"Weekday",45,50]
[2,39878,3,6,21,"Weekday",56,58]
[2,39880,3,8,7,"Sunday",52,52]
[2,39885,3,13,1,"Weekday",40,43]
[2,39885,3,13,18,"Weekday",47,53]
[2,39888,3,16,7,"Weekday",35,35]
[2,39893,3,21,1,"Saturday",41,45]
[2,39894,3,22,11,"Sunday",50,62]
[2,39899,3,27,5,"Weekday",41,42]
[2,39901,3,29,2,"Sunday",51,54]
[2,{"$f":"DATE(2009,C10882,D10882)","v":39902},3,30,9,"Weekday",50,53]
[2,39907,4,4,5,"Saturday",42,43]
[2,39908,4,5,15,"Sunday",47,49]
[2,39913,4,10,9,"Weekday",54,62]
[2,39915,4,12,6,"Sunday",44,45]
[2,39916,4,13,16,"Weekday",58,73]
[2,39919,4,16,16,"Weekday",57,73]
[2,39923,4,20,6,"Weekday",46,47]
[2,39927,4,24,13,"Weekday",49,68]
[2,39929,4,26,10,"Sunday",48,59]
[2,39933,4,30,17,"Weekday",57,81]
[2,39935,5,2,14,"Saturday",61,74]
[2,39936,5,3,23,"Sunday",48,51]
[2,39941,5,8,17,"Weekday",51,60]
[2,39943,5,10,14,"Sunday",53,57]
[2,39947,5,14,21,"Weekday",50,55]
[2,39949,5,16,18,"Saturday",66,83]
[2,39951,5,18,15,"Weekday",62,88]
[2,39956,5,23,10,"Saturday",57,62]
[2,39957,5,24,18,"Sunday",60,67]
[2,39959,5,26,15,"Weekday",64,82]
[2,39963,5,30,22,"Saturday",53,63]
[2,39965,6,1,19,"Weekday",55,69]
[2,39970,6,6,2,"Saturday",45,49]
[2,39973,6,9,17,"Weekday",61,79]
[2,39976,6,12,16,"Weekday",63,76]
[2,39978,6,14,2,"Sunday",53,56]
[2,39979,6,15,23,"Weekday",58,69]
[2,39984,6,20,17,"Saturday",56,69]
[2,39986,6,22,3,"Weekday",46,51]
[2,39990,6,26,24,"Weekday",50,53]
[2,39992,6,28,6,"Sunday",47,53]
[2,39994,6,30,3,"Weekday",46,48]
[2,39998,7,4,21,"Saturday",51,58]
[2,40000,7,6,7,"Weekday",53,59]
[2,40005,7,11,1,"Saturday",50,58]
[2,40007,7,13,15,"Weekday",58,68]
[2,40011,7,17,4,"Weekday",51,55]
[2,40013,7,19,1,"Sunday",55,66]
[2,40014,7,20,11,"Weekday",63,86]
[2,40019,7,25,5,"Saturday",51,56]
[2,40021,7,27,2,"Weekday",49,51]
[2,40024,7,30,22,"Weekday",53,63]
[2,40027,8,2,5,"Sunday",47,50]
[2,40028,8,3,15,"Weekday",59,69]
[2,40033,8,8,9,"Saturday",56,61]
[2,40035,8,10,6,"Weekday",51,53]
[2,40038,8,13,15,"Weekday",63,89]
[2,40041,8,16,9,"Sunday",59,73]
[2,40043,8,18,6,"Weekday",49,53]
[2,40047,8,22,13,"Saturday",65,87]
[2,40049,8,24,10,"Weekday",58,68]
[2,40053,8,28,17,"Weekday",55,84]
[2,40055,8,30,22,"Sunday",54,64]
[2,40057,9,1,10,"Weekday",59,76]
[2,40061,9,5,17,"Saturday",65,87]
[2,40063,9,7,14,"Weekday",61,82]
[2,40067,9,11,21,"Weekday",51,60]
[2,40069,9,13,18,"Sunday",58,70]
[2,40073,9,17,5,"Weekday",47,56]
[2,40075,9,19,21,"Saturday",49,55]
[2,40077,9,21,18,"Weekday",55,77]
[2,40082,9,26,12,"Saturday",56,70]
[2,40083,9,27,22,"Sunday",51,53]
[2,40088,10,2,16,"Weekday",60,89]
[2,40089,10,3,20,"Saturday",54,69]
[2,40091,10,5,22,"Weekday",53,63]
[2,40096,10,10,16,"Saturday",55,61]
[2,40098,10,12,2,"Weekday",49,51]
[2,40102,10,16,20,"Weekday",53,69]
[2,40104,10,18,6,"Sunday",49,52]
[2,40107,10,21,3,"Weekday",42,44]
[2,40110,10,24,20,"Saturday",49,56]
[2,40112,10,26,6,"Weekday",48,51]
[2,40116,10,30,24,"Weekday",42,45]
[2,40118,11,1,21,"Sunday",55,57]
[2,40120,11,3,7,"Weekday",35,38]
[2,40124,11,7,10,"Saturday",42,44]
[2,40126,11,9,10,"Weekday",51,53]
[2,40131,11,14,4,"Saturday",49,54]
[2,40133,11,16,1,"Weekday",41,42]
[2,40137,11,20,8,"Weekday",57,58]
[2,40139,11,22,5,"Sunday",35,35]
[2,40141,11,24,17,"Weekday",52,58]
[2,40145,11,28,8,"Saturday",35,35]
[2,40147,11,30,5,"Weekday",32,32]
[2,40151,12,4,12,"Weekday",41,43]
[2,40153,12,6,9,"Sunday",41,42]
[2,40155,12,8,6,"Weekday",36,36]
[2,40158,12,11,8,"Weekday",31,31]
[2,40161,12,14,9,"Weekday",42,43]
[2,40165,12,18,16,"Weekday",47,51]
[2,40167,12,20,13,"Sunday",55,58]
[2,40169,12,22,10,"Weekday",38,38]
[2,40173,12,26,17,"Saturday",46,51]
[2,40175,12,28,15,"Weekday",51,51]
[3,39815,1,2,7,"Weekday",32,40]
[3,39816,1,3,17,"Saturday",41,41]
[3,39818,1,5,14,"Weekday",46,48]
[3,39822,1,9,21,"Weekday",46,48]
[3,39824,1,11,18,"Sunday",51,52]
[3,39827,1,14,22,"Weekday",53,54]
[3,39830,1,17,21,"Saturday",52,52]
[3,39832,1,19,18,"Weekday",49,51]
[3,39837,1,24,12,"Saturday",52,62]
[3,39838,1,25,22,"Sunday",46,46]
[3,39841,1,28,15,"Weekday",53,58]
[3,39845,2,1,1,"Sunday",48,51]
[3,39849,2,5,19,"Weekday",54,56]
[3,39851,2,7,16,"Saturday",56,59]
[3,39853,2,9,2,"Weekday",53,54]
[3,39857,2,13,20,"Weekday",49,52]
[3,39861,2,17,2,"Weekday",40,46]
[3,39863,2,19,23,"Weekday",48,52]
[3,39865,2,21,20,"Saturday",41,55]
[3,39867,2,23,6,"Weekday",37,41]
[3,39871,2,27,24,"Weekday",49,50]
[3,39873,3,1,21,"Sunday",57,60]
[3,39878,3,6,9,"Weekday",45,50]
[3,39879,3,7,24,"Saturday",45,48]
[3,39881,3,9,10,"Weekday",47,51]
[3,39886,3,14,4,"Saturday",39,42]
[3,39888,3,16,1,"Weekday",59,62]
[3,39892,3,20,8,"Weekday",48,52]
[3,39895,3,23,16,"Weekday",52,63]
[3,39898,3,26,11,"Weekday",51,58]
[3,39900,3,28,8,"Saturday",49,54]
[3,39902,3,30,5,"Weekday",45,51]
[3,39906,4,3,12,"Weekday",51,58]
[3,39908,4,5,9,"Sunday",47,50]
[3,39910,4,7,3,"Weekday",41,43]
[3,39914,4,11,12,"Saturday",56,60]
[3,39916,4,13,9,"Weekday",47,55]
[3,39920,4,17,16,"Weekday",57,61]
[3,39922,4,19,13,"Sunday",58,66]
[3,39927,4,24,7,"Weekday",47,52]
[3,39929,4,26,14,"Sunday",66,76]
[3,39930,4,27,13,"Weekday",67,75]
[3,39935,5,2,7,"Saturday",47,52]
[3,39936,5,3,17,"Sunday",56,61]
[3,39941,5,8,11,"Weekday",54,63]
[3,39942,5,9,21,"Saturday",52,55]
[3,39946,5,13,21,"Weekday",52,56]
[3,39949,5,16,11,"Saturday",57,61]
[3,39950,5,17,21,"Sunday",52,56]
[3,39955,5,22,15,"Weekday",60,67]
[3,39957,5,24,1,"Sunday",49,51]
[3,39958,5,25,22,"Weekday",49,51]
[3,39964,5,31,4,"Sunday",52,53]
[3,39965,6,1,1,"Weekday",53,56]
[3,39969,6,5,19,"Weekday",58,61]
[3,39971,6,7,16,"Sunday",63,71]
[3,39975,6,11,23,"Weekday",51,53]
[3,39977,6,13,20,"Saturday",57,60]
[3,39980,6,16,19,"Weekday",56,60]
[3,39983,6,19,23,"Weekday",52,54]
[3,39985,6,21,20,"Sunday",53,56]
[3,39990,6,26,3,"Weekday",46,54]
[3,39991,6,27,24,"Saturday",52,56]
[3,39993,6,29,10,"Weekday",57,64]
[3,39998,7,4,2,"Saturday",51,53]
[3,39999,7,5,24,"Sunday",51,53]
[3,40004,7,10,7,"Weekday",52,53]
[3,40006,7,12,4,"Sunday",54,55]
[3,40008,7,14,1,"Weekday",57,59]
[3,40011,7,17,19,"Weekday",60,68]
[3,40014,7,20,4,"Weekday",53,55]
[3,40018,7,24,11,"Weekday",61,66]
[3,40020,7,26,8,"Sunday",54,57]
[3,40022,7,28,5,"Weekday",55,58]
[3,40026,8,1,12,"Saturday",64,73]
[3,40029,8,4,2,"Weekday",51,53]
[3,40033,8,8,2,"Saturday",52,56]
[3,40034,8,9,12,"Sunday",64,73]
[3,40036,8,11,9,"Weekday",56,60]
[3,40040,8,15,16,"Saturday",67,76]
[3,40042,8,17,13,"Weekday",68,81]
[3,40046,8,21,9,"Weekday",55,59]
[3,40048,8,23,16,"Sunday",63,71]
[3,40053,8,28,10,"Weekday",58,63]
[3,40054,8,29,20,"Saturday",58,62]
[3,40056,8,31,17,"Weekday",60,64]
[3,40061,9,5,11,"Saturday",61,70]
[3,40062,9,6,24,"Sunday",57,60]
[3,40067,9,11,14,"Weekday",64,78]
[3,40069,9,13,11,"Sunday",57,66]
[3,40070,9,14,21,"Weekday",57,61]
[3,40075,9,19,15,"Saturday",65,74]
[3,40077,9,21,1,"Weekday",56,57]
[3,40080,9,24,7,"Weekday",55,55]
[3,40083,9,27,15,"Sunday",66,83]
[3,40085,9,29,1,"Weekday",50,70]
[3,40089,10,3,19,"Saturday",52,73]
[3,40091,10,5,16,"Weekday",65,87]
[3,40095,10,9,23,"Weekday",57,62]
[3,40097,10,11,14,"Sunday",58,83]
[3,40102,10,16,2,"Weekday",59,60]
[3,40103,10,17,23,"Saturday",52,54]
[3,40105,10,19,20,"Weekday",57,60]
[3,40110,10,24,3,"Saturday",56,59]
[3,40111,10,25,24,"Sunday",54,55]
[3,40114,10,28,5,"Weekday",49,50]
[3,40118,11,1,3,"Sunday",48,52]
[3,40119,11,2,24,"Weekday",48,50]
[3,40124,11,7,7,"Saturday",52,55]
[3,40126,11,9,4,"Weekday",56,57]
[3,40130,11,13,22,"Weekday",51,54]
[3,40131,11,14,12,"Saturday",52,60]
[3,40134,11,17,4,"Weekday",43,44]
[3,40138,11,21,11,"Saturday",55,62]
[3,40140,11,23,8,"Weekday",45,49]
[3,40145,11,28,2,"Saturday",45,52]
[3,40146,11,29,12,"Sunday",44,60]
[3,40148,12,1,19,"Weekday",55,57]
[3,40152,12,5,15,"Saturday",52,53]
[3,40154,12,7,12,"Weekday",54,57]
[3,40159,12,12,6,"Saturday",46,48]
[3,40160,12,13,16,"Sunday",56,59]
[3,40162,12,15,13,"Weekday",54,59]
[3,40166,12,19,2,"Saturday",40,43]
[3,40168,12,21,16,"Weekday",49,58]
[3,40173,12,26,10,"Saturday",42,48]
[3,40174,12,27,20,"Sunday",39,44]
[4,39814,1,1,14,"Weekday",52,55]
[4,39814,1,1,19,"Weekday",49,52]
[4,39817,1,4,20,"Sunday",42,49]
[4,39822,1,9,14,"Weekday",50,57]
[4,39824,1,11,11,"Sunday",40,50]
[4,39828,1,15,18,"Weekday",46,57]
[4,39830,1,17,15,"Saturday",51,59]
[4,39834,1,21,6,"Weekday",40,42]
[4,39836,1,23,18,"Weekday",45,50]
[4,39838,1,25,15,"Sunday",52,55]
[4,39842,1,29,22,"Weekday",49,51]
[4,39844,1,31,19,"Saturday",52,58]
[4,39849,2,5,2,"Weekday",53,55]
[4,39851,2,7,13,"Saturday",62,66]
[4,39852,2,8,19,"Sunday",52,55]
[4,39857,2,13,2,"Weekday",46,49]
[4,39858,2,14,23,"Saturday",43,46]
[4,39860,2,16,20,"Weekday",50,54]
[4,39865,2,21,3,"Saturday",37,39]
[4,39868,2,24,20,"Weekday",42,49]
[4,39871,2,27,6,"Weekday",41,43]
[4,39873,3,1,3,"Sunday",46,49]
[4,39874,3,2,24,"Weekday",43,48]
[4,39879,3,7,7,"Saturday",47,50]
[4,39881,3,9,4,"Weekday",45,47]
[4,39885,3,13,11,"Weekday",52,64]
[4,39887,3,15,7,"Sunday",39,43]
[4,39892,3,20,1,"Weekday",44,49]
[4,39893,3,21,11,"Saturday",53,60]
[4,39895,3,23,8,"Weekday",48,52]
[4,39900,3,28,2,"Saturday",48,49]
[4,39902,3,30,18,"Weekday",57,64]
[4,39906,4,3,5,"Weekday",52,61]
[4,39907,4,4,15,"Saturday",61,70]
[4,39909,4,6,12,"Weekday",50,60]
[4,39914,4,11,6,"Saturday",36,38]
[4,39915,4,12,16,"Sunday",56,67]
[4,39920,4,17,1,"Weekday",47,50]
[4,39922,4,19,6,"Sunday",48,51]
[4,39923,4,20,16,"Weekday",52,56]
[4,39928,4,25,10,"Saturday",52,69]
[4,39929,4,26,20,"Sunday",55,63]
[4,39934,5,1,14,"Weekday",67,84]
[4,39937,5,4,8,"Weekday",52,59]
[4,39940,5,7,17,"Weekday",68,74]
[4,39942,5,9,14,"Saturday",66,71]
[4,39943,5,10,24,"Sunday",48,51]
[4,39948,5,15,18,"Weekday",59,67]
[4,39950,5,17,15,"Sunday",75,91]
[4,39953,5,20,23,"Weekday",55,57]
[4,39956,5,23,18,"Saturday",63,67]
[4,39958,5,25,15,"Weekday",64,68]
[4,39962,5,29,22,"Weekday",51,55]
[4,39964,5,31,19,"Sunday",51,58]
[4,39969,6,5,2,"Weekday",55,58]
[4,39971,6,7,6,"Sunday",49,52]
[4,39972,6,8,19,"Weekday",59,65]
[4,39977,6,13,2,"Saturday",47,49]
[4,39978,6,14,23,"Sunday",52,62]
[4,39983,6,19,17,"Weekday",69,77]
[4,39984,6,20,23,"Saturday",57,61]
[4,39986,6,22,23,"Weekday",56,58]
[4,39991,6,27,6,"Saturday",53,54]
[4,39993,6,29,3,"Weekday",49,51]
[4,39997,7,3,21,"Weekday",62,67]
[4,39999,7,5,7,"Sunday",57,61]
[4,40002,7,8,6,"Weekday",56,59]
[4,40005,7,11,10,"Saturday",64,69]
[4,40007,7,13,7,"Weekday",60,66]
[4,40012,7,18,1,"Saturday",55,60]
[4,40013,7,19,11,"Sunday",71,82]
[4,40018,7,24,5,"Weekday",54,56]
[4,40019,7,25,13,"Saturday",71,84]
[4,40021,7,27,11,"Weekday",66,73]
[4,40026,8,1,5,"Saturday",53,55]
[4,40027,8,2,15,"Sunday",64,71]
[4,40032,8,7,9,"Weekday",67,74]
[4,40034,8,9,6,"Sunday",59,64]
[4,40036,8,11,4,"Weekday",55,57]
[4,40040,8,15,9,"Saturday",65,72]
[4,40041,8,16,19,"Sunday",67,76]
[4,40046,8,21,13,"Weekday",70,79]
[4,40048,8,23,10,"Sunday",63,71]
[4,40052,8,27,17,"Weekday",68,96]
[4,40053,8,28,11,"Weekday",66,89]
[4,40056,8,31,10,"Weekday",58,62]
[4,40060,9,4,17,"Weekday",65,71]
[4,40062,9,6,14,"Sunday",64,72]
[4,40066,9,10,21,"Weekday",59,62]
[4,40068,9,12,18,"Saturday",63,72]
[4,40070,9,14,18,"Weekday",66,70]
[4,40074,9,18,21,"Weekday",64,68]
[4,40076,9,20,18,"Sunday",65,74]
[4,40078,9,22,15,"Weekday",71,96]
[4,40082,9,26,22,"Saturday",56,59]
[4,40084,9,28,19,"Weekday",64,73]
[4,40087,10,1,9,"Weekday",60,64]
[4,40090,10,4,22,"Sunday",53,59]
[4,40095,10,9,16,"Weekday",64,73]
[4,40097,10,11,2,"Sunday",56,57]
[4,40098,10,12,23,"Weekday",50,54]
[4,40103,10,17,6,"Saturday",46,47]
[4,40104,10,18,16,"Sunday",62,68]
[4,40109,10,23,20,"Weekday",51,56]
[4,40111,10,25,6,"Sunday",47,50]
[4,40113,10,27,3,"Weekday",45,47]
[4,40117,10,31,21,"Saturday",55,62]
[4,40119,11,2,7,"Weekday",48,50]
[4,40121,11,4,23,"Weekday",44,46]
[4,40125,11,8,10,"Sunday",48,56]
[4,40127,11,10,7,"Weekday",45,48]
[4,40132,11,15,1,"Sunday",44,47]
[4,40133,11,16,11,"Weekday",43,58]
[4,40138,11,21,5,"Saturday",42,45]
[4,40139,11,22,6,"Sunday",43,46]
[4,40144,11,27,8,"Weekday",42,43]
[4,40146,11,29,5,"Sunday",51,55]
[4,40147,11,30,15,"Weekday",59,62]
[4,40152,12,5,9,"Saturday",43,48]
[4,40155,12,8,19,"Weekday",51,52]
[4,40158,12,11,12,"Weekday",51,58]
[4,40160,12,13,9,"Sunday",40,43]
[4,40161,12,14,19,"Weekday",52,56]
[4,40166,12,19,13,"Saturday",41,55]
[4,40168,12,21,10,"Weekday",36,45]
[4,40172,12,25,10,"Weekday",48,51]
[4,40174,12,27,13,"Sunday",49,55]
[4,40176,12,29,10,"Weekday",52,55]
[5,39815,1,2,17,"Weekday",50,63]
[5,39817,1,4,14,"Sunday",56,66]
[5,39821,1,8,21,"Weekday",56,56]
[5,39824,1,11,17,"Sunday",43,59]
[5,39825,1,12,14,"Weekday",47,62]
[5,39829,1,16,21,"Weekday",47,48]
[5,39831,1,18,18,"Sunday",51,55]
[5,39836,1,23,1,"Weekday",48,49]
[5,39837,1,24,22,"Saturday",44,45]
[5,39841,1,28,24,"Weekday",49,52]
[5,39844,1,31,1,"Saturday",56,58]
[5,39845,2,1,22,"Sunday",41,45]
[5,39850,2,6,16,"Weekday",55,62]
[5,39852,2,8,2,"Sunday",50,52]
[5,39856,2,12,20,"Weekday",45,47]
[5,39858,2,14,15,"Saturday",51,65]
[5,39860,2,16,2,"Weekday",57,60]
[5,39864,2,20,20,"Weekday",53,58]
[5,39866,2,22,6,"Sunday",42,43]
[5,39870,2,26,24,"Weekday",50,54]
[5,39872,2,28,21,"Saturday",50,55]
[5,39875,3,3,22,"Weekday",54,55]
[5,39878,3,6,24,"Weekday",44,45]
[5,39880,3,8,10,"Sunday",54,54]
[5,39885,3,13,4,"Weekday",39,41]
[5,39887,3,15,1,"Sunday",41,42]
[5,39891,3,19,8,"Weekday",52,57]
[5,39893,3,21,5,"Saturday",46,49]
[5,39894,3,22,14,"Sunday",53,65]
[5,39899,3,27,8,"Weekday",50,51]
[5,39901,3,29,5,"Sunday",51,52]
[5,39905,4,2,12,"Weekday",56,73]
[5,39907,4,4,9,"Saturday",62,71]
[5,39910,4,7,12,"Weekday",59,72]
[5,39913,4,10,12,"Weekday",58,68]
[5,39915,4,12,9,"Sunday",56,63]
[5,39919,4,16,16,"Weekday",53,66]
[5,39921,4,18,13,"Saturday",55,63]
[5,39923,4,20,10,"Weekday",48,55]
[5,39927,4,24,3,"Weekday",49,51]
[5,39929,4,26,13,"Sunday",60,74]
[5,39933,4,30,20,"Weekday",49,53]
[5,39935,5,2,17,"Saturday",53,57]
[5,39937,5,4,14,"Weekday",62,70]
[5,39941,5,8,21,"Weekday",53,54]
[5,39944,5,11,10,"Weekday",59,66]
[5,39948,5,15,11,"Weekday",55,83]
[5,39949,5,16,21,"Saturday",48,51]
[5,39951,5,18,18,"Weekday",50,54]
[5,39956,5,23,1,"Saturday",52,54]
[5,39958,5,25,3,"Weekday",51,54]
[5,39962,5,29,15,"Weekday",55,62]
[5,39964,5,31,1,"Sunday",45,46]
[5,39965,6,1,22,"Weekday",54,55]
[5,39970,6,6,16,"Saturday",60,68]
[5,39972,6,8,2,"Weekday",44,45]
[5,39975,6,11,10,"Weekday",65,77]
[5,39978,6,14,5,"Sunday",48,48]
[5,39982,6,18,23,"Weekday",51,52]
[5,39984,6,20,20,"Saturday",56,57]
[5,39986,6,22,6,"Weekday",53,53]
[5,39990,6,26,24,"Weekday",55,56]
[5,39992,6,28,1,"Sunday",52,53]
[5,39997,7,3,3,"Weekday",50,51]
[5,39998,7,4,24,"Saturday",52,53]
[5,40000,7,6,10,"Weekday",63,75]
[5,40005,7,11,4,"Saturday",49,54]
[5,40007,7,13,1,"Weekday",54,55]
[5,40009,7,15,8,"Weekday",60,70]
[5,40013,7,19,4,"Sunday",56,57]
[5,40017,7,23,11,"Weekday",64,71]
[5,40019,7,25,8,"Saturday",58,63]
[5,40021,7,27,5,"Weekday",50,52]
[5,40025,7,31,12,"Weekday",63,71]
[5,40026,8,1,15,"Saturday",63,69]
[5,40029,8,4,5,"Weekday",57,58]
[5,40033,8,8,12,"Saturday",64,74]
[5,40035,8,10,9,"Weekday",61,63]
[5,40039,8,14,16,"Weekday",61,71]
[5,40041,8,16,13,"Sunday",63,70]
[5,40043,8,18,22,"Weekday",57,58]
[5,40047,8,22,16,"Saturday",62,72]
[5,40049,8,24,13,"Weekday",67,74]
[5,40053,8,28,20,"Weekday",46,60]
[5,40055,8,30,17,"Sunday",61,65]
[5,40060,9,4,11,"Weekday",63,93]
[5,{"$f":"DATE(2009,C41026,D41026)","v":40063},9,7,9,"Weekday",56,60]
[5,40063,9,7,17,"Weekday",60,65]
[5,40068,9,12,11,"Saturday",64,71]
[5,40069,9,13,21,"Sunday",56,58]
[5,40074,9,18,15,"Weekday",62,69]
[5,40076,9,20,1,"Sunday",57,58]
[5,40077,9,21,20,"Weekday",60,64]
[5,40082,9,26,15,"Saturday",64,78]
[5,40084,9,28,1,"Weekday",58,59]
[5,40088,10,2,19,"Weekday",60,62]
[5,40090,10,4,5,"Sunday",49,50]
[5,40094,10,8,23,"Weekday",54,56]
[5,40095,10,9,3,"Weekday",52,52]
[5,40098,10,12,5,"Weekday",63,66]
[5,40102,10,16,23,"Weekday",50,53]
[5,40104,10,18,20,"Sunday",52,53]
[5,40109,10,23,3,"Weekday",56,56]
[5,40110,10,24,24,"Saturday",53,53]
[5,40114,10,28,14,"Weekday",65,84]
[5,40117,10,31,3,"Saturday",45,47]
[5,40118,11,1,24,"Sunday",54,55]
[5,40123,11,6,7,"Weekday",44,46]
[5,40125,11,8,4,"Sunday",37,44]
[5,40128,11,11,23,"Weekday",55,55]
[5,40131,11,14,7,"Saturday",52,53]
[5,40133,11,16,4,"Weekday",47,49]
[5,40137,11,20,11,"Weekday",48,58]
[5,40139,11,22,8,"Sunday",45,51]
[5,40141,11,24,5,"Weekday",51,60]
[5,40145,11,28,14,"Saturday",59,76]
[5,40147,11,30,8,"Weekday",46,46]
[5,40151,12,4,15,"Weekday",57,72]
[5,40153,12,6,12,"Sunday",55,76]
[5,40155,12,8,9,"Weekday",47,47]
[5,40159,12,12,16,"Saturday",53,61]
[5,40162,12,15,21,"Weekday",59,61]
[5,40166,12,19,6,"Saturday",49,53]
[5,40167,12,20,16,"Sunday",56,63]
[5,40169,12,22,13,"Weekday",55,67]
[5,40173,12,26,20,"Saturday",34,44]
[5,40175,12,28,17,"Weekday",49,55]
[6,39815,1,2,4,"Weekday",41,43]
[6,39816,1,3,20,"Saturday",46,53]
[6,39821,1,8,14,"Weekday",50,64]
[6,39823,1,10,11,"Saturday",52,74]
[6,39824,1,11,21,"Sunday",52,59]
[6,39829,1,16,15,"Weekday",57,62]
[6,39831,1,18,19,"Sunday",52,53]
[6,39835,1,22,18,"Weekday",57,58]
[6,39837,1,24,15,"Saturday",58,59]
[6,39839,1,26,1,"Weekday",46,49]
[6,39843,1,30,19,"Weekday",58,59]
[6,39845,2,1,5,"Sunday",38,44]
[6,39849,2,5,2,"Weekday",49,54]
[6,39851,2,7,19,"Saturday",52,52]
[6,39856,2,12,2,"Weekday",43,57]
[6,39857,2,13,23,"Weekday",49,50]
[6,39859,2,15,20,"Sunday",55,57]
[6,39864,2,20,3,"Weekday",52,52]
[6,{"$f":"DATE(2009,C45058,D45058)","v":39866},2,22,9,"Sunday",57,61]
[6,39870,2,26,6,"Weekday",50,51]
[6,39872,2,28,3,"Saturday",53,54]
[6,39873,3,1,24,"Sunday",37,51]
[6,39878,3,6,7,"Weekday",37,49]
[6,39880,3,8,4,"Sunday",46,48]
[6,39882,3,10,24,"Weekday",48,51]
[6,39886,3,14,7,"Saturday",41,47]
[6,39888,3,16,4,"Weekday",46,47]
[6,39892,3,20,11,"Weekday",56,61]
[6,39894,3,22,8,"Sunday",52,54]
[6,39899,3,27,2,"Weekday",54,55]
[6,39900,3,28,7,"Saturday",53,54]
[6,39902,3,30,8,"Weekday",52,54]
[6,39906,4,3,15,"Weekday",56,74]
[6,39908,4,5,12,"Sunday",55,75]
[6,39913,4,10,6,"Weekday",52,54]
[6,39914,4,11,16,"Saturday",58,63]
[6,39917,4,14,14,"Weekday",55,65]
[6,39921,4,18,6,"Saturday",45,55]
[6,39922,4,19,16,"Sunday",54,62]
[6,39927,4,24,10,"Weekday",57,63]
[6,39928,4,25,20,"Saturday",52,54]
[6,39931,4,28,7,"Weekday",53,57]
[6,39935,5,2,10,"Saturday",59,65]
[6,39936,5,3,20,"Sunday",53,57]
[6,39941,5,8,14,"Weekday",58,67]
[6,39942,5,9,24,"Saturday",52,56]
[6,39947,5,14,18,"Weekday",58,61]
[6,39948,5,15,14,"Weekday",60,67]
[6,39950,5,17,24,"Sunday",53,56]
[6,39955,5,22,18,"Weekday",58,63]
[6,39957,5,24,15,"Sunday",60,68]
[6,39961,5,28,22,"Weekday",57,64]
[6,39963,5,30,19,"Saturday",61,67]
[6,39965,6,1,5,"Weekday",50,53]
[6,39969,6,5,22,"Weekday",56,58]
[6,39971,6,7,19,"Sunday",57,59]
[6,39976,6,12,2,"Weekday",56,57]
[6,39977,6,13,23,"Saturday",57,59]
[6,39982,6,18,6,"Weekday",59,61]
[6,39982,6,18,12,"Weekday",66,73]
[6,39985,6,21,23,"Sunday",60,63]
[6,39990,6,26,6,"Weekday",61,64]
[6,39992,6,28,3,"Sunday",57,62]
[6,39993,6,29,24,"Weekday",57,59]
[6,39998,7,4,7,"Saturday",58,59]
[6,39999,7,5,19,"Sunday",58,62]
[6,40004,7,10,10,"Weekday",71,81]
[6,40006,7,12,7,"Sunday",62,66]
[6,40008,7,14,4,"Weekday",57,60]
[6,40012,7,18,11,"Saturday",63,68]
[6,40014,7,20,8,"Weekday",61,65]
[6,40017,7,23,2,"Weekday",58,61]
[6,40020,7,26,11,"Sunday",68,76]
[6,40025,7,31,5,"Weekday",60,64]
[6,40026,8,1,15,"Saturday",64,71]
[6,40028,8,3,12,"Weekday",67,74]
[6,40033,8,8,6,"Saturday",63,64]
[6,40036,8,11,13,"Weekday",67,74]
[6,40039,8,14,9,"Weekday",65,71]
[6,40040,8,15,19,"Saturday",64,68]
[6,40042,8,17,16,"Weekday",65,73]
[6,40047,8,22,10,"Saturday",63,72]
[6,40048,8,23,20,"Sunday",61,64]
[6,40053,8,28,20,"Weekday",60,63]
[6,40055,8,30,10,"Sunday",66,75]
[6,40059,9,3,17,"Weekday",63,69]
[6,40061,9,5,14,"Saturday",67,76]
[6,40062,9,6,24,"Sunday",66,69]
[6,40067,9,11,18,"Weekday",62,68]
[6,40071,9,15,3,"Weekday",57,60]
[6,40073,9,17,21,"Weekday",61,65]
[6,40075,9,19,18,"Saturday",61,66]
[6,40077,9,21,15,"Weekday",62,67]
[6,40081,9,25,22,"Weekday",59,61]
[6,40083,9,27,19,"Sunday",62,67]
[6,40087,10,1,18,"Weekday",63,66]
[6,40089,10,3,22,"Saturday",65,69]
[6,40091,10,5,19,"Weekday",61,65]
[6,40096,10,10,2,"Saturday",59,60]
[6,40097,10,11,23,"Sunday",58,61]
[6,40101,10,15,11,"Weekday",63,70]
[6,40104,10,18,2,"Sunday",56,59]
[6,40105,10,19,23,"Weekday",56,58]
[6,40110,10,24,6,"Saturday",44,57]
[6,40112,10,26,3,"Weekday",45,53]
[6,40116,10,30,21,"Weekday",56,61]
[6,40118,11,1,18,"Sunday",57,62]
[6,40120,11,3,3,"Weekday",53,56]
[6,40124,11,7,10,"Saturday",59,63]
[6,40126,11,9,7,"Weekday",43,51]
[6,40131,11,14,1,"Saturday",52,58]
[6,40132,11,15,11,"Sunday",56,60]
[6,40136,11,19,1,"Weekday",50,53]
[6,40138,11,21,14,"Saturday",54,72]
[6,40140,11,23,11,"Weekday",51,70]
[6,40145,11,28,5,"Saturday",45,59]
[6,40146,11,29,15,"Sunday",59,80]
[6,40151,12,4,9,"Weekday",56,59]
[6,40153,12,6,8,"Sunday",46,49]
[6,40154,12,7,15,"Weekday",56,60]
[6,40159,12,12,9,"Saturday",45,56]
[6,40160,12,13,19,"Sunday",52,56]
[6,40165,12,18,13,"Weekday",50,75]
[6,40167,12,20,10,"Sunday",47,68]
[6,40169,12,22,23,"Weekday",48,51]
[6,40173,12,26,13,"Saturday",49,58]
[6,40175,12,28,10,"Weekday",38,52]
[7,39814,1,1,17,"Weekday",44,64]
[7,39816,1,3,14,"Saturday",54,62]
[7,39820,1,7,21,"Weekday",46,52]
[7,39822,1,9,6,"Weekday",51,55]
[7,39824,1,11,14,"Sunday",58,68]
[7,39828,1,15,21,"Weekday",55,61]
[7,39830,1,17,18,"Saturday",55,61]
[7,39835,1,22,1,"Weekday",44,48]
[7,39836,1,23,22,"Weekday",46,56]
[7,39839,1,26,13,"Weekday",52,64]
[7,39843,1,30,1,"Weekday",49,54]
[7,39844,1,31,22,"Saturday",49,56]
[7,39846,2,2,19,"Weekday",38,56]
[7,39851,2,7,2,"Saturday",49,52]
[7,39852,2,8,23,"Sunday",50,57]
[7,39856,2,12,4,"Weekday",36,46]
[7,39859,2,15,2,"Sunday",48,53]
[7,39863,2,19,20,"Weekday",51,55]
[7,39865,2,21,6,"Saturday",49,51]
[7,39867,2,23,3,"Weekday",51,55]
[7,39871,2,27,10,"Weekday",53,56]
[7,39873,3,1,11,"Sunday",57,79]
[7,39877,3,5,24,"Weekday",50,55]
[7,39879,3,7,10,"Saturday",53,63]
[7,39881,3,9,7,"Weekday",45,50]
[7,39886,3,14,1,"Saturday",52,54]
[7,39887,3,15,11,"Sunday",53,55]
[7,39890,3,18,18,"Weekday",51,59]
[7,39893,3,21,14,"Saturday",57,65]
[7,39898,3,26,8,"Weekday",50,57]
[7,39900,3,28,5,"Saturday",52,53]
[7,39901,3,29,15,"Sunday",61,67]
[7,39904,4,1,11,"Weekday",54,67]
[7,39908,4,5,5,"Sunday",52,54]
[7,39912,4,9,12,"Weekday",55,64]
[7,39914,4,11,9,"Saturday",53,61]
[7,39915,4,12,19,"Sunday",55,59]
[7,39920,4,17,13,"Weekday",60,71]
[7,39921,4,18,18,"Saturday",54,59]
[7,39926,4,23,16,"Weekday",54,61]
[7,39928,4,25,13,"Saturday",61,71]
[7,39929,4,26,23,"Sunday",55,56]
[7,39934,5,1,17,"Weekday",58,65]
[7,39936,5,3,14,"Sunday",59,65]
[7,39941,5,8,5,"Weekday",50,51]
[7,39942,5,9,17,"Saturday",57,64]
[7,39944,5,11,14,"Weekday",56,65]
[7,39948,5,15,21,"Weekday",51,61]
[7,39950,5,17,18,"Sunday",53,63]
[7,39955,5,22,1,"Weekday",56,60]
[7,39958,5,25,12,"Weekday",55,61]
[7,39958,5,25,18,"Weekday",56,61]
[7,39963,5,30,1,"Saturday",55,60]
[7,39964,5,31,22,"Sunday",55,59]
[7,39969,6,5,16,"Weekday",64,70]
[7,39971,6,7,2,"Sunday",58,61]
[7,39975,6,11,19,"Weekday",60,65]
[7,39977,6,13,5,"Saturday",55,60]
[7,39979,6,15,2,"Weekday",54,60]
[7,39983,6,19,20,"Weekday",60,65]
[7,39985,6,21,6,"Sunday",58,61]
[7,39989,6,25,24,"Weekday",54,58]
[7,39992,6,28,10,"Sunday",62,69]
[7,39993,6,29,6,"Weekday",53,59]
[7,39997,7,3,24,"Weekday",61,63]
[7,39999,7,5,10,"Sunday",59,64]
[7,40004,7,10,4,"Weekday",56,58]
[7,40006,7,12,1,"Sunday",61,63]
[7,40009,7,15,17,"Weekday",69,76]
[7,40012,7,18,4,"Saturday",60,62]
[7,40013,7,19,14,"Sunday",70,76]
[7,40018,7,24,8,"Weekday",64,69]
[7,40020,7,26,5,"Sunday",62,67]
[7,40024,7,30,12,"Weekday",72,78]
[7,40026,8,1,24,"Saturday",61,65]
[7,40027,8,2,18,"Sunday",64,69]
[7,40032,8,7,12,"Weekday",70,78]
[7,40034,8,9,9,"Sunday",68,76]
[7,40038,8,13,16,"Weekday",67,77]
[7,40040,8,15,13,"Saturday",72,84]
[7,40044,8,19,7,"Weekday",64,69]
[7,40046,8,21,16,"Weekday",65,73]
[7,40048,8,23,13,"Sunday",64,74]
[7,40052,8,27,20,"Weekday",63,67]
[7,40054,8,29,17,"Saturday",65,72]
[7,40056,8,31,14,"Weekday",66,75]
[7,40060,9,4,22,"Weekday",62,65]
[7,40062,9,6,17,"Sunday",65,71]
[7,40067,9,11,11,"Weekday",63,83]
[7,40068,9,12,21,"Saturday",69,72]
[7,40070,9,14,18,"Weekday",65,70]
[7,40074,9,18,15,"Weekday",69,77]
[7,40076,9,20,21,"Sunday",61,66]
[7,40081,9,25,15,"Weekday",67,76]
[7,40083,9,27,1,"Sunday",58,64]
[7,40084,9,28,22,"Weekday",60,65]
[7,40089,10,3,5,"Saturday",56,64]
[7,40091,10,5,22,"Weekday",57,63]
[7,40095,10,9,19,"Weekday",56,62]
[7,40097,10,11,5,"Sunday",46,55]
[7,40101,10,15,23,"Weekday",58,61]
[7,40103,10,17,20,"Saturday",58,71]
[7,40105,10,19,6,"Weekday",51,63]
[7,40109,10,23,5,"Weekday",57,63]
[7,40111,10,25,9,"Sunday",57,65]
[7,40116,10,30,3,"Weekday",45,53]
[7,40117,10,31,24,"Saturday",51,55]
[7,40119,11,2,10,"Weekday",53,57]
[7,40124,11,7,4,"Saturday",54,57]
[7,40126,11,9,12,"Weekday",58,76]
[7,40130,11,13,7,"Weekday",39,41]
[7,40132,11,15,4,"Sunday",34,45]
[7,40133,11,16,14,"Weekday",57,74]
[7,40138,11,21,8,"Saturday",53,59]
[7,40140,11,23,5,"Weekday",42,45]
[7,40143,11,26,3,"Weekday",59,61]
[7,40146,11,29,8,"Sunday",56,63]
[7,40150,12,3,15,"Weekday",60,61]
[7,40152,12,5,12,"Saturday",61,62]
[7,40154,12,7,9,"Weekday",56,61]
[7,40158,12,11,16,"Weekday",61,69]
[7,40160,12,13,10,"Sunday",52,68]
[7,40162,12,15,9,"Weekday",50,52]
[7,40166,12,19,16,"Saturday",55,70]
[7,40168,12,21,13,"Weekday",57,65]
[7,40172,12,25,20,"Weekday",54,57]
[7,40174,12,27,17,"Sunday",50,60]
[7,40177,12,30,17,"Weekday",45,57]
[8,39815,1,2,20,"Weekday",35,40]
[8,39817,1,4,17,"Sunday",46,55]
[8,39821,1,8,24,"Weekday",33,39]
[8,39823,1,10,21,"Saturday",44,51]
[8,39828,1,15,15,"Weekday",53,62]
[8,39829,1,16,8,"Weekday",47,57]
[8,39831,1,18,21,"Sunday",51,60]
[8,39836,1,23,15,"Weekday",56,62]
[8,39838,1,25,1,"Sunday",33,38]
[8,39842,1,29,19,"Weekday",47,58]
[8,39844,1,31,5,"Saturday",42,48]
[8,39846,2,2,15,"Weekday",53,60]
[8,39850,2,6,19,"Weekday",53,54]
[8,39852,2,8,5,"Sunday",49,49]
[8,39856,2,12,23,"Weekday",47,57]
[8,39858,2,14,20,"Saturday",56,56]
[8,39863,2,19,3,"Weekday",49,49]
[8,39863,2,19,22,"Weekday",48,49]
[8,39866,2,22,9,"Sunday",56,58]
[8,39871,2,27,3,"Weekday",34,45]
[8,39872,2,28,24,"Saturday",38,50]
[8,39877,3,5,7,"Weekday",48,51]
[8,39877,3,5,15,"Weekday",58,66]
[8,39880,3,8,13,"Sunday",52,76]
[8,39885,3,13,7,"Weekday",45,49]
[8,39887,3,15,4,"Sunday",55,57]
[8,39891,3,19,11,"Weekday",52,64]
[8,39893,3,21,8,"Saturday",53,57]
[8,39894,3,22,22,"Sunday",49,51]
[8,39899,3,27,11,"Weekday",56,63]
[8,39901,3,29,8,"Sunday",49,55]
[8,39905,4,2,15,"Weekday",52,68]
[8,39907,4,4,12,"Saturday",52,75]
[8,39909,4,6,9,"Weekday",53,64]
[8,39914,4,11,9,"Saturday",54,55]
[8,39915,4,12,12,"Sunday",60,67]
[8,39919,4,16,19,"Weekday",53,57]
[8,39921,4,18,16,"Saturday",53,67]
[8,39923,4,20,13,"Weekday",56,69]
[8,39927,4,24,20,"Weekday",51,58]
[8,39931,4,28,16,"Weekday",56,62]
[8,39934,5,1,10,"Weekday",61,70]
[8,39935,5,2,20,"Saturday",55,60]
[8,39940,5,7,14,"Weekday",57,67]
[8,39941,5,8,24,"Weekday",49,52]
[8,39943,5,10,21,"Sunday",57,60]
[8,39948,5,15,23,"Weekday",59,61]
[8,39949,5,16,24,"Saturday",55,58]
[8,39954,5,21,18,"Weekday",54,62]
[8,39956,5,23,15,"Saturday",61,72]
[8,39958,5,25,1,"Weekday",56,60]
[8,39962,5,29,19,"Weekday",63,70]
[8,39965,6,1,14,"Weekday",69,78]
[8,39968,6,4,22,"Weekday",58,58]
[8,39970,6,6,19,"Saturday",58,75]
[8,39972,6,8,5,"Weekday",57,60]
[8,39976,6,12,23,"Weekday",55,57]
[8,39978,6,14,9,"Sunday",63,71]
[8,39982,6,18,21,"Weekday",62,63]
[8,39984,6,20,23,"Saturday",65,66]
[8,39989,6,25,6,"Weekday",63,64]
[8,39991,6,27,3,"Saturday",64,66]
[8,39992,6,28,24,"Sunday",62,64]
[8,39997,7,3,7,"Weekday",63,63]
[8,40000,7,6,4,"Weekday",56,57]
[8,40003,7,9,10,"Weekday",61,72]
[8,40005,7,11,7,"Saturday",59,63]
[8,40007,7,13,4,"Weekday",57,58]
[8,40011,7,17,11,"Weekday",65,85]
[8,40013,7,19,8,"Sunday",70,77]
[8,40017,7,23,11,"Weekday",70,86]
[8,40019,7,25,11,"Saturday",72,88]
[8,40021,7,27,8,"Weekday",66,72]
[8,40025,7,31,15,"Weekday",71,80]
[8,40027,8,2,12,"Sunday",66,80]
[8,40032,8,7,6,"Weekday",65,66]
[8,40034,8,9,2,"Sunday",62,62]
[8,40035,8,10,12,"Weekday",71,87]
[8,40039,8,14,19,"Weekday",61,66]
[8,40041,8,16,16,"Sunday",67,80]
[8,40046,8,21,10,"Weekday",70,86]
[8,40047,8,22,19,"Saturday",67,74]
[8,40049,8,24,16,"Weekday",65,84]
[8,40054,8,29,10,"Saturday",63,72]
[8,40055,8,30,20,"Sunday",58,59]
[8,40060,9,4,14,"Weekday",67,82]
[8,40061,9,5,24,"Saturday",59,62]
[8,40065,9,9,2,"Weekday",55,67]
[8,40068,9,12,14,"Saturday",68,84]
[8,40069,9,13,24,"Sunday",59,64]
[8,40074,9,18,18,"Weekday",59,65]
[8,40076,9,20,4,"Sunday",57,62]
[8,40080,9,24,22,"Weekday",49,71]
[8,40082,9,26,9,"Saturday",61,74]
[8,40084,9,28,4,"Weekday",58,61]
[8,40088,10,2,22,"Weekday",62,65]
[8,40090,10,4,19,"Sunday",63,65]
[8,40095,10,9,2,"Weekday",53,55]
[8,40096,10,10,23,"Saturday",58,60]
[8,40098,10,12,24,"Weekday",53,56]
[8,40103,10,17,2,"Saturday",55,57]
[8,40104,10,18,23,"Sunday",58,61]
[8,40109,10,23,6,"Weekday",63,64]
[8,40111,10,25,3,"Sunday",41,51]
[8,40112,10,26,24,"Weekday",54,57]
[8,40116,10,30,7,"Weekday",50,55]
[8,40119,11,2,3,"Weekday",56,59]
[8,40123,11,6,10,"Weekday",58,66]
[8,40125,11,8,7,"Sunday",46,57]
[8,40127,11,10,4,"Weekday",51,62]
[8,40131,11,14,11,"Saturday",60,66]
[8,40133,11,16,14,"Weekday",63,75]
[8,40137,11,20,14,"Weekday",49,62]
[8,40139,11,22,11,"Sunday",51,62]
[8,40144,11,27,5,"Weekday",54,57]
[8,40145,11,28,15,"Saturday",63,77]
[8,40147,11,30,12,"Weekday",61,70]
[8,40150,12,3,21,"Weekday",50,55]
[8,40153,12,6,15,"Sunday",51,61]
[8,40158,12,11,9,"Weekday",39,49]
[8,40159,12,12,19,"Saturday",44,50]
[8,40161,12,14,16,"Weekday",53,65]
[8,40166,12,19,10,"Saturday",63,67]
[8,40167,12,20,12,"Sunday",55,67]
[8,40172,12,25,13,"Weekday",49,71]
[8,40173,12,26,23,"Saturday",39,50]
[8,40175,12,28,20,"Weekday",41,49]
[9,39815,1,2,14,"Weekday",53,71]
[9,39816,1,3,24,"Saturday",39,52]
[9,39819,1,6,19,"Weekday",48,57]
[9,39823,1,10,14,"Saturday",57,59]
[9,39827,1,14,21,"Weekday",48,53]
[9,39829,1,16,18,"Weekday",41,54]
[9,39831,1,18,4,"Sunday",39,40]
[9,39835,1,22,22,"Weekday",54,58]
[9,39837,1,24,2,"Saturday",49,52]
[9,39842,1,29,1,"Weekday",46,52]
[9,39843,1,30,22,"Weekday",49,55]
[9,39845,2,1,19,"Sunday",53,54]
[9,39850,2,6,2,"Weekday",51,53]
[9,39853,2,9,15,"Weekday",52,63]
[9,39856,2,12,5,"Weekday",39,48]
[9,39858,2,14,2,"Saturday",44,53]
[9,39859,2,15,23,"Sunday",44,54]
[9,39864,2,20,6,"Weekday",37,39]
[9,39866,2,22,3,"Sunday",45,47]
[9,39870,2,26,6,"Weekday",49,58]
[9,39872,2,28,6,"Saturday",41,52]
[9,39874,3,2,3,"Weekday",39,42]
[9,39878,3,6,10,"Weekday",47,60]
[9,39880,3,8,7,"Sunday",37,46]
[9,39885,3,13,1,"Weekday",51,56]
[9,39887,3,15,13,"Sunday",50,63]
[9,39888,3,16,7,"Weekday",44,53]
[9,39892,3,20,14,"Weekday",58,73]
[9,39894,3,22,11,"Sunday",54,63]
[9,39899,3,27,5,"Weekday",42,45]
[9,39900,3,28,15,"Saturday",47,65]
[9,39904,4,1,20,"Weekday",49,64]
[9,39907,4,4,5,"Saturday",46,47]
[9,39908,4,5,15,"Sunday",64,82]
[9,39913,4,10,9,"Weekday",53,59]
[9,39914,4,11,19,"Saturday",53,60]
[9,39919,4,16,13,"Weekday",55,67]
[9,39922,4,19,3,"Sunday",48,49]
[9,39922,4,19,19,"Sunday",53,59]
[9,39927,4,24,13,"Weekday",61,73]
[9,39928,4,25,23,"Saturday",55,57]
[9,39933,4,30,17,"Weekday",57,65]
[9,39935,5,2,14,"Saturday",68,79]
[9,39938,5,5,18,"Weekday",59,65]
[9,39941,5,8,17,"Weekday",58,68]
[9,39943,5,10,14,"Sunday",61,73]
[9,39947,5,14,21,"Weekday",51,64]
[9,39949,5,16,18,"Saturday",57,83]
[9,39954,5,21,1,"Weekday",52,55]
[9,39956,5,23,1,"Saturday",53,54]
[9,39957,5,24,18,"Sunday",59,67]
[9,39962,5,29,1,"Weekday",55,60]
[9,39963,5,30,22,"Saturday",53,57]
[9,39968,6,4,5,"Weekday",51,57]
[9,39970,6,6,2,"Saturday",57,60]
[9,39973,6,9,8,"Weekday",57,58]
[9,39976,6,12,5,"Weekday",55,60]
[9,39978,6,14,2,"Sunday",57,61]
[9,39982,6,18,20,"Weekday",61,65]
[9,39984,6,20,6,"Saturday",54,54]
[9,39986,6,22,3,"Weekday",53,59]
[9,39989,6,25,23,"Weekday",58,63]
[9,39992,6,28,6,"Sunday",57,60]
[9,39996,7,2,24,"Weekday",60,68]
[9,39998,7,4,10,"Saturday",60,75]
[9,40000,7,6,7,"Weekday",55,62]
[9,40005,7,11,1,"Saturday",57,70]
[9,40007,7,13,6,"Weekday",60,65]
[9,40011,7,17,4,"Weekday",58,61]
[9,40012,7,18,14,"Saturday",68,86]
[9,40014,7,20,11,"Weekday",67,84]
[9,40019,7,25,5,"Saturday",59,62]
[9,40020,7,26,23,"Sunday",61,74]
[9,40025,7,31,8,"Weekday",62,68]
[9,40026,8,1,18,"Saturday",67,78]
[9,40031,8,6,12,"Weekday",72,90]
[9,40033,8,8,9,"Saturday",70,82]
[9,40034,8,9,19,"Sunday",69,77]
[9,40038,8,13,6,"Weekday",62,64]
[9,40041,8,16,9,"Sunday",62,71]
[9,40045,8,20,16,"Weekday",68,85]
[9,40047,8,22,13,"Saturday",73,94]
[9,40048,8,23,23,"Sunday",62,69]
[9,40053,8,28,17,"Weekday",64,73]
[9,40055,8,30,13,"Sunday",64,73]
[9,40059,9,3,20,"Weekday",61,67]
[9,40061,9,5,17,"Saturday",64,85]
[9,40063,9,7,14,"Weekday",72,92]
[9,40067,9,11,21,"Weekday",60,66]
[9,40069,9,13,18,"Sunday",64,70]
[9,40072,9,16,4,"Weekday",59,61]
[9,40075,9,19,21,"Saturday",58,63]
[9,40077,9,21,18,"Weekday",66,74]
[9,40082,9,26,1,"Saturday",57,60]
[9,40083,9,27,22,"Sunday",63,69]
[9,40088,10,2,5,"Weekday",55,57]
[9,40089,10,3,11,"Saturday",62,80]
[9,40091,10,5,22,"Weekday",65,78]
[9,40096,10,10,5,"Saturday",49,52]
[9,40098,10,12,2,"Weekday",45,51]
[9,40102,10,16,20,"Weekday",51,69]
[9,40104,10,18,6,"Sunday",46,52]
[9,40106,10,20,18,"Weekday",59,80]
[9,40110,10,24,9,"Saturday",55,58]
[9,40112,10,26,6,"Weekday",53,53]
[9,40116,10,30,24,"Weekday",54,59]
[9,40118,11,1,10,"Sunday",54,72]
[9,40123,11,6,4,"Weekday",47,49]
[9,40126,11,9,5,"Weekday",44,50]
[9,40126,11,9,10,"Weekday",53,67]
[9,40131,11,14,4,"Saturday",56,58]
[9,40132,11,15,14,"Sunday",58,68]
[9,40137,11,20,8,"Weekday",40,53]
[9,40139,11,22,5,"Sunday",41,45]
[9,40140,11,23,16,"Weekday",56,64]
[9,40145,11,28,8,"Saturday",49,52]
[9,40146,11,29,18,"Sunday",41,55]
[9,40151,12,4,12,"Weekday",55,67]
[9,40153,12,6,9,"Sunday",46,54]
[9,40157,12,10,16,"Weekday",51,58]
[9,40157,12,10,23,"Weekday",46,49]
[9,40161,12,14,9,"Weekday",47,51]
[9,40165,12,18,16,"Weekday",54,61]
[9,40167,12,20,13,"Sunday",57,73]
[9,40171,12,24,20,"Weekday",46,59]
[9,40173,12,26,17,"Saturday",55,64]
[9,40175,12,28,6,"Weekday",36,46]
[10,39814,1,1,20,"Weekday",37,45]
[10,39816,1,3,17,"Saturday",48,55]
[10,39820,1,7,24,"Weekday",51,53]
[10,39822,1,9,21,"Weekday",38,46]
[10,39826,1,13,19,"Weekday",45,47]
[10,39828,1,15,24,"Weekday",39,40]
[10,39830,1,17,21,"Saturday",51,55]
[10,39835,1,22,15,"Weekday",53,67]
[10,39837,1,24,1,"Saturday",56,56]
[10,39838,1,25,22,"Sunday",48,50]
[10,39843,1,30,10,"Weekday",62,72]
[10,39845,2,1,1,"Sunday",45,49]
[10,39849,2,5,19,"Weekday",55,60]
[10,39851,2,7,5,"Saturday",54,58]
[10,39853,2,9,2,"Weekday",48,56]
[10,39857,2,13,9,"Weekday",50,66]
[10,39860,2,16,17,"Weekday",50,72]
[10,39863,2,19,23,"Weekday",35,48]
[10,39865,2,21,9,"Saturday",38,53]
[10,39870,2,26,3,"Weekday",40,44]
[10,39871,2,27,24,"Weekday",38,41]
[10,39873,3,1,10,"Sunday",42,46]
[10,39877,3,5,24,"Weekday",45,50]
[10,39879,3,7,13,"Saturday",54,78]
[10,39884,3,12,7,"Weekday",47,49]
[10,39886,3,14,4,"Saturday",41,42]
[10,39887,3,15,14,"Sunday",51,73]
[10,39892,3,20,8,"Weekday",47,52]
[10,39895,3,23,7,"Weekday",49,55]
[10,39898,3,26,11,"Weekday",52,59]
[10,39900,3,28,8,"Saturday",51,53]
[10,39904,4,1,15,"Weekday",51,72]
[10,39906,4,3,12,"Weekday",55,74]
[10,39908,4,5,9,"Sunday",58,72]
[10,39911,4,8,22,"Weekday",48,55]
[10,39914,4,11,12,"Saturday",56,62]
[10,39918,4,15,19,"Weekday",55,60]
[10,39920,4,17,16,"Weekday",55,62]
[10,39922,4,19,13,"Sunday",53,65]
[10,39926,4,23,20,"Weekday",56,57]
[10,39929,4,26,5,"Sunday",46,47]
[10,39930,4,27,13,"Weekday",62,90]
[10,39934,5,1,20,"Weekday",55,61]
[10,39936,5,3,17,"Sunday",48,63]
[10,39940,5,7,24,"Weekday",54,58]
[10,39942,5,9,21,"Saturday",55,61]
[10,39946,5,13,12,"Weekday",61,73]
[10,39948,5,15,24,"Weekday",55,60]
[10,39950,5,17,21,"Sunday",57,62]
[10,39955,5,22,15,"Weekday",56,72]
[10,39957,5,24,1,"Sunday",47,51]
[10,39961,5,28,19,"Weekday",60,68]
[10,39963,5,30,3,"Saturday",51,55]
[10,39965,6,1,1,"Weekday",57,61]
[10,39969,6,5,19,"Weekday",63,76]
[10,39971,6,7,5,"Sunday",60,63]
[10,39975,6,11,23,"Weekday",57,62]
[10,39977,6,13,9,"Saturday",60,68]
[10,39980,6,16,10,"Weekday",61,69]
[10,39983,6,19,23,"Weekday",58,63]
[10,39985,6,21,9,"Sunday",58,63]
[10,39990,6,26,3,"Weekday",56,64]
[10,39991,6,27,24,"Saturday",57,64]
[10,39994,6,30,3,"Weekday",48,55]
[10,39998,7,4,3,"Saturday",57,61]
[10,39999,7,5,13,"Sunday",68,86]
[10,40004,7,10,7,"Weekday",62,78]
[10,40006,7,12,4,"Sunday",62,66]
[10,40010,7,16,11,"Weekday",64,80]
[10,40011,7,17,10,"Weekday",62,77]
[10,40013,7,19,17,"Sunday",65,86]
[10,40018,7,24,11,"Weekday",65,84]
[10,40020,7,26,8,"Sunday",64,71]
[10,40024,7,30,15,"Weekday",69,95]
[10,40026,8,1,12,"Saturday",68,83]
[10,40028,8,3,17,"Weekday",66,87]
[10,40032,8,7,15,"Weekday",71,81]
[10,40034,8,9,12,"Sunday",66,91]
[10,40038,8,13,19,"Weekday",65,90]
[10,40040,8,15,16,"Saturday",72,94]
[10,40042,8,17,13,"Weekday",70,91]
[10,40045,8,20,8,"Weekday",64,74]
[10,40048,8,23,16,"Sunday",62,85]
[10,40053,8,28,10,"Weekday",61,88]
[10,40054,8,29,20,"Saturday",63,74]
[10,40056,8,31,17,"Weekday",63,84]
[10,40060,9,4,24,"Weekday",53,64]
[10,40062,9,6,15,"Sunday",61,94]
[10,40067,9,11,14,"Weekday",62,85]
[10,40068,9,12,24,"Saturday",56,59]
[10,40073,9,17,18,"Weekday",67,82]
[10,40075,9,19,4,"Saturday",61,67]
[10,40077,9,21,1,"Weekday",53,59]
[10,40079,9,23,22,"Weekday",67,79]
[10,40083,9,27,4,"Sunday",57,60]
[10,40087,10,1,22,"Weekday",57,63]
[10,40089,10,3,19,"Saturday",54,81]
[10,40091,10,5,5,"Weekday",47,56]
[10,40095,10,9,23,"Weekday",46,52]
[10,40099,10,13,9,"Weekday",56,80]
[10,40102,10,16,2,"Weekday",50,62]
[10,40103,10,17,23,"Saturday",58,63]
[10,40108,10,22,6,"Weekday",54,56]
[10,40110,10,24,3,"Saturday",43,49]
[10,40111,10,25,24,"Sunday",45,54]
[10,40116,10,30,16,"Weekday",46,64]
[10,40118,11,1,3,"Sunday",49,54]
[10,40122,11,5,10,"Weekday",55,74]
[10,40124,11,7,7,"Saturday",57,75]
[10,40126,11,9,4,"Weekday",38,46]
[10,40130,11,13,11,"Weekday",55,64]
[10,40133,11,16,23,"Weekday",48,51]
[10,40136,11,19,14,"Weekday",60,79]
[10,40138,11,21,11,"Saturday",54,58]
[10,40140,11,23,8,"Weekday",45,48]
[10,40144,11,27,15,"Weekday",58,79]
[10,40146,11,29,12,"Sunday",52,54]
[10,40151,12,4,6,"Weekday",40,47]
[10,40152,12,5,15,"Saturday",47,73]
[10,40154,12,7,12,"Weekday",50,74]
[10,40158,12,11,19,"Weekday",38,49]
[10,40160,12,13,16,"Sunday",42,59]
[10,40164,12,17,23,"Weekday",39,45]
[10,40166,12,19,19,"Saturday",44,48]
[10,40168,12,21,16,"Weekday",46,61]
[10,40172,12,25,23,"Weekday",35,40]
[10,40174,12,27,20,"Sunday",45,57]
[11,39814,1,1,14,"Weekday",42,43]
[11,39816,1,3,14,"Saturday",44,60]
[11,39820,1,7,17,"Weekday",39,40]
[11,39822,1,9,14,"Weekday",40,40]
[11,39823,1,10,24,"Saturday",33,35]
[11,39828,1,15,18,"Weekday",53,53]
[11,39830,1,17,4,"Saturday",34,36]
[11,39833,1,20,21,"Weekday",43,45]
[11,39836,1,23,18,"Weekday",48,51]
[11,39838,1,25,4,"Sunday",37,38]
[11,39842,1,29,22,"Weekday",48,49]
[11,39844,1,31,19,"Saturday",46,49]
[11,39849,2,5,2,"Weekday",38,50]
[11,39851,2,7,4,"Saturday",41,52]
[11,39852,2,8,8,"Sunday",30,32]
[11,39857,2,13,2,"Weekday",37,40]
[11,39858,2,14,23,"Saturday",49,53]
[11,39863,2,19,6,"Weekday",46,47]
[11,39865,2,21,3,"Saturday",42,44]
[11,39867,2,23,19,"Weekday",46,52]
[11,39871,2,27,6,"Weekday",39,47]
[11,39873,3,1,3,"Sunday",41,55]
[11,39877,3,5,10,"Weekday",52,56]
[11,39879,3,7,7,"Saturday",51,54]
[11,39881,3,9,4,"Weekday",57,59]
[11,39885,3,13,2,"Weekday",33,40]
[11,39887,3,15,7,"Sunday",39,42]
[11,39891,3,19,14,"Weekday",42,43]
[11,39893,3,21,11,"Saturday",48,52]
[11,39895,3,23,8,"Weekday",42,45]
[11,39899,3,27,15,"Weekday",55,70]
[11,39902,3,30,9,"Weekday",50,54]
[11,39905,4,2,18,"Weekday",53,69]
[11,39907,4,4,15,"Saturday",59,81]
[11,39912,4,9,9,"Weekday",51,56]
[11,39913,4,10,19,"Weekday",46,55]
[11,39915,4,12,16,"Sunday",57,73]
[11,39919,4,16,16,"Weekday",53,67]
[11,39921,4,18,19,"Saturday",47,62]
[11,39926,4,23,13,"Weekday",48,65]
[11,39927,4,24,23,"Weekday",39,48]
[11,39929,4,26,20,"Sunday",52,63]
[11,39934,5,1,14,"Weekday",58,84]
[11,39936,5,3,7,"Sunday",50,58]
[11,39940,5,7,17,"Weekday",55,82]
[11,39942,5,9,14,"Saturday",55,79]
[11,39946,5,13,21,"Weekday",48,51]
[11,39948,5,15,18,"Weekday",56,76]
[11,39950,5,17,4,"Sunday",48,53]
[11,39953,5,20,14,"Weekday",57,74]
[11,39956,5,23,18,"Saturday",56,71]
[11,39961,5,28,1,"Weekday",57,71]
[11,39962,5,29,22,"Weekday",53,70]
[11,39964,5,31,8,"Sunday",55,72]
[11,39967,6,3,7,"Weekday",52,67]
[11,39970,6,6,22,"Saturday",57,75]
[11,39975,6,11,5,"Weekday",48,57]
[11,39977,6,13,2,"Saturday",49,60]
[11,39978,6,14,23,"Sunday",56,64]
[11,39983,6,19,6,"Weekday",53,63]
[11,39984,6,20,14,"Saturday",65,96]
[11,39989,6,25,9,"Weekday",62,77]
[11,39991,6,27,6,"Saturday",52,58]
[11,39993,6,29,3,"Weekday",44,50]
[11,39997,7,3,10,"Weekday",60,80]
[11,39999,7,5,7,"Sunday",55,67]
[11,40001,7,7,21,"Weekday",61,76]
[11,40005,7,11,10,"Saturday",63,87]
[11,40007,7,13,7,"Weekday",55,77]
[11,40011,7,17,14,"Weekday",70,94]
[11,40013,7,19,11,"Sunday",60,71]
[11,40018,7,24,5,"Weekday",46,53]
[11,40021,7,27,8,"Weekday",54,73]
[11,40024,7,30,8,"Weekday",55,70]
[11,40025,7,31,18,"Weekday",62,91]
[11,40027,8,2,15,"Sunday",70,103]
[11,40032,8,7,9,"Weekday",61,78]
[11,40033,8,8,19,"Saturday",61,91]
[11,40038,8,13,15,"Weekday",63,82]
[11,40040,8,15,9,"Saturday",55,72]
[11,40041,8,16,19,"Sunday",61,82]
[11,40046,8,21,13,"Weekday",63,94]
[11,40047,8,22,23,"Saturday",58,78]
[11,40052,8,27,17,"Weekday",63,89]
[11,40053,8,28,2,"Weekday",53,62]
[11,40055,8,30,23,"Sunday",60,67]
[11,40060,9,4,17,"Weekday",64,91]
[11,40062,9,6,3,"Sunday",55,64]
[11,40066,9,10,21,"Weekday",58,69]
[11,40068,9,12,18,"Saturday",56,78]
[11,40072,9,16,13,"Weekday",60,96]
[11,40074,9,18,21,"Weekday",50,61]
[11,40076,9,20,18,"Sunday",59,77]
[11,40081,9,25,1,"Weekday",48,63]
[11,40082,9,26,22,"Saturday",54,67]
[11,40087,10,1,5,"Weekday",54,58]
[11,40089,10,3,20,"Saturday",47,66]
[11,40090,10,4,22,"Sunday",43,57]
[11,40095,10,9,5,"Weekday",48,56]
[11,40097,10,11,2,"Sunday",46,54]
[11,40098,10,12,23,"Weekday",50,55]
[11,40103,10,17,6,"Saturday",45,47]
[11,40107,10,21,3,"Weekday",44,54]
[11,40109,10,23,9,"Weekday",47,59]
[11,40111,10,25,6,"Sunday",40,50]
[11,40115,10,29,24,"Weekday",46,53]
[11,40117,10,31,10,"Saturday",54,67]
[11,40119,11,2,7,"Weekday",30,35]
[11,40123,11,6,18,"Weekday",49,64]
[11,40125,11,8,10,"Sunday",46,65]
[11,40130,11,13,4,"Weekday",42,51]
[11,40131,11,14,14,"Saturday",43,50]
[11,40133,11,16,11,"Weekday",45,46]
[11,40138,11,21,3,"Saturday",45,46]
[11,40139,11,22,14,"Sunday",49,62]
[11,40144,11,27,8,"Weekday",45,47]
[11,40145,11,28,18,"Saturday",53,56]
[11,40150,12,3,12,"Weekday",49,56]
[11,40152,12,5,9,"Saturday",38,40]
[11,40154,12,7,18,"Weekday",44,47]
[11,40158,12,11,12,"Weekday",34,46]
[11,40159,12,12,22,"Saturday",28,31]
[11,40164,12,17,16,"Weekday",48,50]
[11,40166,12,19,13,"Saturday",47,48]
[11,40167,12,20,23,"Sunday",51,53]
[11,{"$f":"DATE(2009,C96194,D96194)","v":40172},12,25,1,"Weekday",42,42]
[11,40174,12,27,13,"Sunday",43,46]
[11,40178,12,31,20,"Weekday",40,41]
[12,39815,1,2,17,"Weekday",40,49]
[12,39817,1,4,3,"Sunday",30,34]
[12,39821,1,8,21,"Weekday",39,43]
[12,39824,1,11,8,"Sunday",45,45]
[12,39827,1,14,24,"Weekday",45,48]
[12,39829,1,16,21,"Weekday",49,51]
[12,39831,1,18,18,"Sunday",52,53]
[12,39836,1,23,1,"Weekday",35,35]
[12,39837,1,24,22,"Saturday",37,37]
[12,39840,1,27,23,"Weekday",45,45]
[12,39844,1,31,1,"Saturday",41,42]
[12,39845,2,1,22,"Sunday",40,48]
[12,39850,2,6,5,"Weekday",37,38]
[12,39852,2,8,2,"Sunday",38,40]
[12,39856,2,12,9,"Weekday",43,44]
[12,39858,2,14,6,"Saturday",42,46]
[12,39862,2,18,23,"Weekday",48,50]
[12,39864,2,20,9,"Weekday",50,52]
[12,39866,2,22,6,"Sunday",42,43]
[12,39870,2,26,24,"Weekday",45,51]
[12,39872,2,28,10,"Saturday",52,59]
[12,39875,3,3,13,"Weekday",55,57]
[12,39878,3,6,13,"Weekday",48,62]
[12,39880,3,8,10,"Sunday",49,55]
[12,39885,3,13,4,"Weekday",45,47]
[12,39886,3,14,14,"Saturday",48,52]
[12,39891,3,19,8,"Weekday",41,47]
[12,39892,3,20,20,"Weekday",51,60]
[12,39894,3,22,14,"Sunday",57,68]
[12,39899,3,27,8,"Weekday",44,48]
[12,39900,3,28,18,"Saturday",53,68]
[12,39905,4,2,12,"Weekday",54,63]
[12,39907,4,4,9,"Saturday",49,53]
[12,39909,4,6,11,"Weekday",54,59]
[12,39913,4,10,12,"Weekday",54,66]
[12,39914,4,11,22,"Saturday",55,64]
[12,39919,4,16,16,"Weekday",59,80]
[12,39921,4,18,13,"Saturday",50,51]
[12,39925,4,22,20,"Weekday",51,55]
[12,39926,4,23,18,"Weekday",49,52]
[12,39929,4,26,13,"Sunday",53,61]
[12,39933,4,30,20,"Weekday",56,61]
[12,39935,5,2,17,"Saturday",57,69]
[12,39939,5,6,24,"Weekday",56,60]
[12,39940,5,7,11,"Weekday",64,76]
[12,39943,5,10,17,"Sunday",65,89]
[12,39947,5,14,24,"Weekday",50,54]
[12,39949,5,16,21,"Saturday",54,61]
[12,39954,5,21,4,"Weekday",41,43]
[12,39956,5,23,1,"Saturday",46,48]
[12,39957,5,24,18,"Sunday",55,64]
[12,39962,5,29,4,"Weekday",52,54]
[12,39964,5,31,1,"Sunday",58,63]
[12,39968,6,4,19,"Weekday",60,72]
[12,39970,6,6,5,"Saturday",52,57]
[12,39972,6,8,2,"Weekday",51,55]
[12,39977,6,13,5,"Saturday",50,54]
[12,39978,6,14,5,"Sunday",53,57]
[12,39982,6,18,23,"Weekday",56,61]
[12,39984,6,20,9,"Saturday",62,74]
[12,39989,6,25,3,"Weekday",51,56]
[12,39990,6,26,24,"Weekday",54,58]
[12,39994,6,30,12,"Weekday",67,87]
[12,39997,7,3,3,"Weekday",49,53]
[12,39998,7,4,13,"Saturday",59,69]
[12,40003,7,9,7,"Weekday",51,55]
[12,40005,7,11,4,"Saturday",57,64]
[12,40006,7,12,14,"Sunday",69,99]
[12,40011,7,17,19,"Weekday",65,80]
[12,40012,7,18,17,"Saturday",63,86]
[12,40017,7,23,11,"Weekday",67,88]
[12,40019,7,25,8,"Saturday",61,70]
[12,40020,7,26,18,"Sunday",65,88]
[12,40025,7,31,12,"Weekday",64,80]
[12,40029,8,4,2,"Weekday",56,58]
[12,40031,8,6,15,"Weekday",69,103]
[12,40033,8,8,12,"Saturday",68,87]
[12,40037,8,12,19,"Weekday",65,82]
[12,40039,8,14,16,"Weekday",64,81]
[12,40041,8,16,13,"Sunday",66,86]
[12,40045,8,20,17,"Weekday",69,102]
[12,40047,8,22,16,"Saturday",69,92]
[12,40049,8,24,13,"Weekday",69,87]
[12,40053,8,28,20,"Weekday",58,71]
[12,40055,8,30,17,"Sunday",61,73]
[12,40059,9,3,24,"Weekday",54,63]
[12,40062,9,6,24,"Sunday",52,56]
[12,40066,9,10,14,"Weekday",66,84]
[12,40067,9,11,24,"Weekday",49,55]
[12,40069,9,13,21,"Sunday",50,57]
[12,40074,9,18,4,"Weekday",60,64]
[12,40076,9,20,1,"Sunday",54,59]
[12,40080,9,24,7,"Weekday",51,53]
[12,40082,9,26,4,"Saturday",52,55]
[12,40084,9,28,1,"Weekday",53,68]
[12,40088,10,2,19,"Weekday",59,71]
[12,40090,10,4,5,"Sunday",49,54]
[12,40094,10,8,23,"Weekday",49,56]
[12,40096,10,10,22,"Saturday",55,59]
[12,40098,10,12,5,"Weekday",47,49]
[12,40102,10,16,23,"Weekday",53,58]
[12,40104,10,18,9,"Sunday",56,62]
[12,40109,10,23,3,"Weekday",40,49]
[12,40110,10,24,15,"Saturday",54,74]
[12,40115,10,29,6,"Weekday",40,43]
[12,40117,10,31,3,"Saturday",46,53]
[12,40118,11,1,13,"Sunday",61,71]
[12,40123,11,6,7,"Weekday",46,48]
[12,40125,11,8,4,"Sunday",50,53]
[12,40127,11,10,22,"Weekday",41,47]
[12,40131,11,14,7,"Saturday",44,46]
[12,40132,11,15,17,"Sunday",55,58]
[12,40137,11,20,11,"Weekday",47,52]
[12,40139,11,22,8,"Sunday",37,41]
[12,40143,11,26,15,"Weekday",50,57]
[12,40145,11,28,5,"Saturday",34,37]
[12,40147,11,30,8,"Weekday",39,46]
[12,40151,12,4,15,"Weekday",53,61]
[12,40153,12,6,12,"Sunday",53,57]
[12,40157,12,10,19,"Weekday",45,47]
[12,40159,12,12,16,"Saturday",50,51]
[12,40162,12,15,12,"Weekday",49,52]
[12,40165,12,18,19,"Weekday",43,43]
[12,40167,12,20,16,"Sunday",43,45]
[12,40171,12,24,23,"Weekday",34,38]
[12,40173,12,26,20,"Saturday",46,53]
[12,40175,12,28,17,"Weekday",42,50]
[13,39814,1,1,3,"Weekday",40,41]
[13,39816,1,3,20,"Saturday",45,45]
[13,39821,1,8,14,"Weekday",51,56]
[13,39822,1,9,24,"Weekday",41,41]
[13,39827,1,14,18,"Weekday",43,45]
[13,39829,1,16,4,"Weekday",35,36]
[13,39831,1,18,10,"Sunday",51,53]
[13,39835,1,22,18,"Weekday",41,43]
[13,39837,1,24,4,"Saturday",37,39]
[13,39841,1,28,22,"Weekday",47,47]
[13,39843,1,30,8,"Weekday",47,48]
[13,39845,2,1,5,"Sunday",47,49]
[13,39848,2,4,17,"Weekday",54,55]
[13,39851,2,7,8,"Saturday",53,53]
[13,39856,2,12,2,"Weekday",43,44]
[13,39857,2,13,23,"Weekday",51,51]
[13,39859,2,15,9,"Sunday",40,43]
[13,39864,2,20,3,"Weekday",49,50]
[13,39865,2,21,8,"Saturday",34,36]
[13,39870,2,26,6,"Weekday",40,41]
[13,39872,2,28,3,"Saturday",46,47]
[13,39876,3,4,10,"Weekday",55,65]
[13,39878,3,6,7,"Weekday",43,45]
[13,39880,3,8,4,"Sunday",52,54]
[13,39882,3,10,15,"Weekday",53,62]
[13,39886,3,14,7,"Saturday",38,40]
[13,39890,3,18,14,"Weekday",49,58]
[13,39892,3,20,11,"Weekday",51,60]
[13,39894,3,22,8,"Sunday",47,54]
[13,39898,3,26,15,"Weekday",55,65]
[13,39899,3,27,22,"Weekday",52,56]
[13,39904,4,1,18,"Weekday",58,76]
[13,39906,4,3,15,"Weekday",62,81]
[13,39908,4,5,12,"Sunday",63,79]
[13,39912,4,9,19,"Weekday",47,57]
[13,39916,4,13,11,"Weekday",51,64]
[13,{"$f":"DATE(2009,C107650,D107650)","v":39919},4,16,9,"Weekday",52,64]
[13,39920,4,17,19,"Weekday",53,65]
[13,39922,4,19,16,"Sunday",56,68]
[13,39926,4,23,23,"Weekday",54,62]
[13,39928,4,25,20,"Saturday",56,73]
[13,39933,4,30,18,"Weekday",52,63]
[13,39934,5,1,23,"Weekday",52,64]
[13,39936,5,3,20,"Sunday",60,76]
[13,39941,5,8,14,"Weekday",59,83]
[13,39942,5,9,24,"Saturday",51,58]
[13,39947,5,14,18,"Weekday",53,67]
[13,39950,5,17,9,"Sunday",59,73]
[13,39953,5,20,21,"Weekday",60,72]
[13,39955,5,22,18,"Weekday",54,72]
[13,39957,5,24,4,"Sunday",46,50]
[13,39961,5,28,22,"Weekday",61,79]
[13,39963,5,30,8,"Saturday",56,71]
[13,39967,6,3,16,"Weekday",56,80]
[13,39969,6,5,22,"Weekday",56,74]
[13,39971,6,7,8,"Sunday",57,73]
[13,39976,6,12,2,"Weekday",54,61]
[13,39977,6,13,23,"Saturday",52,59]
[13,39982,6,18,6,"Weekday",63,71]
[13,39984,6,20,23,"Saturday",60,82]
[13,39988,6,24,9,"Weekday",63,76]
[13,39990,6,26,6,"Weekday",56,62]
[13,39992,6,28,3,"Sunday",57,66]
[13,39996,7,2,10,"Weekday",65,84]
[13,39998,7,4,7,"Saturday",57,74]
[13,40001,7,7,14,"Weekday",64,91]
[13,40004,7,10,10,"Weekday",63,81]
[13,40006,7,12,7,"Sunday",62,76]
[13,40010,7,16,14,"Weekday",70,97]
[13,40012,7,18,11,"Saturday",68,92]
[13,40014,7,20,8,"Weekday",57,74]
[13,40018,7,24,21,"Weekday",64,85]
[13,40020,7,26,11,"Sunday",70,89]
[13,40024,7,30,18,"Weekday",63,92]
[13,40026,8,1,15,"Saturday",74,105]
[13,{"$f":"DATE(2009,C110338,D110338)","v":40031},8,6,9,"Weekday",68,77]
[13,40032,8,7,19,"Weekday",69,89]
[13,40036,8,11,4,"Weekday",61,65]
[13,{"$f":"DATE(2009,C110530,D110530)","v":40039},8,14,9,"Weekday",71,85]
[13,40040,8,15,19,"Saturday",67,96]
[13,40045,8,20,13,"Weekday",69,91]
[13,40046,8,21,23,"Weekday",57,72]
[13,40048,8,23,20,"Sunday",60,74]
[13,40053,8,28,11,"Weekday",66,82]
[13,40054,8,29,23,"Saturday",63,73]
[13,40059,9,3,17,"Weekday",64,86]
[13,40061,9,5,3,"Saturday",60,65]
[13,40062,9,6,24,"Sunday",64,73]
[13,40067,9,11,18,"Weekday",65,84]
[13,40070,9,14,2,"Weekday",58,65]
[13,40073,9,17,21,"Weekday",62,77]
[13,40075,9,19,18,"Saturday",54,74]
[13,40080,9,24,1,"Weekday",47,59]
[13,40081,9,25,22,"Weekday",57,69]
[13,40083,9,27,19,"Sunday",61,79]
[13,40088,10,2,1,"Weekday",61,66]
[13,40089,10,3,22,"Saturday",59,64]
[13,40094,10,8,5,"Weekday",52,55]
[13,40096,10,10,2,"Saturday",57,62]
[13,40097,10,11,23,"Sunday",56,61]
[13,40101,10,15,2,"Weekday",38,45]
[13,40104,10,18,2,"Sunday",42,51]
[13,40108,10,22,9,"Weekday",48,56]
[13,40110,10,24,6,"Saturday",46,52]
[13,40112,10,26,3,"Weekday",47,54]
[13,40116,10,30,10,"Weekday",59,69]
[13,40118,11,1,9,"Sunday",53,55]
[13,40122,11,5,13,"Weekday",57,66]
[13,40124,11,7,10,"Saturday",58,66]
[13,40126,11,9,7,"Weekday",40,41]
[13,40130,11,13,14,"Weekday",63,76]
[13,40132,11,15,11,"Sunday",55,58]
[13,40135,11,18,16,"Weekday",55,62]
[13,40138,11,21,14,"Saturday",56,58]
[13,40140,11,23,11,"Weekday",47,51]
[13,40144,11,27,18,"Weekday",47,51]
[13,40146,11,29,15,"Sunday",51,62]
[13,{"$f":"DATE(2009,C113218,D113218)","v":40151},12,4,9,"Weekday",39,39]
[13,40152,12,5,7,"Saturday",36,36]
[13,40157,12,10,12,"Weekday",50,59]
[13,40158,12,11,22,"Weekday",38,41]
[13,40160,12,13,19,"Sunday",46,49]
[13,40165,12,18,13,"Weekday",48,51]
[13,40166,12,19,23,"Saturday",36,39]
[13,40169,12,22,14,"Weekday",44,51]
[13,40173,12,26,13,"Saturday",47,51]
[13,40174,12,27,23,"Sunday",42,44]
[14,39814,1,1,17,"Weekday",35,48]
[14,39816,1,3,3,"Saturday",24,28]
[14,39820,1,7,21,"Weekday",25,32]
[14,39821,1,8,21,"Weekday",28,33]
[14,39826,1,13,24,"Weekday",36,42]
[14,39828,1,15,21,"Weekday",37,45]
[14,39830,1,17,18,"Saturday",35,48]
[14,39835,1,22,1,"Weekday",40,48]
[14,39836,1,23,22,"Weekday",34,41]
[14,39841,1,28,8,"Weekday",31,32]
[14,39843,1,30,1,"Weekday",41,44]
[14,39844,1,31,22,"Saturday",35,42]
[14,39849,2,5,5,"Weekday",35,44]
[14,39851,2,7,2,"Saturday",33,39]
[14,39855,2,11,9,"Weekday",45,52]
[14,39855,2,11,19,"Weekday",48,59]
[14,39859,2,15,2,"Sunday",34,42]
[14,39863,2,19,9,"Weekday",29,41]
[14,39865,2,21,6,"Saturday",30,38]
[14,39869,2,25,24,"Weekday",42,56]
[14,39871,2,27,10,"Weekday",32,44]
[14,39873,3,1,2,"Sunday",40,42]
[14,39877,3,5,13,"Weekday",51,68]
[14,39879,3,7,10,"Saturday",49,63]
[14,39884,3,12,4,"Weekday",38,50]
[14,39885,3,13,14,"Weekday",39,58]
[14,39889,3,17,15,"Weekday",38,48]
[14,39891,3,19,17,"Weekday",45,62]
[14,39893,3,21,14,"Saturday",40,59]
[14,39898,3,26,8,"Weekday",42,53]
[14,39899,3,27,18,"Weekday",48,66]
[14,39901,3,29,15,"Sunday",49,66]
[14,39906,4,3,22,"Weekday",43,65]
[14,39907,4,4,18,"Saturday",48,74]
[14,39912,4,9,12,"Weekday",51,71]
[14,39913,4,10,22,"Weekday",44,59]
[14,39918,4,15,16,"Weekday",55,82]
[14,39920,4,17,13,"Weekday",39,51]
[14,39923,4,20,13,"Weekday",46,61]
[14,39926,4,23,16,"Weekday",48,69]
[14,39928,4,25,13,"Saturday",41,57]
[14,39932,4,29,20,"Weekday",49,67]
[14,39934,5,1,17,"Weekday",48,68]
[14,39936,5,3,3,"Sunday",39,47]
[14,39940,5,7,20,"Weekday",50,67]
[14,39942,5,9,17,"Saturday",55,85]
[14,39946,5,13,24,"Weekday",42,52]
[14,39948,5,15,21,"Weekday",44,62]
[14,39953,5,20,4,"Weekday",48,64]
[14,39955,5,22,1,"Weekday",46,63]
[14,39958,5,25,3,"Weekday",37,53]
[14,39961,5,28,4,"Weekday",45,58]
[14,39963,5,30,1,"Saturday",45,65]
[14,39964,5,31,22,"Sunday",51,69]
[14,39969,6,5,5,"Weekday",46,67]
[14,39971,6,7,2,"Sunday",41,54]
[14,39974,6,10,18,"Weekday",51,67]
[14,39977,6,13,5,"Saturday",50,63]
[14,39979,6,15,2,"Weekday",42,61]
[14,39983,6,19,9,"Weekday",54,80]
[14,39985,6,21,6,"Sunday",42,56]
[14,39989,6,25,24,"Weekday",55,81]
[14,39992,6,28,1,"Sunday",50,69]
[14,39996,7,2,3,"Weekday",45,65]
[14,39997,7,3,13,"Weekday",59,81]
[14,39999,7,5,10,"Sunday",52,75]
[14,40004,7,10,4,"Weekday",50,71]
[14,40005,7,11,14,"Saturday",63,103]
[14,40009,7,15,8,"Weekday",54,79]
[14,40011,7,17,17,"Weekday",63,103]
[14,40013,7,19,14,"Sunday",65,102]
[14,40018,7,24,8,"Weekday",55,79]
[14,40019,7,25,18,"Saturday",61,92]
[14,40024,7,30,12,"Weekday",56,86]
[14,40026,8,1,15,"Saturday",62,99]
[14,40030,8,5,15,"Weekday",64,102]
[14,40032,8,7,12,"Weekday",61,99]
[14,40033,8,8,22,"Saturday",57,85]
[14,40038,8,13,16,"Weekday",61,97]
[14,40040,8,15,13,"Saturday",60,92]
[14,40043,8,18,6,"Weekday",53,71]
[14,40046,8,21,16,"Weekday",60,89]
[14,40048,8,23,2,"Sunday",50,70]
[14,40052,8,27,20,"Weekday",54,82]
[14,40054,8,29,17,"Saturday",61,93]
[14,40056,8,31,23,"Weekday",47,71]
[14,40060,9,4,20,"Weekday",55,77]
[14,40062,9,6,17,"Sunday",59,91]
[14,40066,9,10,24,"Weekday",52,71]
[14,40068,9,12,21,"Saturday",56,79]
[14,40073,9,17,4,"Weekday",50,60]
[14,40074,9,18,6,"Weekday",47,58]
[14,40076,9,20,21,"Sunday",48,68]
[14,40081,9,25,4,"Weekday",39,53]
[14,40083,9,27,1,"Sunday",44,54]
[14,40087,10,1,19,"Weekday",46,71]
[14,40089,10,3,5,"Saturday",48,64]
[14,40091,10,5,13,"Weekday",60,86]
[14,40095,10,9,8,"Weekday",36,51]
[14,40097,10,11,5,"Sunday",38,51]
[14,40101,10,15,23,"Weekday",42,60]
[14,40103,10,17,9,"Saturday",35,50]
[14,40105,10,19,6,"Weekday",39,51]
[14,40108,10,22,4,"Weekday",42,54]
[14,40111,10,25,9,"Sunday",42,54]
[14,40116,10,30,3,"Weekday",31,43]
[14,40117,10,31,13,"Saturday",48,75]
[14,40122,11,5,7,"Weekday",44,50]
[14,40124,11,7,4,"Saturday",38,42]
[14,40125,11,8,11,"Sunday",45,59]
[14,40130,11,13,7,"Weekday",38,45]
[14,40131,11,14,17,"Saturday",52,68]
[14,40136,11,19,11,"Weekday",40,53]
[14,40138,11,21,8,"Saturday",35,42]
[14,40139,11,22,18,"Sunday",37,47]
[14,40142,11,25,18,"Weekday",39,56]
[14,40145,11,28,21,"Saturday",34,40]
[14,40150,12,3,15,"Weekday",43,57]
[14,40152,12,5,12,"Saturday",42,54]
[14,40156,12,9,19,"Weekday",34,43]
[14,40158,12,11,16,"Weekday",41,54]
[14,40160,12,13,1,"Sunday",34,39]
[14,40164,12,17,19,"Weekday",34,43]
[14,40166,12,19,16,"Saturday",44,63]
[14,40170,12,23,23,"Weekday",25,33]
[14,40172,12,25,20,"Weekday",33,44]
[14,40174,12,27,17,"Sunday",38,49]
[15,39814,1,1,12,"Weekday",43,64]
[15,39815,1,2,20,"Weekday",36,49]
[15,39817,1,4,17,"Sunday",44,65]
[15,39821,1,8,24,"Weekday",42,53]
[15,39823,1,10,21,"Saturday",37,50]
[15,39828,1,15,4,"Weekday",41,42]
[15,39831,1,18,19,"Sunday",51,62]
[15,39834,1,21,18,"Weekday",52,59]
[15,39836,1,23,4,"Weekday",43,44]
[15,39838,1,25,1,"Sunday",51,61]
[15,39842,1,29,8,"Weekday",46,56]
[15,39844,1,31,5,"Saturday",47,58]
[15,39849,2,5,2,"Weekday",39,46]
[15,39850,2,6,8,"Weekday",49,55]
[15,39852,2,8,5,"Sunday",42,47]
[15,39856,2,12,23,"Weekday",49,60]
[15,39858,2,14,9,"Saturday",44,63]
[15,39862,2,18,19,"Weekday",49,60]
[15,39864,2,20,12,"Weekday",49,68]
[15,39869,2,25,6,"Weekday",39,45]
[15,39871,2,27,3,"Weekday",38,47]
[15,39872,2,28,13,"Saturday",51,76]
[15,39877,3,5,7,"Weekday",37,49]
[15,39880,3,8,2,"Sunday",42,54]
[15,39883,3,11,10,"Weekday",45,68]
[15,39885,3,13,7,"Weekday",36,51]
[15,39886,3,14,17,"Saturday",53,81]
[15,39891,3,19,11,"Weekday",48,73]
[15,39893,3,21,8,"Saturday",47,66]
[15,39896,3,24,17,"Weekday",54,86]
[15,39899,3,27,11,"Weekday",55,76]
[15,39900,3,28,21,"Saturday",42,61]
[15,39905,4,2,15,"Weekday",60,93]
[15,39907,4,4,12,"Saturday",58,89]
[15,39911,4,8,19,"Weekday",54,69]
[15,39913,4,10,24,"Weekday",49,59]
[15,39915,4,12,12,"Sunday",59,80]
[15,39919,4,16,19,"Weekday",54,75]
[15,39921,4,18,16,"Saturday",62,92]
[15,39925,4,22,23,"Weekday",57,70]
[15,39927,4,24,20,"Weekday",60,78]
[15,39931,4,28,7,"Weekday",53,73]
[15,39933,4,30,23,"Weekday",47,57]
[15,39935,5,2,20,"Saturday",57,76]
[15,39940,5,7,3,"Weekday",56,57]
[15,39941,5,8,24,"Weekday",52,69]
[15,39943,5,10,21,"Sunday",57,83]
[15,39947,5,14,22,"Weekday",57,60]
[15,39949,5,16,24,"Saturday",58,68]
[15,39954,5,21,18,"Weekday",63,89]
[15,39956,5,23,4,"Saturday",54,64]
[15,39960,5,27,22,"Weekday",56,82]
[15,39962,5,29,8,"Weekday",56,84]
[15,39965,6,1,5,"Weekday",57,80]
[15,39968,6,4,22,"Weekday",60,90]
[15,39970,6,6,8,"Saturday",61,83]
[15,39975,6,11,2,"Weekday",54,73]
[15,39976,6,12,23,"Weekday",56,75]
[15,39978,6,14,9,"Sunday",58,86]
[15,39982,6,18,12,"Weekday",63,102]
[15,39984,6,20,12,"Saturday",65,104]
[15,39989,6,25,6,"Weekday",58,78]
[15,39991,6,27,3,"Saturday",52,76]
[15,39995,7,1,10,"Weekday",64,95]
[15,39997,7,3,7,"Weekday",63,81]
[15,39999,7,5,3,"Sunday",59,74]
[15,40003,7,9,10,"Weekday",70,98]
[15,40005,7,11,7,"Saturday",54,83]
[15,40009,7,15,14,"Weekday",75,103]
[15,40011,7,17,11,"Weekday",74,100]
[15,40013,7,19,8,"Sunday",72,91]
[15,40016,7,22,10,"Weekday",72,97]
[15,40019,7,25,11,"Saturday",71,94]
[15,40023,7,29,18,"Weekday",70,99]
[15,40025,7,31,15,"Weekday",75,112]
[15,40027,8,2,12,"Sunday",65,99]
[15,40030,8,5,3,"Weekday",51,73]
[15,40033,8,8,15,"Saturday",74,108]
[15,40038,8,13,9,"Weekday",71,98]
[15,40039,8,14,19,"Weekday",71,90]
[15,40041,8,16,16,"Sunday",69,113]
[15,40045,8,20,23,"Weekday",71,94]
[15,40047,8,22,10,"Saturday",70,98]
[15,40052,8,27,13,"Weekday",74,98]
[15,40053,8,28,23,"Weekday",59,78]
[15,40055,8,30,20,"Sunday",54,86]
[15,40060,9,4,3,"Weekday",56,72]
[15,40061,9,5,24,"Saturday",59,80]
[15,40064,9,8,17,"Weekday",69,105]
[15,40068,9,12,3,"Saturday",54,78]
[15,40072,9,16,21,"Weekday",58,87]
[15,40074,9,18,18,"Weekday",61,89]
[15,40076,9,20,4,"Sunday",52,73]
[15,40080,9,24,22,"Weekday",50,75]
[15,40084,9,28,4,"Weekday",51,60]
[15,40087,10,1,1,"Weekday",52,71]
[15,40088,10,2,22,"Weekday",52,75]
[15,40090,10,4,8,"Sunday",53,80]
[15,40095,10,9,2,"Weekday",46,65]
[15,40096,10,10,12,"Saturday",66,97]
[15,40101,10,15,11,"Weekday",60,87]
[15,40103,10,17,2,"Saturday",50,67]
[15,40104,10,18,12,"Sunday",63,89]
[15,40109,10,23,6,"Weekday",43,52]
[15,40111,10,25,3,"Sunday",44,54]
[15,40115,10,29,10,"Weekday",55,77]
[15,40118,11,1,18,"Sunday",64,75]
[15,40121,11,4,13,"Weekday",58,87]
[15,40123,11,6,10,"Weekday",52,74]
[15,40125,11,8,7,"Sunday",41,49]
[15,40129,11,12,14,"Weekday",60,78]
[15,40131,11,14,11,"Saturday",58,75]
[15,40133,11,16,5,"Weekday",40,55]
[15,40137,11,20,14,"Weekday",55,74]
[15,40139,11,22,11,"Sunday",53,66]
[15,40143,11,26,18,"Weekday",48,64]
[15,40145,11,28,15,"Saturday",57,72]
[15,40147,11,30,12,"Weekday",53,68]
[15,40152,12,5,16,"Saturday",55,72]
[15,40153,12,6,15,"Sunday",57,70]
[15,40157,12,10,22,"Weekday",43,52]
[15,40159,12,12,19,"Saturday",45,55]
[15,40164,12,17,13,"Weekday",46,69]
[15,40165,12,18,23,"Weekday",42,54]
[15,40169,12,22,23,"Weekday",29,39]
[15,40172,12,25,13,"Weekday",44,62]
[15,40173,12,26,23,"Saturday",37,52]
[15,{"$f":"DATE(2009,C131394,D131394)","v":40178},12,31,17,"Weekday",43,59]
[16,39815,1,2,3,"Weekday",29,31]
[16,39816,1,3,24,"Saturday",35,36]
[16,39822,1,9,6,"Weekday",22,24]
[16,39823,1,10,3,"Saturday",28,30]
[16,39827,1,14,21,"Weekday",40,43]
[16,39829,1,16,7,"Weekday",19,20]
[16,39834,1,21,1,"Weekday",18,22]
[16,39835,1,22,23,"Weekday",27,28]
[16,39837,1,24,7,"Saturday",24,24]
[16,39842,1,29,1,"Weekday",40,45]
[16,39843,1,30,22,"Weekday",30,32]
[16,39848,2,4,5,"Weekday",15,16]
[16,39850,2,6,2,"Weekday",19,22]
[16,39852,2,8,14,"Sunday",39,42]
[16,39856,2,12,5,"Weekday",23,25]
[16,39858,2,14,2,"Saturday",36,37]
[16,39862,2,18,9,"Weekday",37,45]
[16,39864,2,20,6,"Weekday",35,35]
[16,39866,2,22,3,"Sunday",40,42]
[16,39869,2,25,21,"Weekday",45,47]
[16,39872,2,28,6,"Saturday",25,27]
[16,39876,3,4,13,"Weekday",51,62]
[16,39878,3,6,10,"Weekday",39,44]
[16,39880,3,8,7,"Sunday",23,25]
[16,39884,3,12,14,"Weekday",30,30]
[16,39887,3,15,4,"Sunday",37,38]
[16,39890,3,18,17,"Weekday",37,43]
[16,39892,3,20,14,"Weekday",45,62]
[16,39894,3,22,11,"Sunday",45,54]
[16,39898,3,26,18,"Weekday",43,52]
[16,39900,3,28,15,"Saturday",47,59]
[16,39904,4,1,11,"Weekday",40,47]
[16,39906,4,3,18,"Weekday",45,54]
[16,39911,4,8,12,"Weekday",46,65]
[16,39912,4,9,22,"Weekday",39,47]
[16,39914,4,11,19,"Saturday",45,47]
[16,39919,4,16,13,"Weekday",40,48]
[16,39921,4,18,2,"Saturday",37,38]
[16,39925,4,22,16,"Weekday",50,66]
[16,39927,4,24,13,"Weekday",43,57]
[16,39928,4,25,23,"Saturday",39,46]
[16,{"$f":"DATE(2009,C134274,D134274)","v":39933},4,30,17,"Weekday",49,63]
[16,39935,5,2,3,"Saturday",32,40]
[16,39938,5,5,9,"Weekday",45,55]
[16,{"$f":"DATE(2009,C134466,D134466)","v":39941},5,8,17,"Weekday",54,70]
[16,39943,5,10,3,"Sunday",38,45]
[16,39947,5,14,21,"Weekday",50,55]
[16,39949,5,16,7,"Saturday",30,36]
[16,39954,5,21,1,"Weekday",44,48]
[16,39955,5,22,16,"Weekday",53,63]
[16,39960,5,27,4,"Weekday",35,40]
[16,39962,5,29,1,"Weekday",49,57]
[16,39963,5,30,22,"Saturday",49,64]
[16,39968,6,4,5,"Weekday",36,41]
[16,39970,6,6,2,"Saturday",39,45]
[16,39972,6,8,7,"Weekday",39,43]
[16,39976,6,12,5,"Weekday",47,55]
[16,39978,6,14,2,"Sunday",55,64]
[16,39982,6,18,9,"Weekday",52,62]
[16,39984,6,20,6,"Saturday",47,55]
[16,39988,6,24,13,"Weekday",56,74]
[16,39989,6,25,14,"Weekday",63,80]
[16,39992,6,28,6,"Sunday",46,50]
[16,39996,7,2,13,"Weekday",67,93]
[16,39998,7,4,10,"Saturday",57,69]
[16,40003,7,9,4,"Weekday",46,53]
[16,40006,7,12,3,"Sunday",59,64]
[16,40006,7,12,10,"Sunday",56,62]
[16,40010,7,16,17,"Weekday",64,79]
[16,40012,7,18,14,"Saturday",67,88]
[16,40017,7,23,8,"Weekday",44,54]
[16,40018,7,24,18,"Weekday",60,78]
[16,40020,7,26,14,"Sunday",68,93]
[16,40025,7,31,8,"Weekday",52,65]
[16,40026,8,1,18,"Saturday",53,76]
[16,40031,8,6,12,"Weekday",61,88]
[16,40032,8,7,22,"Weekday",49,60]
[16,40037,8,12,16,"Weekday",59,82]
[16,40037,8,12,21,"Weekday",50,62]
[16,40040,8,15,22,"Saturday",49,56]
[16,40045,8,20,16,"Weekday",60,76]
[16,40047,8,22,2,"Saturday",44,49]
[16,40051,8,26,20,"Weekday",51,69]
[16,{"$f":"DATE(2009,C137154,D137154)","v":40053},8,28,17,"Weekday",61,81]
[16,40057,9,1,8,"Weekday",45,54]
[16,40059,9,3,20,"Weekday",54,74]
[16,{"$f":"DATE(2009,C137346,D137346)","v":40061},9,5,17,"Saturday",56,79]
[16,40065,9,9,24,"Weekday",45,57]
[16,40067,9,11,21,"Weekday",40,47]
[16,40069,9,13,7,"Sunday",36,37]
[16,40074,9,18,15,"Weekday",50,55]
[16,40075,9,19,21,"Saturday",53,61]
[16,40080,9,24,4,"Weekday",48,57]
[16,40082,9,26,1,"Saturday",50,57]
[16,40086,9,30,8,"Weekday",43,51]
[16,40088,10,2,5,"Weekday",34,36]
[16,40091,10,5,22,"Weekday",36,45]
[16,40094,10,8,8,"Weekday",49,56]
[16,40096,10,10,5,"Saturday",47,49]
[16,40098,10,12,2,"Weekday",33,35]
[16,40102,10,16,9,"Weekday",47,55]
[16,40104,10,18,6,"Sunday",48,50]
[16,40108,10,22,13,"Weekday",50,64]
[16,40110,10,24,9,"Saturday",42,47]
[16,40115,10,29,3,"Weekday",31,34]
[16,40116,10,30,13,"Weekday",52,68]
[16,40118,11,1,10,"Sunday",43,51]
[16,40123,11,6,4,"Weekday",37,37]
[16,40125,11,8,20,"Sunday",46,47]
[16,40129,11,12,7,"Weekday",31,35]
[16,40130,11,13,17,"Weekday",39,41]
[16,40132,11,15,14,"Sunday",46,52]
[16,40137,11,20,8,"Weekday",31,32]
[16,40138,11,21,18,"Saturday",41,47]
[16,40143,11,26,3,"Weekday",27,29]
[16,40144,11,27,21,"Weekday",37,42]
[16,40146,11,29,18,"Sunday",41,48]
[16,40151,12,4,12,"Weekday",36,37]
[16,40152,12,5,22,"Saturday",43,45]
[16,40157,12,10,16,"Weekday",42,49]
[16,40158,12,11,5,"Weekday",24,25]
[16,40158,12,11,6,"Weekday",26,28]
[16,40158,12,11,7,"Weekday",28,30]
[16,40158,12,11,8,"Weekday",30,32]
[16,40158,12,11,9,"Weekday",32,35]
[16,40158,12,11,10,"Weekday",34,37]
[16,40158,12,11,11,"Weekday",38,41]
[16,40158,12,11,12,"Weekday",40,45]
[16,40158,12,11,13,"Weekday",43,49]
[16,40158,12,11,14,"Weekday",43,48]
[16,40158,12,11,15,"Weekday",42,47]
[16,40158,12,11,16,"Weekday",42,46]
[16,40158,12,11,17,"Weekday",40,43]
[16,40158,12,11,18,"Weekday",37,40]
[16,40158,12,11,19,"Weekday",35,37]
[16,40158,12,11,20,"Weekday",33,35]
[16,40158,12,11,21,"Weekday",31,32]
[16,40158,12,11,22,"Weekday",29,30]
[16,40158,12,11,23,"Weekday",29,30]
[16,40158,12,11,24,"Weekday",32,33]
[16,40159,12,12,1,"Saturday",34,36]
[16,40159,12,12,2,"Saturday",36,38]
[16,40159,12,12,3,"Saturday",36,38]
[16,40159,12,12,4,"Saturday",36,38]
[16,40159,12,12,5,"Saturday",34,36]
[16,40159,12,12,6,"Saturday",32,34]
[16,40159,12,12,7,"Saturday",29,31]
[16,40159,12,12,8,"Saturday",28,30]
[16,40159,12,12,9,"Saturday",27,29]
[16,40159,12,12,10,"Saturday",26,28]
[16,40159,12,12,11,"Saturday",27,29]
[16,40159,12,12,12,"Saturday",28,30]
[16,40159,12,12,13,"Saturday",29,31]
[16,40159,12,12,14,"Saturday",28,31]
[16,40159,12,12,15,"Saturday",28,31]
[16,40159,12,12,16,"Saturday",27,30]
[16,40159,12,12,17,"Saturday",26,29]
[16,40159,12,12,18,"Saturday",25,28]
[16,40159,12,12,19,"Saturday",24,26]
[16,40159,12,12,20,"Saturday",24,26]
[16,40159,12,12,21,"Saturday",24,26]
[16,40159,12,12,22,"Saturday",24,26]
[16,40159,12,12,23,"Saturday",24,26]
[16,40159,12,12,24,"Saturday",25,27]
[16,40160,12,13,1,"Sunday",25,28]
[16,40160,12,13,2,"Sunday",26,28]
[16,40160,12,13,3,"Sunday",26,27]
[16,40160,12,13,4,"Sunday",25,26]
[16,40160,12,13,5,"Sunday",27,29]
[16,40160,12,13,6,"Sunday",28,31]
[16,40160,12,13,7,"Sunday",29,32]
[16,40160,12,13,8,"Sunday",29,33]
[16,{"$f":"DATE(2009,C139714,D139714)","v":40160},12,13,9,"Sunday",29,33]
[16,40160,12,13,10,"Sunday",28,32]
[16,40160,12,13,11,"Sunday",30,35]
[16,40160,12,13,12,"Sunday",31,36]
[16,40160,12,13,13,"Sunday",33,38]
[16,40160,12,13,14,"Sunday",31,36]
[16,40160,12,13,15,"Sunday",31,35]
[16,40160,12,13,16,"Sunday",29,32]
[16,40160,12,13,17,"Sunday",29,32]
[16,40160,12,13,18,"Sunday",28,31]
[16,40160,12,13,19,"Sunday",27,30]
[16,40160,12,13,20,"Sunday",28,31]
[16,40160,12,13,21,"Sunday",29,32]
[16,40160,12,13,22,"Sunday",29,32]
[16,40160,12,13,23,"Sunday",29,32]
[16,40160,12,13,24,"Sunday",28,31]
[16,40161,12,14,1,"Weekday",28,31]
[16,40161,12,14,2,"Weekday",27,30]
[16,40161,12,14,3,"Weekday",27,29]
[16,40161,12,14,4,"Weekday",26,28]
[16,40161,12,14,5,"Weekday",26,28]
[16,40161,12,14,6,"Weekday",26,28]
[16,40161,12,14,7,"Weekday",25,27]
[16,40161,12,14,8,"Weekday",25,28]
[16,40161,12,14,9,"Weekday",25,28]
[16,40161,12,14,10,"Weekday",25,28]
[16,40161,12,14,11,"Weekday",29,32]
[16,40161,12,14,12,"Weekday",32,36]
[16,40161,12,14,13,"Weekday",34,40]
[16,40161,12,14,14,"Weekday",34,39]
[16,40161,12,14,15,"Weekday",34,38]
[16,40161,12,14,16,"Weekday",34,38]
[16,40161,12,14,17,"Weekday",32,36]
[16,40161,12,14,18,"Weekday",30,33]
[16,40161,12,14,19,"Weekday",28,30]
[16,40161,12,14,20,"Weekday",26,28]
[16,40161,12,14,21,"Weekday",24,26]
[16,40161,12,14,22,"Weekday",21,23]
[16,40161,12,14,23,"Weekday",20,22]
[16,40161,12,14,24,"Weekday",20,21]
[16,40162,12,15,1,"Weekday",20,22]
[16,40162,12,15,2,"Weekday",21,22]
[16,40162,12,15,3,"Weekday",21,22]
[16,40162,12,15,4,"Weekday",21,22]
[16,40162,12,15,5,"Weekday",22,22]
[16,40162,12,15,6,"Weekday",22,22]
[16,40162,12,15,7,"Weekday",21,22]
[16,40162,12,15,8,"Weekday",27,29]
[16,40162,12,15,9,"Weekday",32,36]
[16,40162,12,15,10,"Weekday",38,42]
[16,40162,12,15,11,"Weekday",38,42]
[16,40162,12,15,12,"Weekday",38,42]
[16,40162,12,15,13,"Weekday",38,42]
[16,40162,12,15,14,"Weekday",38,41]
[16,40162,12,15,15,"Weekday",37,41]
[16,40162,12,15,16,"Weekday",37,40]
[16,40162,12,15,17,"Weekday",37,40]
[16,40162,12,15,18,"Weekday",37,40]
[16,40162,12,15,19,"Weekday",37,40]
[16,40162,12,15,20,"Weekday",35,38]
[16,40162,12,15,21,"Weekday",34,37]
[16,40162,12,15,22,"Weekday",32,35]
[16,40162,12,15,23,"Weekday",30,32]
[16,40162,12,15,24,"Weekday",28,30]
[16,{"$f":"DATE(2009,C139778,D139778)","v":40163},12,16,1,"Weekday",27,29]
[16,40163,12,16,2,"Weekday",27,29]
[16,40163,12,16,3,"Weekday",28,30]
[16,40163,12,16,4,"Weekday",30,31]
[16,40163,12,16,5,"Weekday",30,31]
[16,40163,12,16,6,"Weekday",30,31]
[16,40163,12,16,7,"Weekday",30,31]
[16,40163,12,16,8,"Weekday",32,33]
[16,40163,12,16,9,"Weekday",33,35]
[16,40163,12,16,10,"Weekday",35,37]
[16,40163,12,16,11,"Weekday",37,40]
[16,40163,12,16,12,"Weekday",40,43]
[16,40163,12,16,13,"Weekday",43,46]
[16,40163,12,16,14,"Weekday",41,44]
[16,40163,12,16,15,"Weekday",40,42]
[16,40163,12,16,16,"Weekday",38,40]
[16,40163,12,16,17,"Weekday",37,39]
[16,40163,12,16,18,"Weekday",36,38]
[16,40163,12,16,19,"Weekday",35,37]
[16,40163,12,16,20,"Weekday",35,36]
[16,40163,12,16,21,"Weekday",34,35]
[16,40163,12,16,22,"Weekday",34,35]
[16,40163,12,16,23,"Weekday",34,35]
[16,40163,12,16,24,"Weekday",35,35]
[16,40164,12,17,1,"Weekday",35,36]
[16,40164,12,17,2,"Weekday",36,37]
[16,40164,12,17,3,"Weekday",36,37]
[16,40164,12,17,4,"Weekday",36,37]
[16,40164,12,17,5,"Weekday",35,36]
[16,40164,12,17,6,"Weekday",33,35]
[16,40164,12,17,7,"Weekday",32,33]
[16,40164,12,17,8,"Weekday",34,36]
[16,40164,12,17,9,"Weekday",36,38]
[16,40164,12,17,10,"Weekday",39,40]
[16,40164,12,17,11,"Weekday",39,42]
[16,40164,12,17,12,"Weekday",40,43]
[16,40164,12,17,13,"Weekday",41,44]
[16,40164,12,17,14,"Weekday",39,41]
[16,40164,12,17,15,"Weekday",36,38]
[16,40164,12,17,16,"Weekday",34,35]
[16,40164,12,17,17,"Weekday",32,33]
[16,40164,12,17,18,"Weekday",30,32]
[16,40164,12,17,19,"Weekday",27,29]
[16,40164,12,17,20,"Weekday",27,29]
[16,40164,12,17,21,"Weekday",26,28]
[16,40164,12,17,22,"Weekday",24,26]
[16,40164,12,17,23,"Weekday",23,24]
[16,40164,12,17,24,"Weekday",21,23]
[16,40165,12,18,1,"Weekday",20,22]
[16,40165,12,18,2,"Weekday",20,22]
[16,40165,12,18,3,"Weekday",20,22]
[16,40165,12,18,4,"Weekday",19,22]
[16,40165,12,18,5,"Weekday",19,21]
[16,40165,12,18,6,"Weekday",18,21]
[16,40165,12,18,7,"Weekday",18,20]
[16,40165,12,18,8,"Weekday",24,26]
[16,40165,12,18,9,"Weekday",29,32]
[16,40165,12,18,10,"Weekday",36,39]
[16,40165,12,18,11,"Weekday",38,42]
[16,40165,12,18,12,"Weekday",40,46]
[16,40165,12,18,13,"Weekday",43,49]
[16,40165,12,18,14,"Weekday",42,48]
[16,40165,12,18,15,"Weekday",41,47]
[16,40165,12,18,16,"Weekday",41,45]
[16,{"$f":"DATE(2009,C139842,D139842)","v":40165},12,18,17,"Weekday",36,40]
[16,40165,12,18,18,"Weekday",31,34]
[16,40165,12,18,19,"Weekday",26,28]
[16,40165,12,18,20,"Weekday",25,27]
[16,40165,12,18,21,"Weekday",24,25]
[16,40165,12,18,22,"Weekday",21,23]
[16,40165,12,18,23,"Weekday",20,21]
[16,40165,12,18,24,"Weekday",19,20]
[16,40166,12,19,1,"Saturday",18,20]
[16,40166,12,19,2,"Saturday",18,20]
[16,40166,12,19,3,"Saturday",18,20]
[16,40166,12,19,4,"Saturday",18,20]
[16,40166,12,19,5,"Saturday",17,19]
[16,40166,12,19,6,"Saturday",17,19]
[16,40166,12,19,7,"Saturday",15,17]
[16,40166,12,19,8,"Saturday",22,26]
[16,40166,12,19,9,"Saturday",28,33]
[16,40166,12,19,10,"Saturday",34,42]
[16,40166,12,19,11,"Saturday",37,45]
[16,40166,12,19,12,"Saturday",40,49]
[16,40166,12,19,13,"Saturday",42,52]
[16,40166,12,19,14,"Saturday",41,51]
[16,40166,12,19,15,"Saturday",40,49]
[16,40166,12,19,16,"Saturday",39,47]
[16,40166,12,19,17,"Saturday",34,41]
[16,40166,12,19,18,"Saturday",30,34]
[16,40166,12,19,19,"Saturday",25,28]
[16,40166,12,19,20,"Saturday",24,27]
[16,40166,12,19,21,"Saturday",23,26]
[16,40166,12,19,22,"Saturday",22,25]
[16,40166,12,19,23,"Saturday",21,23]
[16,40166,12,19,24,"Saturday",19,21]
[16,40167,12,20,1,"Sunday",18,20]
[16,40167,12,20,2,"Sunday",16,18]
[16,40167,12,20,3,"Sunday",15,16]
[16,40167,12,20,4,"Sunday",13,15]
[16,40167,12,20,5,"Sunday",13,14]
[16,40167,12,20,6,"Sunday",12,13]
[16,40167,12,20,7,"Sunday",11,12]
[16,40167,12,20,8,"Sunday",15,17]
[16,40167,12,20,9,"Sunday",20,22]
[16,40167,12,20,10,"Sunday",24,26]
[16,40167,12,20,11,"Sunday",30,36]
[16,40167,12,20,12,"Sunday",36,45]
[16,40167,12,20,13,"Sunday",42,55]
[16,40167,12,20,14,"Sunday",41,53]
[16,40167,12,20,15,"Sunday",40,52]
[16,40167,12,20,16,"Sunday",39,51]
[16,40167,12,20,17,"Sunday",36,46]
[16,40167,12,20,18,"Sunday",34,42]
[16,40167,12,20,19,"Sunday",31,38]
[16,40167,12,20,20,"Sunday",29,36]
[16,40167,12,20,21,"Sunday",28,34]
[16,40167,12,20,22,"Sunday",27,32]
[16,40167,12,20,23,"Sunday",26,31]
[16,40167,12,20,24,"Sunday",26,31]
[16,40168,12,21,1,"Weekday",27,32]
[16,40168,12,21,2,"Weekday",29,34]
[16,40168,12,21,3,"Weekday",31,37]
[16,40168,12,21,4,"Weekday",33,39]
[16,40168,12,21,5,"Weekday",34,41]
[16,40168,12,21,6,"Weekday",35,42]
[16,40168,12,21,7,"Weekday",36,43]
[16,40168,12,21,8,"Weekday",36,41]
[16,{"$f":"DATE(2009,C139906,D139906)","v":40168},12,21,9,"Weekday",35,39]
[16,40168,12,21,10,"Weekday",34,37]
[16,40168,12,21,11,"Weekday",34,37]
[16,40168,12,21,12,"Weekday",33,36]
[16,40168,12,21,13,"Weekday",33,35]
[16,40168,12,21,14,"Weekday",34,36]
[16,40168,12,21,15,"Weekday",35,37]
[16,40168,12,21,16,"Weekday",36,37]
[16,40168,12,21,17,"Weekday",35,36]
[16,40168,12,21,18,"Weekday",34,35]
[16,40168,12,21,19,"Weekday",33,33]
[16,40168,12,21,20,"Weekday",32,33]
[16,40168,12,21,21,"Weekday",31,32]
[16,40168,12,21,22,"Weekday",30,31]
[16,40168,12,21,23,"Weekday",30,31]
[16,40168,12,21,24,"Weekday",31,32]
[16,40169,12,22,1,"Weekday",31,32]
[16,40169,12,22,2,"Weekday",32,32]
[16,40169,12,22,3,"Weekday",31,31]
[16,40169,12,22,4,"Weekday",29,30]
[16,40169,12,22,5,"Weekday",29,30]
[16,40169,12,22,6,"Weekday",29,30]
[16,40169,12,22,7,"Weekday",29,30]
[16,40169,12,22,8,"Weekday",29,30]
[16,40169,12,22,9,"Weekday",29,30]
[16,40169,12,22,10,"Weekday",29,30]
[16,40169,12,22,11,"Weekday",33,34]
[16,40169,12,22,12,"Weekday",37,39]
[16,40169,12,22,13,"Weekday",41,43]
[16,40169,12,22,14,"Weekday",40,42]
[16,40169,12,22,15,"Weekday",39,41]
[16,40169,12,22,16,"Weekday",37,39]
[16,40169,12,22,17,"Weekday",36,38]
[16,40169,12,22,18,"Weekday",35,37]
[16,40169,12,22,19,"Weekday",34,36]
[16,40169,12,22,20,"Weekday",32,34]
[16,40169,12,22,21,"Weekday",31,32]
[16,40169,12,22,22,"Weekday",29,30]
[16,40169,12,22,23,"Weekday",27,28]
[16,40169,12,22,24,"Weekday",27,28]
[16,40170,12,23,1,"Weekday",27,28]
[16,40170,12,23,2,"Weekday",28,29]
[16,40170,12,23,3,"Weekday",29,30]
[16,40170,12,23,4,"Weekday",31,32]
[16,40170,12,23,5,"Weekday",31,32]
[16,40170,12,23,6,"Weekday",31,32]
[16,40170,12,23,7,"Weekday",31,32]
[16,40170,12,23,8,"Weekday",34,35]
[16,40170,12,23,9,"Weekday",36,37]
[16,40170,12,23,10,"Weekday",38,40]
[16,40170,12,23,11,"Weekday",40,42]
[16,40170,12,23,12,"Weekday",42,44]
[16,40170,12,23,13,"Weekday",44,47]
[16,40170,12,23,14,"Weekday",43,46]
[16,40170,12,23,15,"Weekday",43,46]
[16,40170,12,23,16,"Weekday",43,45]
[16,40170,12,23,17,"Weekday",41,43]
[16,40170,12,23,18,"Weekday",39,40]
[16,40170,12,23,19,"Weekday",37,38]
[16,40170,12,23,20,"Weekday",34,35]
[16,40170,12,23,21,"Weekday",31,32]
[16,40170,12,23,22,"Weekday",28,29]
[16,40170,12,23,23,"Weekday",26,27]
[16,40170,12,23,24,"Weekday",26,27]
[16,{"$f":"DATE(2009,C139970,D139970)","v":40171},12,24,1,"Weekday",27,27]
[16,40171,12,24,2,"Weekday",28,28]
[16,40171,12,24,3,"Weekday",29,30]
[16,40171,12,24,4,"Weekday",31,32]
[16,40171,12,24,5,"Weekday",32,32]
[16,40171,12,24,6,"Weekday",32,33]
[16,40171,12,24,7,"Weekday",33,33]
[16,40171,12,24,8,"Weekday",34,35]
[16,40171,12,24,9,"Weekday",35,36]
[16,40171,12,24,10,"Weekday",37,37]
[16,40171,12,24,11,"Weekday",39,40]
[16,40171,12,24,12,"Weekday",41,43]
[16,40171,12,24,13,"Weekday",44,46]
[16,40171,12,24,14,"Weekday",41,43]
[16,40171,12,24,15,"Weekday",38,39]
[16,40171,12,24,16,"Weekday",35,35]
[16,40171,12,24,17,"Weekday",33,34]
[16,40171,12,24,18,"Weekday",32,33]
[16,40171,12,24,19,"Weekday",31,32]
[16,40171,12,24,20,"Weekday",31,32]
[16,40171,12,24,21,"Weekday",31,32]
[16,40171,12,24,22,"Weekday",31,32]
[16,40171,12,24,23,"Weekday",31,32]
[16,40171,12,24,24,"Weekday",31,31]
[16,40172,12,25,1,"Weekday",31,31]
[16,40172,12,25,2,"Weekday",29,30]
[16,40172,12,25,3,"Weekday",27,28]
[16,40172,12,25,4,"Weekday",26,26]
[16,40172,12,25,5,"Weekday",26,27]
[16,40172,12,25,6,"Weekday",26,27]
[16,40172,12,25,7,"Weekday",26,27]
[16,40172,12,25,8,"Weekday",29,30]
[16,40172,12,25,9,"Weekday",31,33]
[16,40172,12,25,10,"Weekday",34,35]
[16,40172,12,25,11,"Weekday",36,37]
[16,40172,12,25,12,"Weekday",38,40]
[16,40172,12,25,13,"Weekday",40,42]
[16,40172,12,25,14,"Weekday",40,42]
[16,40172,12,25,15,"Weekday",39,41]
[16,40172,12,25,16,"Weekday",39,40]
[16,40172,12,25,17,"Weekday",38,40]
[16,40172,12,25,18,"Weekday",38,39]
[16,40172,12,25,19,"Weekday",37,39]
[16,40172,12,25,20,"Weekday",37,39]
[16,40172,12,25,21,"Weekday",38,40]
[16,40172,12,25,22,"Weekday",38,40]
[16,40172,12,25,23,"Weekday",37,40]
[16,40172,12,25,24,"Weekday",36,38]
[16,40173,12,26,1,"Saturday",34,37]
[16,40173,12,26,2,"Saturday",33,35]
[16,40173,12,26,3,"Saturday",32,34]
[16,40173,12,26,4,"Saturday",31,33]
[16,40173,12,26,5,"Saturday",32,34]
[16,40173,12,26,6,"Saturday",33,35]
[16,40173,12,26,7,"Saturday",35,37]
[16,40173,12,26,8,"Saturday",37,39]
[16,40173,12,26,9,"Saturday",39,42]
[16,40173,12,26,10,"Saturday",42,45]
[16,40173,12,26,11,"Saturday",42,45]
[16,40173,12,26,12,"Saturday",43,46]
[16,40173,12,26,13,"Saturday",44,46]
[16,40173,12,26,14,"Saturday",44,46]
[16,40173,12,26,15,"Saturday",44,46]
[16,40173,12,26,16,"Saturday",44,46]
[16,{"$f":"DATE(2009,C140034,D140034)","v":40173},12,26,17,"Saturday",39,41]
[16,40173,12,26,18,"Saturday",35,36]
[16,40173,12,26,19,"Saturday",30,31]
[16,40173,12,26,20,"Saturday",30,32]
[16,40173,12,26,21,"Saturday",30,32]
[16,40173,12,26,22,"Saturday",30,33]
[16,40173,12,26,23,"Saturday",30,33]
[16,40173,12,26,24,"Saturday",31,34]
[16,40174,12,27,1,"Sunday",31,34]
[16,40174,12,27,2,"Sunday",31,34]
[16,40174,12,27,3,"Sunday",31,34]
[16,40174,12,27,4,"Sunday",30,33]
[16,40174,12,27,5,"Sunday",30,33]
[16,40174,12,27,6,"Sunday",29,32]
[16,40174,12,27,7,"Sunday",29,31]
[16,40174,12,27,8,"Sunday",30,33]
[16,40174,12,27,9,"Sunday",31,34]
[16,40174,12,27,10,"Sunday",32,35]
[16,40174,12,27,11,"Sunday",35,39]
[16,40174,12,27,12,"Sunday",37,44]
[16,40174,12,27,13,"Sunday",40,48]
[16,40174,12,27,14,"Sunday",39,47]
[16,40174,12,27,15,"Sunday",38,46]
[16,40174,12,27,16,"Sunday",38,44]
[16,40174,12,27,17,"Sunday",36,41]
[16,40174,12,27,18,"Sunday",34,38]
[16,40174,12,27,19,"Sunday",31,35]
[16,40174,12,27,20,"Sunday",32,36]
[16,40174,12,27,21,"Sunday",33,36]
[16,40174,12,27,22,"Sunday",33,37]
[16,40174,12,27,23,"Sunday",33,36]
[16,40174,12,27,24,"Sunday",32,35]
[16,40175,12,28,1,"Weekday",31,33]
[16,40175,12,28,2,"Weekday",30,31]
[16,40175,12,28,3,"Weekday",30,31]
[16,40175,12,28,4,"Weekday",29,30]
[16,40175,12,28,5,"Weekday",30,31]
[16,40175,12,28,6,"Weekday",30,31]
[16,40175,12,28,7,"Weekday",31,32]
[16,40175,12,28,8,"Weekday",33,34]
[16,40175,12,28,9,"Weekday",34,35]
[16,40175,12,28,10,"Weekday",36,37]
[16,40175,12,28,11,"Weekday",39,41]
[16,40175,12,28,12,"Weekday",43,45]
[16,40175,12,28,13,"Weekday",46,48]
[16,40175,12,28,14,"Weekday",44,47]
[16,40175,12,28,15,"Weekday",43,45]
[16,40175,12,28,16,"Weekday",42,43]
[16,40175,12,28,17,"Weekday",40,41]
[16,40175,12,28,18,"Weekday",39,39]
[16,40175,12,28,19,"Weekday",37,37]
[16,40175,12,28,20,"Weekday",35,35]
[16,40175,12,28,21,"Weekday",32,33]
[16,40175,12,28,22,"Weekday",30,30]
[16,40175,12,28,23,"Weekday",29,29]
[16,40175,12,28,24,"Weekday",29,30]
[16,40176,12,29,1,"Weekday",29,30]
[16,40176,12,29,2,"Weekday",29,29]
[16,40176,12,29,3,"Weekday",27,27]
[16,40176,12,29,4,"Weekday",25,25]
[16,40176,12,29,5,"Weekday",24,24]
[16,40176,12,29,6,"Weekday",23,23]
[16,40176,12,29,7,"Weekday",22,22]
[16,40176,12,29,8,"Weekday",25,26]
[16,{"$f":"DATE(2009,C140098,D140098)","v":40176},12,29,9,"Weekday",28,29]
[16,40176,12,29,10,"Weekday",31,32]
[16,40176,12,29,11,"Weekday",36,40]
[16,40176,12,29,12,"Weekday",42,47]
[16,40176,12,29,13,"Weekday",46,54]
[16,40176,12,29,14,"Weekday",46,53]
[16,40176,12,29,15,"Weekday",44,51]
[16,40176,12,29,16,"Weekday",44,50]
[16,40176,12,29,17,"Weekday",42,47]
[16,40176,12,29,18,"Weekday",40,45]
[16,40176,12,29,19,"Weekday",38,42]
[16,40176,12,29,20,"Weekday",36,41]
[16,40176,12,29,21,"Weekday",34,39]
[16,40176,12,29,22,"Weekday",32,37]
[16,40176,12,29,23,"Weekday",31,37]
[16,40176,12,29,24,"Weekday",32,38]
[16,40177,12,30,1,"Weekday",33,39]
[16,40177,12,30,2,"Weekday",33,39]
[16,40177,12,30,3,"Weekday",32,38]
[16,40177,12,30,4,"Weekday",31,37]
[16,40177,12,30,5,"Weekday",30,35]
[16,40177,12,30,6,"Weekday",29,32]
[16,40177,12,30,7,"Weekday",27,29]
[16,40177,12,30,8,"Weekday",29,32]
[16,40177,12,30,9,"Weekday",31,35]
[16,40177,12,30,10,"Weekday",32,37]
[16,40177,12,30,11,"Weekday",31,35]
[16,40177,12,30,12,"Weekday",30,32]
[16,40177,12,30,13,"Weekday",28,29]
[16,40177,12,30,14,"Weekday",29,31]
[16,40177,12,30,15,"Weekday",29,32]
[16,40177,12,30,16,"Weekday",29,33]
[16,40177,12,30,17,"Weekday",28,31]
[16,40177,12,30,18,"Weekday",26,29]
[16,40177,12,30,19,"Weekday",24,27]
[16,40177,12,30,20,"Weekday",23,27]
[16,40177,12,30,21,"Weekday",23,26]
[16,40177,12,30,22,"Weekday",22,25]
[16,40177,12,30,23,"Weekday",22,25]
[16,40177,12,30,24,"Weekday",23,27]
[16,40178,12,31,1,"Weekday",24,28]
[16,40178,12,31,2,"Weekday",25,29]
[16,40178,12,31,3,"Weekday",25,29]
[16,40178,12,31,4,"Weekday",25,29]
[16,40178,12,31,5,"Weekday",25,28]
[16,40178,12,31,6,"Weekday",24,28]
[16,40178,12,31,7,"Weekday",24,27]
[16,40178,12,31,8,"Weekday",25,29]
[16,40178,12,31,9,"Weekday",26,29]
[16,40178,12,31,10,"Weekday",27,31]
[16,40178,12,31,11,"Weekday",29,33]
[16,40178,12,31,12,"Weekday",31,36]
[16,40178,12,31,13,"Weekday",32,38]
[16,40178,12,31,14,"Weekday",32,38]
[16,40178,12,31,15,"Weekday",32,37]
[16,40178,12,31,16,"Weekday",31,36]
[16,40178,12,31,17,"Weekday",30,35]
[16,40178,12,31,18,"Weekday",29,33]
[16,40178,12,31,19,"Weekday",26,29]
[16,40178,12,31,20,"Weekday",28,32]
[16,40178,12,31,21,"Weekday",28,33]
[16,40178,12,31,22,"Weekday",28,32]
[16,40178,12,31,23,"Weekday",27,32]
[16,40178,12,31,24,"Weekday",25,31]

{"sheet":"General Look Up Tables","index":7,"n_rows":1727,"n_cols":9,"rows_kept":1727,"cut":false,"hidden":true,"merged":[[0,0,0,1]]}
["tbl_Zip_Codes",null,null,null,"List_Building_Types",null,"Source of Heating",null,"List_CTRL"]
["ZIP Code","Climate Zone",null,null,"Auditorium",null,"Gas",null,"Fixed"]
[12,16,null,null,"Cleanroom",null,"Electric",null,"OAT"]
[16,16,null,null,"Commercial and Industrial Storage"]
[17,16,null,null,"Convention Center"]
[18,16,null,null,"Data Center"]
[19,16,null,null,"College"]
[20,16,null,null,"Financial Institution"]
[22,2,null,null,"Grocery Store"]
[26,16,null,null,"Gymnasium"]
[28,16,null,null,"Hospital"]
[29,16,null,null,"Hotel/Lodging"]
[31,16,null,null,"Industrial Factories"]
[32,5,null,null,"Library"]
[33,16,null,null,"Laboratories"]
[34,16,null,null,"Mall"]
[35,16,null,null,"Manufacturing Factories"]
[37,16,null,null,"Medical Office/Clinic"]
[38,16,null,null,"Museum"]
[39,16,null,null,"Office"]
[40,16,null,null,"Religious Facility"]
[44,16,null,null,"Restaurant"]
[47,16,null,null,"Retail Merchandise/Wholesale"]
[48,2,null,null,"School"]
[49,16,null,null,"Theater"]
[50,16]
[51,16]
[52,16]
[54,1]
[55,16]
[58,16]
[65,16]
[90001,8]
[90002,8]
[90003,8]
[90004,9]
[90005,9]
[90006,9]
[90007,8]
[90008,8]
[90011,8]
[90012,9]
[90013,9]
[90014,9]
[90015,9]
[90016,8]
[90017,9]
[90018,8]
[90019,9]
[90020,9]
[90021,9]
[90022,9]
[90023,9]
[90024,9]
[90025,6]
[90026,9]
[90027,9]
[90028,9]
[90029,9]
[90031,9]
[90032,9]
[90033,9]
[90034,8]
[90035,9]
[90036,9]
[90037,8]
[90038,9]
[90039,9]
[90040,8]
[90041,9]
[90042,9]
[90043,8]
[90044,8]
[90045,6]
[90046,9]
[90047,8]
[90048,9]
[90049,6]
[90056,8]
[90057,9]
[90058,8]
[90059,8]
[90061,8]
[90062,8]
[90063,9]
[90064,9]
[90065,9]
[90066,6]
[90067,9]
[90068,9]
[90069,9]
[90071,9]
[90073,6]
[90077,9]
[90089,8]
[90094,6]
[90095,9]
[90201,8]
[90210,9]
[90211,9]
[90212,9]
[90220,8]
[90221,8]
[90222,8]
[90230,8]
[90232,8]
[90240,8]
[90241,8]
[90242,8]
[90245,6]
[90247,8]
[90248,8]
[90249,8]
[90250,8]
[90254,6]
[90255,8]
[90260,8]
[90262,8]
[90263,6]
[90265,6]
[90266,6]
[90270,8]
[90272,6]
[90274,6]
[90275,6]
[90277,6]
[90278,6]
[90280,8]
[90290,6]
[90291,6]
[90292,6]
[90293,6]
[90301,8]
[90302,8]
[90303,8]
[90304,8]
[90305,8]
[90401,6]
[90402,6]
[90403,6]
[90404,6]
[90405,6]
[90501,6]
[90502,6]
[90503,6]
[90504,8]
[90505,6]
[90506,8]
[90601,9]
[90602,9]
[90603,9]
[90604,9]
[90605,9]
[90606,9]
[90620,8]
[90621,8]
[90623,8]
[90630,8]
[90631,8]
[90638,9]
[90639,9]
[90640,9]
[90650,8]
[90660,9]
[90670,9]
[90680,8]
[90701,8]
[90703,8]
[90704,6]
[90706,8]
[90710,6]
[90712,8]
[90713,8]
[90715,8]
[90716,8]
[90717,6]
[90720,8]
[90723,8]
[90731,6]
[90732,6]
[90740,6]
[90742,6]
[90743,6]
[90744,6]
[90745,6]
[90746,8]
[90747,8]
[90755,6]
[90802,6]
[90803,6]
[90804,6]
[90805,8]
[90806,6]
[90807,8]
[90808,8]
[90810,6]
[90813,6]
[90814,6]
[90815,6]
[90822,6]
[90840,6]
[91001,9]
[91006,9]
[91007,9]
[91008,9]
[91010,9]
[91011,9]
[91016,9]
[91020,9]
[91024,9]
[91030,9]
[91040,16]
[91042,16]
[91101,9]
[91103,9]
[91104,9]
[91105,9]
[91106,9]
[91107,9]
[91108,9]
[91123,9]
[91201,9]
[91202,9]
[91203,9]
[91204,9]
[91205,9]
[91206,9]
[91207,9]
[91208,9]
[91214,9]
[91301,9]
[91302,9]
[91303,9]
[91304,9]
[91306,9]
[91307,9]
[91311,9]
[91316,9]
[91320,6]
[91321,9]
[91324,9]
[91325,9]
[91326,9]
[91330,9]
[91331,9]
[91335,9]
[91340,9]
[91342,9]
[91343,9]
[91344,9]
[91345,9]
[91350,9]
[91351,9]
[91352,9]
[91354,9]
[91355,9]
[91356,9]
[91360,9]
[91361,9]
[91362,9]
[91364,9]
[91367,9]
[91371,9]
[91377,9]
[91381,9]
[91384,9]
[91387,9]
[91390,16]
[91401,9]
[91402,9]
[91403,9]
[91405,9]
[91406,9]
[91411,9]
[91423,9]
[91436,9]
[91501,9]
[91502,9]
[91504,9]
[91505,9]
[91506,9]
[91521,9]
[91522,9]
[91523,9]
[91601,9]
[91602,9]
[91604,9]
[91605,9]
[91606,9]
[91607,9]
[91608,9]
[91701,10]
[91702,9]
[91706,9]
[91708,10]
[91709,10]
[91710,10]
[91711,9]
[91722,9]
[91723,9]
[91724,9]
[91730,10]
[91731,9]
[91732,9]
[91733,9]
[91737,10]
[91739,10]
[91740,9]
[91741,9]
[91744,9]
[91745,9]
[91746,9]
[91748,9]
[91750,9]
[91752,10]
[91754,9]
[91755,9]
[91759,16]
[91761,10]
[91762,10]
[91763,10]
[91764,10]
[91765,9]
[91766,9]
[91767,9]
[91768,9]
[91770,9]
[91773,9]
[91775,9]
[91776,9]
[91780,9]
[91784,10]
[91786,10]
[91789,9]
[91790,9]
[91791,9]
[91792,9]
[91801,9]
[91803,9]
[91901,10]
[91902,7]
[91905,14]
[91906,14]
[91910,7]
[91911,7]
[91913,7]
[91914,10]
[91915,7]
[91916,14]
[91917,10]
[91932,7]
[91934,14]
[91935,10]
[91941,7]
[91942,7]
[91945,7]
[91950,7]
[91962,14]
[91963,14]
[91977,10]
[91978,10]
[91980,14]
[92003,10]
[92004,15]
[92007,7]
[92008,7]
[92009,7]
[92010,7]
[92011,7]
[92014,7]
[92019,10]
[92020,10]
[92021,10]
[92024,7]
[92025,10]
[92026,10]
[92027,10]
[92028,10]
[92029,10]
[92036,14]
[92037,7]
[92040,10]
[92054,7]
[92055,7]
[92056,7]
[92057,7]
[92058,7]
[92059,10]
[92060,14]
[92061,10]
[92064,10]
[92065,10]
[92066,14]
[92067,7]
[92069,10]
[92070,14]
[92071,10]
[92075,7]
[92078,10]
[92081,7]
[92082,10]
[92083,7]
[92084,7]
[92086,14]
[92091,7]
[92093,7]
[92096,10]
[92101,7]
[92102,7]
[92103,7]
[92104,7]
[92105,7]
[92106,7]
[92107,7]
[92108,7]
[92109,7]
[92110,7]
[92111,7]
[92113,7]
[92114,7]
[92115,7]
[92116,7]
[92117,7]
[92118,7]
[92119,7]
[92120,7]
[92121,7]
[92122,7]
[92123,7]
[92124,7]
[92126,7]
[92127,10]
[92128,10]
[92129,7]
[92130,7]
[92131,10]
[92134,7]
[92135,7]
[92136,7]
[92139,7]
[92140,7]
[92145,7]
[92152,7]
[92154,7]
[92155,7]
[92173,7]
[92182,7]
[92201,15]
[92203,15]
[92210,15]
[92211,15]
[92220,15]
[92223,10]
[92225,15]
[92227,15]
[92230,15]
[92231,15]
[92233,15]
[92234,15]
[92236,15]
[92239,15]
[92240,15]
[92241,15]
[92242,15]
[92243,15]
[92249,15]
[92250,15]
[92251,15]
[92252,14]
[92253,15]
[92254,15]
[92256,14]
[92257,15]
[92259,15]
[92260,15]
[92262,15]
[92264,15]
[92267,15]
[92270,15]
[92274,15]
[92276,15]
[92277,14]
[92278,14]
[92280,15]
[92281,15]
[92282,15]
[92283,15]
[92284,14]
[92285,14]
[92301,14]
[92304,15]
[92305,16]
[92307,14]
[92308,14]
[92309,14]
[92310,14]
[92311,14]
[92313,10]
[92314,16]
[92315,16]
[92316,10]
[92317,16]
[92318,10]
[92320,10]
[92321,16]
[92322,16]
[92324,10]
[92325,16]
[92327,14]
[92328,14]
[92332,14]
[92333,16]
[92335,10]
[92336,10]
[92337,10]
[92338,14]
[92339,16]
[92341,16]
[92342,14]
[92344,14]
[92345,14]
[92346,10]
[92347,14]
[92350,10]
[92352,16]
[92354,10]
[92356,14]
[92358,16]
[92359,16]
[92363,15]
[92364,14]
[92365,14]
[92368,14]
[92371,14]
[92372,14]
[92373,10]
[92374,10]
[92376,10]
[92377,10]
[92378,16]
[92382,16]
[92384,14]
[92385,16]
[92389,14]
[92391,16]
[92392,14]
[92394,14]
[92395,14]
[92397,16]
[92399,10]
[92401,10]
[92404,16]
[92405,10]
[92407,10]
[92408,10]
[92410,10]
[92411,10]
[92501,10]
[92503,10]
[92504,10]
[92505,10]
[92506,10]
[92507,10]
[92508,10]
[92509,10]
[92518,10]
[92521,10]
[92530,10]
[92532,10]
[92536,15]
[92539,16]
[92543,10]
[92544,10]
[92545,10]
[92548,10]
[92549,16]
[92551,10]
[92553,10]
[92555,10]
[92557,10]
[92561,16]
[92562,10]
[92563,10]
[92567,10]
[92570,10]
[92571,10]
[92582,10]
[92583,10]
[92584,10]
[92585,10]
[92586,10]
[92587,10]
[92590,10]
[92591,10]
[92592,10]
[92595,10]
[92596,10]
[92602,8]
[92603,8]
[92604,8]
[92606,8]
[92610,8]
[92612,8]
[92614,8]
[92617,6]
[92618,8]
[92620,8]
[92624,6]
[92625,6]
[92626,6]
[92627,6]
[92629,6]
[92630,8]
[92637,8]
[92646,6]
[92647,6]
[92648,6]
[92649,6]
[92651,6]
[92653,6]
[92655,6]
[92656,6]
[92657,6]
[92660,6]
[92661,6]
[92662,6]
[92663,6]
[92672,6]
[92673,6]
[92675,6]
[92676,8]
[92677,6]
[92679,8]
[92683,6]
[92688,8]
[92691,8]
[92692,8]
[92694,8]
[92697,6]
[92701,8]
[92702,8]
[92703,8]
[92704,8]
[92705,8]
[92706,8]
[92707,8]
[92708,6]
[92780,8]
[92782,8]
[92801,8]
[92802,8]
[92804,8]
[92805,8]
[92806,8]
[92807,8]
[92808,8]
[92821,8]
[92823,8]
[92831,8]
[92832,8]
[92833,8]
[92835,8]
[92840,8]
[92841,8]
[92843,8]
[92844,6]
[92845,8]
[92860,10]
[92861,8]
[92865,8]
[92866,8]
[92867,8]
[92868,8]
[92869,8]
[92870,8]
[92879,10]
[92880,10]
[92881,10]
[92882,10]
[92883,10]
[92886,8]
[92887,8]
[93001,6]
[93003,6]
[93004,6]
[93010,6]
[93012,6]
[93013,6]
[93015,9]
[93021,9]
[93022,9]
[93023,9]
[93030,6]
[93033,6]
[93035,6]
[93036,6]
[93040,9]
[93041,6]
[93042,6]
[93043,6]
[93060,9]
[93063,9]
[93065,9]
[93066,9]
[93067,6]
[93101,6]
[93103,6]
[93105,5]
[93106,6]
[93108,6]
[93109,6]
[93110,6]
[93111,6]
[93117,6]
[93201,13]
[93202,13]
[93203,13]
[93204,13]
[93205,16]
[93206,13]
[93207,13]
[93210,13]
[93212,13]
[93215,13]
[93219,13]
[93221,13]
[93222,16]
[93223,13]
[93224,13]
[93225,16]
[93226,16]
[93230,13]
[93234,13]
[93235,13]
[93238,16]
[93239,13]
[93240,16]
[93241,13]
[93242,13]
[93243,16]
[93244,13]
[93245,13]
[93247,13]
[93249,13]
[93250,13]
[93251,13]
[93252,13]
[93254,4]
[93255,16]
[93256,13]
[93257,13]
[93260,13]
[93261,13]
[93262,16]
[93263,13]
[93265,16]
[93266,13]
[93267,13]
[93268,13]
[93270,13]
[93271,13]
[93272,13]
[93274,13]
[93276,13]
[93277,13]
[93280,13]
[93283,16]
[93285,16]
[93286,13]
[93287,13]
[93291,13]
[93292,13]
[93301,13]
[93304,13]
[93305,13]
[93306,13]
[93307,13]
[93308,13]
[93309,13]
[93311,13]
[93312,13]
[93313,13]
[93314,13]
[93401,5]
[93402,5]
[93405,5]
[93407,5]
[93420,5]
[93422,4]
[93426,4]
[93427,5]
[93428,5]
[93429,5]
[93430,5]
[93432,4]
[93433,5]
[93434,5]
[93435,5]
[93436,5]
[93437,5]
[93440,5]
[93441,5]
[93442,5]
[93444,5]
[93445,5]
[93446,4]
[93449,5]
[93450,4]
[93451,4]
[93452,5]
[93453,4]
[93454,5]
[93455,5]
[93458,5]
[93460,5]
[93461,4]
[93463,5]
[93465,4]
[93501,14]
[93505,14]
[93510,14]
[93512,16]
[93513,16]
[93514,16]
[93516,14]
[93517,16]
[93518,16]
[93519,14]
[93523,14]
[93524,14]
[93526,16]
[93527,16]
[93528,14]
[93529,16]
[93531,16]
[93532,14]
[93534,14]
[93535,14]
[93536,14]
[93541,16]
[93543,14]
[93544,14]
[93545,16]
[93546,16]
[93550,16]
[93551,14]
[93552,14]
[93553,14]
[93554,14]
[93555,14]
[93560,14]
[93561,16]
[93562,14]
[93563,16]
[93591,14]
[93601,13]
[93602,16]
[93603,13]
[93604,16]
[93608,13]
[93609,13]
[93610,13]
[93611,13]
[93612,13]
[93614,13]
[93615,13]
[93616,13]
[93618,13]
[93619,13]
[93620,12]
[93621,13]
[93622,13]
[93623,16]
[93625,13]
[93626,13]
[93627,13]
[93628,16]
[93630,13]
[93631,13]
[93633,16]
[93634,16]
[93635,12]
[93636,13]
[93637,13]
[93638,13]
[93640,13]
[93641,13]
[93643,16]
[93644,13]
[93645,13]
[93646,13]
[93647,13]
[93648,13]
[93650,13]
[93651,13]
[93652,13]
[93653,13]
[93654,13]
[93656,13]
[93657,13]
[93660,13]
[93662,13]
[93664,16]
[93667,13]
[93668,13]
[93669,16]
[93675,13]
[93701,13]
[93702,13]
[93703,13]
[93704,13]
[93705,13]
[93706,13]
[93710,13]
[93711,13]
[93720,13]
[93721,13]
[93722,13]
[93723,13]
[93725,13]
[93726,13]
[93727,13]
[93728,13]
[93730,13]
[93737,13]
[93741,13]
[93901,3]
[93905,3]
[93906,3]
[93907,3]
[93908,3]
[93920,3]
[93923,3]
[93924,3]
[93925,3]
[93926,3]
[93927,3]
[93930,4]
[93932,4]
[93933,3]
[93940,3]
[93943,3]
[93944,3]
[93950,3]
[93953,3]
[93955,3]
[93960,3]
[94002,3]
[94005,3]
[94010,3]
[94014,3]
[94015,3]
[94019,3]
[94020,3]
[94021,3]
[94022,4]
[94024,4]
[94025,3]
[94027,3]
[94028,3]
[94030,3]
[94035,4]
[94037,3]
[94038,3]
[94040,4]
[94041,4]
[94043,4]
[94044,3]
[94060,3]
[94061,3]
[94062,3]
[94063,3]
[94065,3]
[94066,3]
[94070,3]
[94074,3]
[94080,3]
[94085,4]
[94086,4]
[94087,4]
[94089,4]
[94102,3]
[94103,3]
[94104,3]
[94105,3]
[94107,3]
[94108,3]
[94109,3]
[94110,3]
[94111,3]
[94112,3]
[94114,3]
[94115,3]
[94116,3]
[94117,3]
[94118,3]
[94121,3]
[94122,3]
[94123,3]
[94124,3]
[94127,3]
[94128,3]
[94129,3]
[94130,3]
[94131,3]
[94132,3]
[94133,3]
[94134,3]
[94158,3]
[94301,4]
[94303,4]
[94304,4]
[94305,4]
[94306,4]
[94401,3]
[94402,3]
[94403,3]
[94404,3]
[94501,3]
[94502,3]
[94503,2]
[94505,12]
[94506,12]
[94507,12]
[94508,2]
[94509,12]
[94510,12]
[94511,12]
[94512,12]
[94513,12]
[94514,12]
[94515,2]
[94517,12]
[94518,12]
[94519,12]
[94520,12]
[94521,12]
[94523,12]
[94525,12]
[94526,12]
[94528,12]
[94530,3]
[94531,12]
[94533,12]
[94534,12]
[94535,12]
[94536,3]
[94538,3]
[94539,3]
[94541,3]
[94542,3]
[94544,3]
[94545,3]
[94546,3]
[94547,3]
[94548,12]
[94549,12]
[94550,12]
[94551,12]
[94552,3]
[94553,12]
[94555,3]
[94556,12]
[94558,2]
[94559,2]
[94560,3]
[94561,12]
[94563,12]
[94564,3]
[94565,12]
[94566,12]
[94567,2]
[94568,12]
[94569,12]
[94571,12]
[94572,3]
[94574,2]
[94576,2]
[94577,3]
[94578,3]
[94579,3]
[94580,3]
[94582,12]
[94583,12]
[94585,12]
[94586,12]
[94587,3]
[94588,12]
[94589,3]
[94590,3]
[94591,12]
[94592,3]
[94595,12]
[94596,12]
[94597,12]
[94598,12]
[94599,2]
[94601,3]
[94602,3]
[94603,3]
[94605,3]
[94606,3]
[94607,3]
[94608,3]
[94609,3]
[94610,3]
[94611,3]
[94612,3]
[94613,3]
[94618,3]
[94619,3]
[94621,3]
[94702,3]
[94703,3]
[94704,3]
[94705,3]
[94706,3]
[94707,3]
[94708,3]
[94709,3]
[94710,3]
[94720,3]
[94801,3]
[94803,3]
[94804,3]
[94805,3]
[94806,3]
[94901,2]
[94903,2]
[94904,2]
[94920,3]
[94922,1]
[94923,1]
[94924,3]
[94925,3]
[94928,2]
[94929,3]
[94930,2]
[94931,2]
[94933,3]
[94937,3]
[94938,3]
[94939,2]
[94940,3]
[94941,3]
[94945,2]
[94946,2]
[94947,2]
[94949,2]
[94951,2]
[94952,2]
[94954,2]
[94956,3]
[94960,2]
[94963,2]
[94964,2]
[94965,3]
[94970,3]
[94971,3]
[94972,2]
[94973,2]
[95002,4]
[95003,3]
[95004,4]
[95005,3]
[95006,3]
[95008,4]
[95010,3]
[95012,3]
[95013,4]
[95014,4]
[95017,3]
[95018,3]
[95019,3]
[95020,4]
[95023,4]
[95030,4]
[95032,4]
[95033,4]
[95035,4]
[95037,4]
[95039,3]
[95043,4]
[95045,4]
[95046,4]
[95050,4]
[95051,4]
[95053,4]
[95054,4]
[95060,3]
[95062,3]
[95064,3]
[95065,3]
[95066,3]
[95070,4]
[95073,3]
[95076,3]
[95110,4]
[95111,4]
[95112,4]
[95113,4]
[95116,4]
[95117,4]
[95118,4]
[95119,4]
[95120,4]
[95121,4]
[95122,4]
[95123,4]
[95124,4]
[95125,4]
[95126,4]
[95127,4]
[95128,4]
[95129,4]
[95130,4]
[95131,4]
[95132,4]
[95133,4]
[95134,4]
[95135,4]
[95136,4]
[95138,4]
[95139,4]
[95140,4]
[95141,4]
[95148,4]
[95192,4]
[95202,12]
[95203,12]
[95204,12]
[95205,12]
[95206,12]
[95207,12]
[95209,12]
[95210,12]
[95211,12]
[95212,12]
[95215,12]
[95219,12]
[95220,12]
[95222,12]
[95223,16]
[95228,12]
[95230,12]
[95231,12]
[95232,12]
[95236,12]
[95237,12]
[95240,12]
[95242,12]
[95245,12]
[95246,12]
[95247,12]
[95249,12]
[95251,12]
[95252,12]
[95253,12]
[95255,12]
[95257,12]
[95258,12]
[95301,12]
[95303,12]
[95304,12]
[95305,12]
[95306,12]
[95307,12]
[95310,12]
[95311,12]
[95313,12]
[95315,12]
[95316,12]
[95317,12]
[95318,16]
[95319,12]
[95320,12]
[95321,12]
[95322,12]
[95323,12]
[95324,12]
[95326,12]
[95327,12]
[95328,12]
[95329,12]
[95330,12]
[95333,12]
[95334,12]
[95335,16]
[95336,12]
[95337,12]
[95338,12]
[95340,12]
[95341,12]
[95345,12]
[95346,16]
[95348,12]
[95350,12]
[95351,12]
[95354,12]
[95355,12]
[95356,12]
[95357,12]
[95358,12]
[95360,12]
[95361,12]
[95363,12]
[95364,16]
[95365,12]
[95366,12]
[95367,12]
[95368,12]
[95369,12]
[95370,12]
[95372,12]
[95374,12]
[95376,12]
[95377,12]
[95379,12]
[95380,12]
[95382,12]
[95383,12]
[95385,12]
[95386,12]
[95388,12]
[95389,16]
[95391,12]
[95401,2]
[95403,2]
[95404,2]
[95405,2]
[95407,2]
[95409,2]
[95410,1]
[95412,1]
[95415,2]
[95417,1]
[95420,1]
[95421,1]
[95422,2]
[95423,2]
[95425,2]
[95426,2]
[95427,1]
[95428,2]
[95429,2]
[95432,1]
[95436,2]
[95437,1]
[95439,2]
[95441,2]
[95442,2]
[95443,2]
[95444,2]
[95445,1]
[95446,2]
[95448,2]
[95449,2]
[95450,1]
[95451,2]
[95452,2]
[95453,2]
[95454,2]
[95456,1]
[95457,2]
[95458,2]
[95459,1]
[95460,1]
[95461,2]
[95462,1]
[95463,2]
[95464,2]
[95465,1]
[95466,2]
[95467,2]
[95468,1]
[95469,2]
[95470,2]
[95472,2]
[95476,2]
[95482,2]
[95485,2]
[95488,1]
[95490,2]
[95492,2]
[95493,2]
[95494,2]
[95497,1]
[95501,1]
[95503,1]
[95511,2]
[95514,2]
[95519,1]
[95521,1]
[95524,1]
[95525,1]
[95526,2]
[95527,16]
[95528,1]
[95531,1]
[95536,1]
[95540,1]
[95542,2]
[95543,16]
[95546,2]
[95547,1]
[95548,1]
[95549,1]
[95550,2]
[95551,1]
[95552,2]
[95554,2]
[95555,1]
[95556,2]
[95558,1]
[95560,2]
[95562,1]
[95563,16]
[95564,1]
[95565,1]
[95567,1]
[95568,16]
[95569,2]
[95570,1]
[95573,2]
[95585,1]
[95587,2]
[95589,1]
[95595,2]
[95602,11]
[95603,11]
[95605,12]
[95606,12]
[95607,12]
[95608,12]
[95610,12]
[95612,12]
[95614,12]
[95615,12]
[95616,12]
[95618,12]
[95619,12]
[95620,12]
[95621,12]
[95623,12]
[95624,12]
[95626,12]
[95627,12]
[95628,12]
[95629,12]
[95630,12]
[95631,16]
[95632,12]
[95633,12]
[95634,12]
[95635,12]
[95636,16]
[95637,12]
[95638,12]
[95639,12]
[95640,12]
[95641,12]
[95642,12]
[95645,11]
[95648,11]
[95650,11]
[95651,12]
[95652,12]
[95653,12]
[95655,12]
[95658,11]
[95659,11]
[95660,12]
[95661,11]
[95662,12]
[95663,11]
[95664,12]
[95665,12]
[95666,16]
[95667,12]
[95668,11]
[95669,12]
[95670,12]
[95672,12]
[95673,12]
[95674,11]
[95677,11]
[95678,11]
[95679,12]
[95681,11]
[95682,12]
[95683,12]
[95684,12]
[95685,12]
[95686,12]
[95687,12]
[95688,12]
[95689,12]
[95690,12]
[95691,12]
[95692,11]
[95693,12]
[95694,12]
[95695,12]
[95698,12]
[95699,12]
[95701,16]
[95703,11]
[95709,12]
[95713,11]
[95714,16]
[95715,16]
[95717,16]
[95720,16]
[95721,16]
[95722,11]
[95724,16]
[95726,16]
[95728,16]
[95735,16]
[95742,12]
[95746,11]
[95747,11]
[95757,12]
[95758,12]
[95762,12]
[95765,11]
[95776,12]
[95811,12]
[95814,12]
[95815,12]
[95816,12]
[95817,12]
[95818,12]
[95819,12]
[95820,12]
[95821,12]
[95822,12]
[95823,12]
[95824,12]
[95825,12]
[95826,12]
[95827,12]
[95828,12]
[95829,12]
[95830,12]
[95831,12]
[95832,12]
[95833,12]
[95834,12]
[95835,12]
[95836,12]
[95837,12]
[95838,12]
[95841,12]
[95842,12]
[95843,12]
[95864,12]
[95901,11]
[95903,11]
[95910,16]
[95912,11]
[95914,11]
[95915,16]
[95916,16]
[95917,11]
[95918,11]
[95919,11]
[95920,11]
[95922,16]
[95923,16]
[95925,16]
[95926,11]
[95928,11]
[95932,11]
[95934,16]
[95935,11]
[95936,16]
[95937,12]
[95938,11]
[95939,11]
[95941,16]
[95942,16]
[95943,11]
[95944,16]
[95945,11]
[95946,11]
[95947,16]
[95948,11]
[95949,11]
[95950,11]
[95951,11]
[95953,11]
[95954,16]
[95955,11]
[95956,16]
[95957,11]
[95959,11]
[95960,16]
[95961,11]
[95962,11]
[95963,11]
[95965,11]
[95966,11]
[95968,11]
[95969,11]
[95970,11]
[95971,16]
[95972,11]
[95973,11]
[95975,11]
[95977,11]
[95979,11]
[95981,16]
[95982,11]
[95983,16]
[95984,16]
[95987,11]
[95988,11]
[95991,11]
[95993,11]
[96001,11]
[96002,11]
[96003,11]
[96006,16]
[96007,11]
[96008,11]
[96010,16]
[96013,16]
[96014,16]
[96015,16]
[96016,16]
[96017,16]
[96019,11]
[96020,16]
[96021,11]
[96022,11]
[96023,16]
[96024,16]
[96025,16]
[96027,16]
[96028,16]
[96031,16]
[96032,16]
[96033,11]
[96034,16]
[96035,11]
[96038,16]
[96039,16]
[96040,16]
[96041,16]
[96044,16]
[96046,16]
[96047,11]
[96048,16]
[96050,16]
[96051,11]
[96052,16]
[96054,16]
[96055,11]
[96056,16]
[96057,16]
[96058,16]
[96059,11]
[96061,16]
[96062,11]
[96063,16]
[96064,16]
[96065,16]
[96067,16]
[96069,11]
[96071,16]
[96073,11]
[96075,16]
[96076,16]
[96080,11]
[96084,11]
[96085,16]
[96086,16]
[96087,11]
[96088,11]
[96091,16]
[96093,16]
[96094,16]
[96096,11]
[96097,16]
[96101,16]
[96103,16]
[96104,16]
[96105,16]
[96106,16]
[96107,16]
[96108,16]
[96109,16]
[96111,16]
[96112,16]
[96113,16]
[96114,16]
[96115,16]
[96116,16]
[96117,16]
[96118,16]
[96119,16]
[96120,16]
[96121,16]
[96122,16]
[96123,16]
[96124,16]
[96125,16]
[96126,16]
[96128,16]
[96129,16]
[96130,16]
[96132,16]
[96133,16]
[96134,16]
[96136,16]
[96137,16]
[96140,16]
[96141,16]
[96142,16]
[96143,16]
[96145,16]
[96146,16]
[96148,16]
[96150,16]
[96161,16]
[96162,16]

{"sheet":"_SSC","index":8,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":true,"merged":[]}
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"Customer Information\",\"Guid\":\"3ARC4H\",\"Index\":1,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}","{\"InputDetection\":0,\"RecalcMode\":0,\"Layout\":0,\"LayoutSamePagesHeightEnabled\":false,\"Theme\":{\"BgColor\":\"#FFFFFFFF\",\"BgImage\":\"\",\"InputBorderStyle\":2,\"AppliedTheme\":\"\"},\"SmartphoneSettings\":{\"ViewportLock\":true,\"UseOldViewEngine\":false,\"EnableZoom\":false,\"EnableSwipe\":false,\"HideToolbar\":false,\"InheritBackgroundColor\":false,\"CheckboxFlavor\":1,\"ShowBubble\":false},\"Name\":\"\",\"Flavor\":-1,\"Edition\":0,\"CopyProtect\":{\"IsEnabled\":false,\"DomainName\":\"\"},\"HideSscPoweredlogo\":false,\"AspnetConfig\":{\"BrowseUrl\":\"http://localhost/ssc\",\"FileExtension\":0},\"NodeSecureLoginEnabled\":false,\"SmartphoneTheme\":1,\"Toolbar\":{\"Position\":1,\"IsSubmit\":true,\"IsPrint\":true,\"IsPrintAll\":false,\"IsReset\":true,\"IsUpdate\":true},\"ConfigureSubmit\":{\"IsShowCaptcha\":false,\"IsUseSscWebServer\":true,\"ReceiverCode\":\"\",\"IsFreeService\":false,\"IsAdvanceService\":false,\"IsSecureEmail\":false,\"IsDemonstrationService\":true,\"AfterSuccessfulSubmit\":\"\",\"AfterFailSubmit\":\"\",\"AfterCancelWizard\":\"\",\"IsUseOwnWebServer\":false,\"OwnWebServerURL\":\"\",\"OwnWebServerTarget\":\"\",\"SubmitTarget\":0},\"IgnoreBgInputCell\":false,\"ButtonStyle\":0,\"ResponsiveDesignDisabled\":false,\"HideLookupRange\":false,\"BrowserStorageEnabled\":false,\"RealtimeSyncEnabled\":true,\"GoogleAnalyticsTrackingId\":\"\",\"GoogleApiKey\":\"\",\"ChartSelected\":3,\"ChartYAxisFixed\":false}","{\"BrowserAndLocation\":{\"ConversionPath\":\"\\\\\\\\vmware-host\\\\Shared Folders\\\\Documents\\\\SpreadsheetConverter\",\"SelectedBrowsers\":[]},\"SpreadsheetServer\":{\"Username\":\"\",\"Password\":\"\",\"ServerUrl\":\"\"},\"ConfigureSubmitDefault\":{\"Email\":\"\",\"Free\":false,\"Advanced\":false,\"AdvancedSecured\":false,\"Demo\":true},\"MessageBubble\":{\"Close\":false,\"TopMsg\":0},\"CustomizeTheme\":{\"Theme\":\"\"},\"QrSetting\":{\"ShowOnConversion\":true},\"CongratsPage\":{\"LastOpenedVersion\":\"\"},\"WordPressPluginSetting\":{\"IsPluginInstalled\":false},\"Preferences\":{\"IsAdvancedSettingModelInitialize\":true,\"IsCaptchaInitialize\":true,\"IsNodeSettingInitialize\":false,\"IsRequiredFieldModalInitialize\":true,\"IsSubmitDialogModelInitialize\":true,\"IsToolbarButtonModelInitialize\":true,\"IsWizardButtonModelInitialize\":true,\"ReadFromHidden\":false,\"AdvancedSetting\":null,\"NodeSetting\":{\"LoginText\":{\"LoginButtonText\":\"Login\",\"PageDescription\":\"Restricted access only\",\"LoginErrorMessage\":\"Authentication failed, please check your username and password.\",\"PlaceholderPassword\":\"password\",\"PlaceholderUsername\":\"username / email\",\"UserExtraMessage\":\"\"}},\"Captcha\":{\"Heading\":\"Enter the number displayed below.\",\"Message\":\"This is to verify that you are a human visitor, to prevent automated form submissions.\",\"OkButton\":\"OK\",\"CancelButton\":\"Cancel\",\"ErrorMessage\":\"Your answer is incorrect, please try again.\"},\"RequiredField\":{\"ErrorMessage\":\"The fields with the red border are required or invalid.\",\"OkButton\":\"OK\",\"DDLDefaultRequiredText\":\"Please Select\"},\"WizardButton\":{\"Next\":\"Next\",\"Previous\":\"Previous\",\"Cancel\":\"Cancel\",\"Finish\":\"Finish\"},\"ToolbarButton\":{\"Submit\":\"Submit\",\"Print\":\"Print\",\"PrintAll\":\"Print All\",\"Reset\":\"Reset\",\"Update\":\"Update\",\"Back\":\"Back\"},\"SubmitDialog\":{\"SubmitDialogHeading\":\"Submit Successful.\",\"SubmitDialogDesc\":\"The form was successfully submitted.\",\"BeforeSubmitDesc\":\"The form is being submitted.\",\"OfflineHeading\":\"Save until online\",\"OfflineDesc\":\"You are currently offline and the submit failed. Do you want to save the submit and send it later when you are online.\",\"OfflineConfirm\":\"Do you want to save?\",\"OfflineSubmitHeading\":\"Offline forms submit confirmation\",\"OfflineSubmitDesc\":\"There are Offline form(s), which are now ready to submit in server.\",\"OfflineSubmitConfirm\":\"Do you want to submit?\",\"FailOfflineHeading\":\"Offline Form submit failed\",\"FailOfflineDesc\":\"Unable to connect to the Internet. Please try submitting the offline forms later in internet connection.\",\"OfflineSubmitWait\":\"It may take sometime to finish all submits depending on the size of offline forms and internet connection.\",\"OfflineSubmitWaitCounter\":\"Left\",\"OfflineSubmitError\":\"Submit error: Please try later.\"}},\"UxPreferences\":null}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"Chilled Water System\",\"Guid\":\"YI3W2H\",\"Index\":2,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"Sheet1\",\"Guid\":\"GA8GH6\",\"Index\":3,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"Hot Water System Template\",\"Guid\":\"BX1AMP\",\"Index\":4,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"HVAC Air Template\",\"Guid\":\"N91GTT\",\"Index\":5,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"Refrigeration Template\",\"Guid\":\"YSH3TN\",\"Index\":6,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"CTZ2\",\"Guid\":\"6852PF\",\"Index\":7,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":true,\"HiddenInExcel\":true,\"SheetId\":-1,\"Name\":\"General Look Up Tables\",\"Guid\":\"6KKV6C\",\"Index\":8,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]
[null,null,"{\"IsHide\":false,\"HiddenInExcel\":false,\"SheetId\":-1,\"Name\":\"Refrigeration Look Up Tables\",\"Guid\":\"4SFSUK\",\"Index\":9,\"VisibleRange\":\"\",\"SheetTheme\":{\"TabColor\":\"\",\"BodyColor\":\"\",\"BodyImage\":\"\"}}"]